{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["LUMINARIAS","CALCULO","MANUAL DE USO","CONSULTA"],"not_rendered":{"charts":0,"images":9,"macros":0,"external_links":0,"defined_names":16,"comments":0,"pivot_tables":1},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"LUMINARIAS","index":0,"n_rows":29521,"n_cols":15,"rows_kept":4500,"cut":true,"hidden":true,"merged":[],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["ANCHO CALZADA","DISPOSICION","Clase de iluminación","Luminaria","Lámpara","Resultado","Separación  [m]","Altura de montaje [m]","Saliente sobre la calzada [m]","Inclination [°]","Lm [cd/m²]","U0","Ul","TI [%]","SR"]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,7,0,5,0.79,0.43,0.52,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,7,0,10,0.79,0.46,0.52,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,7,0,15,0.8,0.48,0.52,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,7.5,0,0,0.75,0.44,0.57999999999999996,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,7.5,0,5,0.76,0.48,0.6,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,7.5,0,10,0.76,0.49,0.59,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,7.5,0,15,0.77,0.52,0.6,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,7,0,0,0.81,0.42,0.55000000000000004,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,7,0,5,0.82,0.45,0.56999999999999995,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,7,0,10,0.83,0.48,0.56999999999999995,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,7,0,15,0.83,0.5,0.56999999999999995,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,7.5,0,0,0.78,0.47,0.62,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,7.5,0,5,0.79,0.5,0.64,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,7.5,0,10,0.8,0.52,0.64,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,7.5,0,15,0.8,0.54,0.64,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,8,0,0,0.75,0.51,0.68,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,8,0,5,0.76,0.53,0.71,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,8,0,10,0.77,0.55000000000000004,0.71,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,8,0,15,0.77,0.56999999999999995,0.71,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,6.5,0,5,0.9,0.43,0.53,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,6.5,0,10,0.9,0.46,0.54,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,6.5,0,15,0.91,0.48,0.54,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,7,0,0,0.85,0.44,0.6,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,7,0,5,0.86,0.47,0.62,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,7,0,10,0.87,0.5,0.62,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,7,0,15,0.87,0.52,0.62,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,7.5,0,0,0.82,0.49,0.67,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,7.5,0,5,0.83,0.52,0.69,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,7.5,0,10,0.83,0.53,0.69,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,7.5,0,15,0.84,0.55000000000000004,0.69,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,8,0,0,0.79,0.53,0.72,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,8,0,5,0.8,0.55000000000000004,0.74,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,8,0,10,0.8,0.56000000000000005,0.75,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,8,0,15,0.8,0.57999999999999996,0.75,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,8.5,0,0,0.76,0.56000000000000005,0.73,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,8.5,0,5,0.77,0.56999999999999995,0.77,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,8.5,0,10,0.77,0.59,0.78,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,8.5,0,15,0.77,0.6,0.78,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,6,0,5,0.98,0.4,0.5,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,6,0,10,0.99,0.44,0.5,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,6,0,15,0.99,0.46,0.5,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,6.5,0,0,0.93,0.42,0.56999999999999995,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,6.5,0,5,0.94,0.45,0.59,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,6.5,0,10,0.95,0.48,0.57999999999999996,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,6.5,0,15,0.95,0.49,0.59,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,7,0,0,0.89,0.46,0.65,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,7,0,5,0.9,0.5,0.66,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,7,0,10,0.91,0.52,0.66,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,7,0,15,0.91,0.53,0.67,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,7.5,0,0,0.86,0.51,0.72,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,7.5,0,5,0.87,0.54,0.73,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,7.5,0,10,0.87,0.55000000000000004,0.73,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,7.5,0,15,0.88,0.56000000000000005,0.73,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,8,0,0,0.83,0.54,0.74,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,8,0,5,0.83,0.56000000000000005,0.76,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,8,0,10,0.84,0.56999999999999995,0.78,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,8,0,15,0.84,0.59,0.78,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,8.5,0,0,0.8,0.56000000000000005,0.77,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,8.5,0,5,0.8,0.57999999999999996,0.8,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,8.5,0,10,0.81,0.59,0.8,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,8.5,0,15,0.81,0.61,0.8,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,9,0,0,0.77,0.57999999999999996,0.82,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,9,0,5,0.77,0.6,0.85,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,9,0,10,0.78,0.61,0.85,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,9,0,15,0.78,0.62,0.84,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,9.5,0,5,0.75,0.62,0.88,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,9.5,0,10,0.75,0.63,0.86,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,9.5,0,15,0.75,0.64,0.85,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,6,0,5,1.03,0.42,0.54,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,6,0,10,1.04,0.45,0.54,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,6,0,15,1.04,0.47,0.55000000000000004,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,6.5,0,0,0.97,0.44,0.61,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,6.5,0,5,0.99,0.47,0.63,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,6.5,0,10,0.99,0.5,0.63,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,6.5,0,15,1,0.51,0.63,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,7,0,0,0.93,0.49,0.69,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,7,0,5,0.95,0.52,0.7,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,7,0,10,0.95,0.53,0.71,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,7,0,15,0.96,0.55000000000000004,0.71,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,7.5,0,0,0.9,0.52,0.74,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,7.5,0,5,0.91,0.55000000000000004,0.76,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,7.5,0,10,0.92,0.56000000000000005,0.76,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,7.5,0,15,0.92,0.56999999999999995,0.76,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,8,0,0,0.87,0.55000000000000004,0.76,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,8,0,5,0.88,0.56999999999999995,0.78,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,8,0,10,0.88,0.57999999999999996,0.8,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,8,0,15,0.88,0.59,0.8,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,8.5,0,0,0.84,0.56999999999999995,0.8,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,8.5,0,5,0.84,0.57999999999999996,0.83,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,8.5,0,10,0.85,0.6,0.83,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,8.5,0,15,0.85,0.61,0.82,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,9,0,0,0.81,0.59,0.86,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,9,0,5,0.81,0.6,0.87,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,9,0,10,0.82,0.62,0.85,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,9,0,15,0.82,0.63,0.85,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,9.5,0,0,0.78,0.62,0.89,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,9.5,0,5,0.78,0.63,0.88,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,9.5,0,10,0.79,0.64,0.87,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,9.5,0,15,0.79,0.65,0.86,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,10,0,0,0.75,0.64,0.9,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,10,0,5,0.76,0.65,0.89,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,10,0,10,0.76,0.66,0.88,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,10,0,15,0.76,0.66,0.87,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,6,0,0,1.07,0.41,0.57999999999999996,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,6,0,5,1.08,0.45,0.6,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,6,0,10,1.0900000000000001,0.48,0.59,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,6,0,15,1.1000000000000001,0.49,0.6,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,6.5,0,0,1.02,0.46,0.67,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,6.5,0,5,1.04,0.49,0.68,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,6.5,0,10,1.05,0.52,0.68,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,6.5,0,15,1.05,0.53,0.68,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,7,0,0,0.98,0.51,0.74,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,7,0,5,1,0.53,0.74,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,7,0,10,1,0.55000000000000004,0.74,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,7,0,15,1.01,0.55000000000000004,0.75,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,7.5,0,0,0.95,0.53,0.78,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,7.5,0,5,0.96,0.55000000000000004,0.79,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,7.5,0,10,0.96,0.56999999999999995,0.79,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,7.5,0,15,0.97,0.57999999999999996,0.79,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,8,0,0,0.91,0.56000000000000005,0.8,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,8,0,5,0.92,0.57999999999999996,0.82,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,8,0,10,0.93,0.59,0.83,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,8,0,15,0.93,0.6,0.83,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,8.5,0,0,0.88,0.57999999999999996,0.86,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,8.5,0,5,0.89,0.59,0.86,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,8.5,0,10,0.89,0.6,0.85,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,8.5,0,15,0.89,0.61,0.85,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,9,0,0,0.85,0.6,0.88,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,9,0,5,0.86,0.61,0.88,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,9,0,10,0.86,0.63,0.87,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,9,0,15,0.86,0.63,0.86,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,9.5,0,0,0.82,0.63,0.9,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,9.5,0,5,0.83,0.64,0.9,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,9.5,0,10,0.83,0.65,0.89,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,9.5,0,15,0.83,0.65,0.87,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,10,0,0,0.79,0.65,0.91,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,10,0,5,0.8,0.66,0.91,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,10,0,10,0.8,0.66,0.89,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,10,0,15,0.8,0.66,0.88,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,6,0,0,1.1200000000000001,0.43,0.63,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,6,0,5,1.1399999999999999,0.47,0.65,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,6,0,10,1.1499999999999999,0.5,0.65,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,6,0,15,1.1599999999999999,0.51,0.65,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,6.5,0,0,1.08,0.49,0.71,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,6.5,0,5,1.1000000000000001,0.51,0.73,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,6.5,0,10,1.1000000000000001,0.54,0.73,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,6.5,0,15,1.1100000000000001,0.54,0.73,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,7,0,0,1.04,0.5,0.78,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,7,0,5,1.05,0.53,0.78,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,7,0,10,1.06,0.55000000000000004,0.78,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,7,0,15,1.06,0.56000000000000005,0.78,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,7.5,0,0,1,0.53,0.8,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,7.5,0,5,1.01,0.56000000000000005,0.82,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,7.5,0,10,1.02,0.56999999999999995,0.82,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,7.5,0,15,1.02,0.59,0.82,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,8,0,0,0.96,0.56000000000000005,0.85,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,8,0,5,0.97,0.57999999999999996,0.85,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,8,0,10,0.98,0.59,0.85,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,8,0,15,0.98,0.6,0.84,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,8.5,0,0,0.93,0.59,0.87,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,8.5,0,5,0.94,0.6,0.88,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,8.5,0,10,0.94,0.61,0.87,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,8.5,0,15,0.94,0.62,0.87,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,9,0,0,0.9,0.61,0.89,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,9,0,5,0.9,0.62,0.9,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,9,0,10,0.91,0.64,0.89,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,9,0,15,0.91,0.63,0.88,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,9.5,0,0,0.86,0.64,0.91,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,9.5,0,5,0.87,0.65,0.91,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,9.5,0,10,0.87,0.65,0.9,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,9.5,0,15,0.88,0.65,0.89,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,10,0,0,0.83,0.67,0.92,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,10,0,5,0.84,0.66,0.91,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,10,0,10,0.84,0.66,0.9,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,10,0,15,0.85,0.66,0.89,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,6,0,0,1.19,0.46,0.69,2,0.81]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,6,0,5,1.21,0.49,0.7,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,6,0,10,1.22,0.51,0.71,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,6,0,15,1.23,0.53,0.71,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,6.5,0,0,1.1399999999999999,0.49,0.76,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,6.5,0,5,1.1599999999999999,0.52,0.76,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,6.5,0,10,1.17,0.54,0.77,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,6.5,0,15,1.17,0.55000000000000004,0.77,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,7,0,0,1.1000000000000001,0.51,0.81,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,7,0,5,1.1100000000000001,0.53,0.82,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,7,0,10,1.1200000000000001,0.55000000000000004,0.81,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,7,0,15,1.1299999999999999,0.56999999999999995,0.81,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,7.5,0,0,1.06,0.54,0.83,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,7.5,0,5,1.07,0.56000000000000005,0.84,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,7.5,0,10,1.08,0.57999999999999996,0.85,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,7.5,0,15,1.08,0.59,0.84,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,8,0,0,1.02,0.56999999999999995,0.87,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,8,0,5,1.03,0.59,0.87,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,8,0,10,1.04,0.6,0.87,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,8,0,15,1.04,0.6,0.87,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,8.5,0,0,0.98,0.59,0.89,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,8.5,0,5,0.99,0.61,0.89,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,8.5,0,10,1,0.62,0.89,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,8.5,0,15,1,0.62,0.89,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,9,0,0,0.95,0.62,0.9,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,9,0,5,0.96,0.63,0.9,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,9,0,10,0.96,0.63,0.89,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,9,0,15,0.96,0.64,0.9,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,9.5,0,0,0.91,0.65,0.92,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,9.5,0,5,0.92,0.65,0.91,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,9.5,0,10,0.93,0.65,0.9,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,9.5,0,15,0.93,0.65,0.9,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,10,0,0,0.88,0.67,0.93,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,10,0,5,0.89,0.66,0.92,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,10,0,10,0.89,0.67,0.91,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,10,0,15,0.89,0.67,0.9,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,6,0,0,1.27,0.47,0.74,2,0.81]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,6,0,5,1.28,0.49,0.75,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,6,0,10,1.3,0.52,0.75,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,6,0,15,1.3,0.53,0.76,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,6.5,0,0,1.21,0.49,0.8,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,6.5,0,5,1.23,0.52,0.81,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,6.5,0,10,1.24,0.54,0.8,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,6.5,0,15,1.25,0.55000000000000004,0.8,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,7,0,0,1.17,0.51,0.83,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,7,0,5,1.18,0.54,0.84,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,7,0,10,1.19,0.56000000000000005,0.84,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,7,0,15,1.2,0.56999999999999995,0.83,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,7.5,0,0,1.1200000000000001,0.54,0.86,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,7.5,0,5,1.1399999999999999,0.56999999999999995,0.86,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,7.5,0,10,1.1399999999999999,0.59,0.87,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,7.5,0,15,1.1499999999999999,0.59,0.86,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,8,0,0,1.08,0.56999999999999995,0.88,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,8,0,5,1.0900000000000001,0.6,0.88,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,8,0,10,1.1000000000000001,0.6,0.89,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,8,0,15,1.1000000000000001,0.6,0.88,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,8.5,0,0,1.04,0.6,0.9,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,8.5,0,5,1.05,0.62,0.9,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,8.5,0,10,1.06,0.62,0.89,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,8.5,0,15,1.06,0.62,0.89,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,9,0,0,1.01,0.63,0.91,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,9,0,5,1.02,0.63,0.91,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,9,0,10,1.02,0.63,0.91,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,9,0,15,1.02,0.64,0.9,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,9.5,0,0,0.97,0.65,0.93,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,9.5,0,5,0.98,0.65,0.92,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,9.5,0,10,0.98,0.65,0.91,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,9.5,0,15,0.99,0.66,0.9,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,10,0,0,0.94,0.66,0.93,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,10,0,5,0.95,0.66,0.92,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,10,0,10,0.95,0.67,0.92,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,10,0,15,0.95,0.67,0.92,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,6,0,0,1.35,0.46,0.79,2,0.81]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,6,0,5,1.37,0.49,0.79,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,6,0,10,1.38,0.52,0.79,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,6,0,15,1.39,0.54,0.79,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,6.5,0,0,1.3,0.49,0.84,1,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,6.5,0,5,1.31,0.52,0.84,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,6.5,0,10,1.32,0.55000000000000004,0.84,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,6.5,0,15,1.33,0.55000000000000004,0.82,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,7,0,0,1.25,0.51,0.86,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,7,0,5,1.26,0.54,0.87,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,7,0,10,1.27,0.56999999999999995,0.86,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,7,0,15,1.28,0.56999999999999995,0.86,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,7.5,0,0,1.2,0.55000000000000004,0.88,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,7.5,0,5,1.21,0.57999999999999996,0.88,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,7.5,0,10,1.22,0.57999999999999996,0.88,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,7.5,0,15,1.22,0.57999999999999996,0.88,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,8,0,0,1.1599999999999999,0.59,0.9,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,8,0,5,1.17,0.6,0.89,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,8,0,10,1.17,0.6,0.89,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,8,0,15,1.18,0.6,0.89,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,8.5,0,0,1.1100000000000001,0.61,0.91,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,8.5,0,5,1.1200000000000001,0.62,0.91,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,8.5,0,10,1.1299999999999999,0.62,0.91,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,8.5,0,15,1.1299999999999999,0.62,0.89,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,9,0,0,1.07,0.63,0.93,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,9,0,5,1.08,0.63,0.92,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,9,0,10,1.0900000000000001,0.64,0.92,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,9,0,15,1.0900000000000001,0.64,0.9,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,9.5,0,0,1.04,0.65,0.94,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,9.5,0,5,1.05,0.65,0.93,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,9.5,0,10,1.05,0.65,0.93,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,9.5,0,15,1.05,0.66,0.91,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,10,0,0,1,0.66,0.94,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,10,0,5,1.01,0.67,0.93,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,10,0,10,1.01,0.67,0.94,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,10,0,15,1.01,0.67,0.93,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,6,0,0,1.44,0.46,0.83,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,6,0,5,1.47,0.49,0.83,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,6,0,10,1.48,0.52,0.83,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,6,0,15,1.49,0.53,0.82,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,6.5,0,0,1.39,0.49,0.86,1,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,6.5,0,5,1.41,0.52,0.86,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,6.5,0,10,1.42,0.55000000000000004,0.86,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,6.5,0,15,1.43,0.55000000000000004,0.85,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,7,0,0,1.33,0.52,0.87,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,7,0,5,1.35,0.56000000000000005,0.87,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,7,0,10,1.36,0.57999999999999996,0.87,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,7,0,15,1.37,0.56999999999999995,0.86,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,7.5,0,0,1.28,0.56000000000000005,0.88,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,7.5,0,5,1.3,0.57999999999999996,0.88,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,7.5,0,10,1.31,0.59,0.87,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,7.5,0,15,1.31,0.6,0.87,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,8,0,0,1.24,0.6,0.9,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,8,0,5,1.25,0.6,0.9,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,8,0,10,1.26,0.61,0.9,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,8,0,15,1.26,0.61,0.9,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,8.5,0,0,1.19,0.61,0.92,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,8.5,0,5,1.2,0.62,0.91,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,8.5,0,10,1.21,0.62,0.91,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,8.5,0,15,1.21,0.63,0.89,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,9,0,0,1.1499999999999999,0.63,0.93,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,9,0,5,1.1599999999999999,0.63,0.92,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,9,0,10,1.17,0.64,0.92,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,9,0,15,1.17,0.64,0.91,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,9.5,0,0,1.1100000000000001,0.65,0.94,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,9.5,0,5,1.1200000000000001,0.65,0.93,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,9.5,0,10,1.1200000000000001,0.66,0.94,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,9.5,0,15,1.1299999999999999,0.66,0.93,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,10,0,0,1.07,0.67,0.94,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,10,0,5,1.08,0.67,0.94,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,10,0,10,1.08,0.67,0.95,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,10,0,15,1.0900000000000001,0.67,0.94,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,6,0,0,1.56,0.46,0.86,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,6,0,5,1.58,0.5,0.85,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,6,0,10,1.6,0.52,0.86,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,6,0,15,1.6,0.53,0.85,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,6.5,0,0,1.49,0.5,0.87,1,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,6.5,0,5,1.52,0.53,0.87,1,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,6.5,0,10,1.53,0.55000000000000004,0.87,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,6.5,0,15,1.54,0.55000000000000004,0.86,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,7,0,0,1.44,0.54,0.88,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,7,0,5,1.46,0.56000000000000005,0.88,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,7,0,10,1.46,0.57999999999999996,0.87,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,7,0,15,1.47,0.57999999999999996,0.86,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,7.5,0,0,1.38,0.57999999999999996,0.9,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,7.5,0,5,1.4,0.59,0.9,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,7.5,0,10,1.41,0.6,0.89,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,7.5,0,15,1.41,0.6,0.89,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,8,0,0,1.33,0.59,0.92,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,8,0,5,1.35,0.6,0.91,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,8,0,10,1.35,0.61,0.91,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,8,0,15,1.36,0.61,0.9,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,8.5,0,0,1.28,0.61,0.94,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,8.5,0,5,1.3,0.62,0.93,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,8.5,0,10,1.3,0.63,0.92,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,8.5,0,15,1.31,0.63,0.92,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,9,0,0,1.24,0.63,0.94,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,9,0,5,1.25,0.63,0.94,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,9,0,10,1.26,0.64,0.95,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,9,0,15,1.26,0.64,0.94,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,9.5,0,0,1.2,0.65,0.94,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,9.5,0,5,1.21,0.65,0.94,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,9.5,0,10,1.21,0.66,0.95,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,9.5,0,15,1.21,0.66,0.94,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,10,0,0,1.1499999999999999,0.68,0.95,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,10,0,5,1.1599999999999999,0.68,0.94,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,10,0,10,1.17,0.69,0.95,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,10,0,15,1.17,0.69,0.94,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,6,0,0,1.69,0.47,0.86,1,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,6,0,5,1.71,0.5,0.86,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,6,0,10,1.73,0.52,0.86,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,6,0,15,1.74,0.53,0.85,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,6.5,0,0,1.62,0.51,0.88,1,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,6.5,0,5,1.64,0.53,0.87,1,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,6.5,0,10,1.65,0.55000000000000004,0.87,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,6.5,0,15,1.66,0.55000000000000004,0.86,1,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,7,0,0,1.56,0.55000000000000004,0.9,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,7,0,5,1.58,0.56000000000000005,0.89,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,7,0,10,1.59,0.56999999999999995,0.89,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,7,0,15,1.59,0.57999999999999996,0.89,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,7.5,0,0,1.5,0.56999999999999995,0.92,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,7.5,0,5,1.52,0.57999999999999996,0.91,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,7.5,0,10,1.52,0.59,0.91,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,7.5,0,15,1.53,0.6,0.9,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,8,0,0,1.44,0.59,0.94,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,8,0,5,1.46,0.6,0.93,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,8,0,10,1.47,0.61,0.92,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,8,0,15,1.47,0.62,0.92,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,8.5,0,0,1.39,0.61,0.94,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,8.5,0,5,1.4,0.62,0.94,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,8.5,0,10,1.41,0.62,0.94,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,8.5,0,15,1.41,0.63,0.93,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,9,0,0,1.34,0.63,0.95,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,9,0,5,1.35,0.64,0.94,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,9,0,10,1.36,0.64,0.95,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,9,0,15,1.36,0.64,0.94,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,9.5,0,0,1.29,0.65,0.95,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,9.5,0,5,1.31,0.65,0.94,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,9.5,0,10,1.31,0.66,0.94,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,9.5,0,15,1.31,0.66,0.94,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,10,0,0,1.25,0.68,0.95,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,10,0,5,1.26,0.68,0.94,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,10,0,10,1.27,0.68,0.94,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,10,0,15,1.27,0.69,0.93,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,6,0,0,1.84,0.48,0.88,1,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,6,0,5,1.87,0.5,0.87,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,6,0,10,1.88,0.52,0.87,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,6,0,15,1.89,0.52,0.86,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,6.5,0,0,1.77,0.52,0.9,1,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,6.5,0,5,1.79,0.53,0.89,1,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,6.5,0,10,1.8,0.54,0.89,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,6.5,0,15,1.81,0.55000000000000004,0.89,1,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,7,0,0,1.7,0.55000000000000004,0.92,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,7,0,5,1.72,0.56000000000000005,0.92,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,7,0,10,1.73,0.56999999999999995,0.91,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,7,0,15,1.74,0.57999999999999996,0.91,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,7.5,0,0,1.63,0.57999999999999996,0.93,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,7.5,0,5,1.65,0.59,0.93,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,7.5,0,10,1.66,0.6,0.93,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,7.5,0,15,1.67,0.6,0.92,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,8,0,0,1.57,0.59,0.94,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,8,0,5,1.59,0.6,0.94,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,8,0,10,1.6,0.61,0.93,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,8,0,15,1.6,0.62,0.93,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,8.5,0,0,1.52,0.62,0.95,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,8.5,0,5,1.53,0.62,0.94,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,8.5,0,10,1.54,0.63,0.94,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,8.5,0,15,1.54,0.63,0.94,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,9,0,0,1.46,0.64,0.95,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,9,0,5,1.48,0.64,0.95,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,9,0,10,1.48,0.65,0.95,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,9,0,15,1.49,0.65,0.94,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,9.5,0,0,1.41,0.66,0.95,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,9.5,0,5,1.42,0.66,0.94,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,9.5,0,10,1.43,0.67,0.95,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,9.5,0,15,1.43,0.68,0.94,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,10,0,0,1.36,0.68,0.95,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,10,0,5,1.38,0.68,0.94,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,10,0,10,1.38,0.69,0.94,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,10,0,15,1.38,0.7,0.94,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,6,0,0,2.02,0.49,0.91,1,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,6,0,5,2.0499999999999998,0.5,0.9,1,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,6,0,10,2.0699999999999998,0.52,0.89,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,6,0,15,2.08,0.53,0.89,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,6.5,0,0,1.94,0.52,0.93,1,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,6.5,0,5,1.97,0.53,0.93,1,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,6.5,0,10,1.99,0.55000000000000004,0.92,1,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,6.5,0,15,2,0.56000000000000005,0.92,1,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,7,0,0,1.87,0.55000000000000004,0.93,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,7,0,5,1.89,0.56999999999999995,0.93,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,7,0,10,1.9,0.56999999999999995,0.93,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,7,0,15,1.91,0.57999999999999996,0.92,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,7.5,0,0,1.8,0.56999999999999995,0.93,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,7.5,0,5,1.82,0.57999999999999996,0.93,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,7.5,0,10,1.83,0.59,0.93,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,7.5,0,15,1.84,0.6,0.92,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,8,0,0,1.73,0.59,0.95,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,8,0,5,1.75,0.6,0.95,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,8,0,10,1.76,0.6,0.94,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,8,0,15,1.76,0.61,0.93,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,8.5,0,0,1.67,0.61,0.95,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,8.5,0,5,1.69,0.62,0.94,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,8.5,0,10,1.69,0.63,0.94,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,8.5,0,15,1.7,0.63,0.93,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,9,0,0,1.61,0.64,0.95,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,9,0,5,1.62,0.64,0.94,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,9,0,10,1.63,0.66,0.94,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,9,0,15,1.63,0.66,0.93,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,9.5,0,0,1.55,0.66,0.95,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,9.5,0,5,1.57,0.67,0.94,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,9.5,0,10,1.57,0.68,0.95,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,9.5,0,15,1.57,0.68,0.94,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,10,0,0,1.5,0.68,0.96,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,10,0,5,1.51,0.69,0.95,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,10,0,10,1.52,0.69,0.95,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,10,0,15,1.52,0.7,0.95,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",20,6,0,0,1.01,0.39,0.52,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",21,6,0,0,0.96,0.37,0.48,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",21,9.5,0,0,0.74,0.61,0.86,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",21,10,0,0,0.72,0.63,0.89,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",21,10,0,5,0.72,0.64,0.88,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",21,10,0,10,0.72,0.65,0.87,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",21,10,0,15,0.72,0.66,0.86,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",22,6,0,0,0.92,0.34,0.43,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",22,6,0,5,0.94,0.38,0.45,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",22,6,0,10,0.94,0.42,0.45,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",22,6,0,15,0.95,0.44,0.45,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",22,6.5,0,0,0.88,0.39,0.52,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",22,9,0,0,0.73,0.56999999999999995,0.77,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",22,9,0,5,0.74,0.59,0.81,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",22,9,0,10,0.74,0.6,0.81,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",22,9,0,15,0.74,0.61,0.81,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",22,9.5,0,0,0.71,0.6,0.82,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",22,9.5,0,5,0.71,0.61,0.86,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",22,9.5,0,10,0.72,0.62,0.85,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",22,9.5,0,15,0.72,0.63,0.84,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",22,10,0,0,0.68,0.62,0.86,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",22,10,0,5,0.69,0.64,0.87,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",22,10,0,10,0.69,0.65,0.86,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",22,10,0,15,0.69,0.65,0.85,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,6,0,0,0.88,0.31,0.39,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,6,0,5,0.89,0.36,0.4,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,6,0,10,0.9,0.4,0.41,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,6,0,15,0.91,0.42,0.41,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,6.5,0,0,0.85,0.36,0.47,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,6.5,0,5,0.86,0.4,0.48,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,6.5,0,10,0.86,0.44,0.49,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,6.5,0,15,0.87,0.45,0.49,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,8.5,0,0,0.73,0.55000000000000004,0.72,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,8.5,0,5,0.73,0.56999999999999995,0.75,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,8.5,0,10,0.74,0.57999999999999996,0.76,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,8.5,0,15,0.74,0.59,0.76,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,9,0,0,0.7,0.56999999999999995,0.74,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,9,0,5,0.71,0.57999999999999996,0.78,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,9,0,10,0.71,0.6,0.79,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,9,0,15,0.71,0.61,0.79,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,9.5,0,0,0.68,0.59,0.78,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,9.5,0,5,0.68,0.6,0.82,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,9.5,0,10,0.68,0.61,0.82,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,9.5,0,15,0.69,0.62,0.81,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,10,0,0,0.65,0.61,0.84,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,10,0,5,0.66,0.62,0.86,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,10,0,10,0.66,0.64,0.85,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,10,0,15,0.66,0.64,0.84,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,6,0,0,0.84,0.28000000000000003,0.34,2,0.81]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,6,0,5,0.86,0.33,0.36,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,6,0,10,0.86,0.37,0.36,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,6,0,15,0.87,0.4,0.37,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,6.5,0,0,0.81,0.34,0.42,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,6.5,0,5,0.82,0.38,0.44,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,6.5,0,10,0.83,0.42,0.44,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,6.5,0,15,0.83,0.44,0.44,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,7,0,0,0.78,0.39,0.5,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,8,0,0,0.72,0.49,0.64,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,8,0,5,0.73,0.52,0.67,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,8,0,10,0.73,0.53,0.67,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,8,0,15,0.74,0.55000000000000004,0.67,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,8.5,0,0,0.7,0.53,0.69,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,8.5,0,5,0.7,0.55000000000000004,0.72,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,8.5,0,10,0.71,0.56999999999999995,0.73,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,8.5,0,15,0.71,0.57999999999999996,0.72,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,9,0,0,0.67,0.56000000000000005,0.72,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,9,0,5,0.68,0.56999999999999995,0.75,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,9,0,10,0.68,0.59,0.76,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,9,0,15,0.68,0.6,0.76,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,9.5,0,0,0.65,0.57999999999999996,0.75,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,9.5,0,5,0.65,0.59,0.79,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,9.5,0,10,0.66,0.6,0.8,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,9.5,0,15,0.66,0.61,0.79,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,10,0,0,0.63,0.6,0.8,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,10,0,5,0.63,0.61,0.82,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,10,0,10,0.63,0.63,0.83,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,10,0,15,0.63,0.63,0.81,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,6,0,0,0.81,0.25,0.31,2,0.81]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,6,0,5,0.82,0.31,0.32,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,6,0,10,0.83,0.35,0.33,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,6,0,15,0.83,0.38,0.34,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,6.5,0,0,0.78,0.32,0.38,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,6.5,0,5,0.79,0.36,0.4,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,6.5,0,10,0.8,0.4,0.4,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,6.5,0,15,0.8,0.42,0.4,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,7,0,0,0.75,0.36,0.45,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,7,0,5,0.76,0.41,0.47,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,7,0,10,0.76,0.44,0.47,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,7,0,15,0.77,0.46,0.48,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,7.5,0,0,0.72,0.42,0.53,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,7.5,0,5,0.73,0.46,0.55000000000000004,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,7.5,0,10,0.73,0.47,0.55000000000000004,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,7.5,0,15,0.74,0.5,0.55000000000000004,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,8,0,0,0.69,0.47,0.6,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,8,0,5,0.7,0.5,0.62,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,8,0,10,0.71,0.52,0.63,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,8,0,15,0.71,0.54,0.62,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,8.5,0,0,0.67,0.51,0.65,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,8.5,0,5,0.68,0.53,0.68,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,8.5,0,10,0.68,0.55000000000000004,0.69,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,8.5,0,15,0.68,0.56000000000000005,0.69,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,9,0,0,0.65,0.55000000000000004,0.7,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,9,0,5,0.65,0.56000000000000005,0.73,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,9,0,10,0.65,0.57999999999999996,0.74,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,9,0,15,0.66,0.59,0.73,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,9.5,0,0,0.62,0.56999999999999995,0.73,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,9.5,0,5,0.63,0.57999999999999996,0.76,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,9.5,0,10,0.63,0.6,0.77,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,9.5,0,15,0.63,0.61,0.77,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,10,0,0,0.6,0.59,0.76,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,10,0,5,0.61,0.6,0.79,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,10,0,10,0.61,0.61,0.8,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,10,0,15,0.61,0.62,0.8,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,6,0,0,0.78,0.22,0.26,2,0.81]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,6,0,5,0.79,0.28000000000000003,0.28000000000000003,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,6,0,10,0.8,0.33,0.28999999999999998,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,6,0,15,0.8,0.36,0.28999999999999998,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,6.5,0,0,0.75,0.28999999999999998,0.34,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,6.5,0,5,0.76,0.34,0.37,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,6.5,0,10,0.77,0.38,0.37,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,6.5,0,15,0.77,0.4,0.37,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,7,0,0,0.72,0.34,0.4,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,7,0,5,0.73,0.39,0.43,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,7,0,10,0.73,0.42,0.43,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,7,0,15,0.74,0.44,0.44,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,7.5,0,0,0.69,0.39,0.48,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,7.5,0,5,0.7,0.43,0.5,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,7.5,0,10,0.7,0.46,0.51,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,7.5,0,15,0.71,0.48,0.51,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,8,0,0,0.67,0.44,0.56000000000000005,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,8,0,5,0.67,0.48,0.56999999999999995,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,8,0,10,0.68,0.49,0.57999999999999996,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,8,0,15,0.68,0.52,0.57999999999999996,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,8.5,0,0,0.64,0.49,0.61,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,8.5,0,5,0.65,0.51,0.64,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,8.5,0,10,0.65,0.54,0.65,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,8.5,0,15,0.65,0.55000000000000004,0.65,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,9,0,0,0.62,0.53,0.67,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,9,0,5,0.63,0.55000000000000004,0.7,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,9,0,10,0.63,0.56999999999999995,0.71,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,9,0,15,0.63,0.57999999999999996,0.7,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,9.5,0,0,0.6,0.56000000000000005,0.71,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,9.5,0,5,0.6,0.56999999999999995,0.74,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,9.5,0,10,0.61,0.59,0.75,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,9.5,0,15,0.61,0.6,0.75,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,10,0,0,0.57999999999999996,0.57999999999999996,0.74,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,10,0,5,0.57999999999999996,0.59,0.77,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,10,0,10,0.59,0.6,0.78,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,10,0,15,0.59,0.61,0.78,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,6,0,0,0.75,0.18,0.22,2,0.81]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,6,0,5,0.76,0.25,0.25,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,6,0,10,0.77,0.31,0.25,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,6,0,15,0.77,0.34,0.26,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,6.5,0,0,0.72,0.26,0.3,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,6.5,0,5,0.73,0.32,0.33,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,6.5,0,10,0.74,0.36,0.33,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,6.5,0,15,0.74,0.39,0.34,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,7,0,0,0.69,0.33,0.37,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,7,0,5,0.7,0.37,0.39,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,7,0,10,0.71,0.41,0.4,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,7,0,15,0.71,0.43,0.4,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,7.5,0,0,0.67,0.37,0.43,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,7.5,0,5,0.67,0.41,0.46,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,7.5,0,10,0.68,0.44,0.46,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,7.5,0,15,0.68,0.46,0.47,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,8,0,0,0.64,0.42,0.51,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,8,0,5,0.65,0.46,0.53,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,8,0,10,0.65,0.47,0.54,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,8,0,15,0.66,0.5,0.54,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,8.5,0,0,0.62,0.47,0.57999999999999996,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,8.5,0,5,0.63,0.49,0.6,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,8.5,0,10,0.63,0.52,0.61,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,8.5,0,15,0.63,0.53,0.61,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,9,0,0,0.6,0.51,0.63,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,9,0,5,0.6,0.53,0.66,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,9,0,10,0.61,0.55000000000000004,0.67,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,9,0,15,0.61,0.56000000000000005,0.67,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,9.5,0,0,0.57999999999999996,0.54,0.69,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,9.5,0,5,0.57999999999999996,0.56000000000000005,0.71,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,9.5,0,10,0.57999999999999996,0.57999999999999996,0.73,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,9.5,0,15,0.57999999999999996,0.59,0.71,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,10,0,0,0.56000000000000005,0.56999999999999995,0.72,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,10,0,5,0.56000000000000005,0.57999999999999996,0.75,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,10,0,10,0.56000000000000005,0.6,0.76,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,10,0,15,0.56000000000000005,0.61,0.76,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,6,0,0,0.72,0.16,0.18,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,6,0,5,0.73,0.22,0.21,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,6,0,10,0.74,0.28000000000000003,0.22,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,6,0,15,0.74,0.32,0.22,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,6.5,0,0,0.69,0.23,0.26,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,6.5,0,5,0.7,0.28999999999999998,0.28999999999999998,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,6.5,0,10,0.71,0.34,0.28999999999999998,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,6.5,0,15,0.71,0.37,0.3,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,7,0,0,0.67,0.3,0.33,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,7,0,5,0.68,0.35,0.36,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,7,0,10,0.68,0.39,0.37,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,7,0,15,0.68,0.41,0.37,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,7.5,0,0,0.64,0.35,0.39,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,7.5,0,5,0.65,0.39,0.42,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,7.5,0,10,0.65,0.42,0.43,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,7.5,0,15,0.66,0.45,0.43,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,8,0,0,0.62,0.39,0.46,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,8,0,5,0.63,0.44,0.49,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,8,0,10,0.63,0.45,0.5,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,8,0,15,0.63,0.48,0.5,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,8.5,0,0,0.6,0.45,0.54,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,8.5,0,5,0.6,0.47,0.56000000000000005,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,8.5,0,10,0.61,0.49,0.56999999999999995,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,8.5,0,15,0.61,0.51,0.56000000000000005,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,9,0,0,0.57999999999999996,0.49,0.59,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,9,0,5,0.57999999999999996,0.51,0.62,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,9,0,10,0.57999999999999996,0.53,0.63,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,9,0,15,0.59,0.54,0.63,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,9.5,0,0,0.56000000000000005,0.53,0.65,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,9.5,0,5,0.56000000000000005,0.54,0.68,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,9.5,0,10,0.56000000000000005,0.56999999999999995,0.69,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,9.5,0,15,0.56000000000000005,0.57999999999999996,0.68,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,10,0,0,0.54,0.56000000000000005,0.71,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,10,0,5,0.54,0.57999999999999996,0.72,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,10,0,10,0.54,0.6,0.73,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,10,0,15,0.54,0.61,0.73,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,6,0,0,0.7,0.14000000000000001,0.15,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,6,0,5,0.71,0.19,0.18,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,6,0,10,0.71,0.26,0.19,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,6,0,15,0.72,0.28999999999999998,0.2,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,6.5,0,0,0.67,0.2,0.21,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,6.5,0,5,0.68,0.26,0.26,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,6.5,0,10,0.68,0.32,0.26,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,6.5,0,15,0.69,0.34,0.26,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,7,0,0,0.64,0.27,0.3,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,7,0,5,0.65,0.33,0.33,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,7,0,10,0.66,0.36,0.33,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,7,0,15,0.66,0.39,0.34,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,7.5,0,0,0.62,0.33,0.36,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,7.5,0,5,0.63,0.38,0.39,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,7.5,0,10,0.63,0.41,0.39,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,7.5,0,15,0.63,0.44,0.39,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,8,0,0,0.6,0.37,0.42,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,8,0,5,0.6,0.42,0.45,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,8,0,10,0.61,0.44,0.46,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,8,0,15,0.61,0.46,0.46,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,8.5,0,0,0.57999999999999996,0.42,0.49,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,8.5,0,5,0.57999999999999996,0.46,0.52,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,8.5,0,10,0.59,0.47,0.53,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,8.5,0,15,0.59,0.5,0.52,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,9,0,0,0.56000000000000005,0.47,0.55000000000000004,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,9,0,5,0.56000000000000005,0.49,0.59,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,9,0,10,0.56000000000000005,0.52,0.59,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,9,0,15,0.56999999999999995,0.53,0.59,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,9.5,0,0,0.54,0.51,0.61,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,9.5,0,5,0.54,0.52,0.65,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,9.5,0,10,0.54,0.55000000000000004,0.65,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,9.5,0,15,0.54,0.56000000000000005,0.65,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,10,0,0,0.52,0.54,0.68,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,10,0,5,0.52,0.56000000000000005,0.69,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,10,0,10,0.52,0.57999999999999996,0.71,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,10,0,15,0.53,0.59,0.7,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,6,0,0,0.67,0.11,0.13,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,6,0,5,0.69,0.17,0.16,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,6,0,10,0.69,0.23,0.16,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,6,0,15,0.7,0.27,0.17,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,6.5,0,0,0.65,0.17,0.18,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,6.5,0,5,0.66,0.23,0.22,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,6.5,0,10,0.66,0.3,0.23,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,6.5,0,15,0.67,0.32,0.23,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,7,0,0,0.62,0.24,0.26,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,7,0,5,0.63,0.3,0.3,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,7,0,10,0.64,0.34,0.3,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,7,0,15,0.64,0.37,0.3,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,7.5,0,0,0.6,0.31,0.33,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,7.5,0,5,0.61,0.35,0.36,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,7.5,0,10,0.61,0.38,0.37,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,7.5,0,15,0.61,0.42,0.37,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,8,0,0,0.57999999999999996,0.35,0.38,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,8,0,5,0.57999999999999996,0.39,0.42,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,8,0,10,0.59,0.42,0.42,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,8,0,15,0.59,0.44,0.42,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,8.5,0,0,0.56000000000000005,0.4,0.45,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,8.5,0,5,0.56000000000000005,0.44,0.48,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,8.5,0,10,0.56000000000000005,0.46,0.49,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,8.5,0,15,0.56999999999999995,0.48,0.49,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,9,0,0,0.54,0.45,0.52,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,9,0,5,0.54,0.47,0.55000000000000004,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,9,0,10,0.55000000000000004,0.5,0.55000000000000004,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,9,0,15,0.55000000000000004,0.51,0.55000000000000004,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,9.5,0,0,0.52,0.49,0.56999999999999995,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,9.5,0,5,0.52,0.51,0.61,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,9.5,0,10,0.53,0.53,0.62,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,9.5,0,15,0.53,0.55000000000000004,0.61,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,10,0,0,0.5,0.52,0.64,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,10,0,5,0.51,0.54,0.67,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,10,0,10,0.51,0.56000000000000005,0.67,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,10,0,15,0.51,0.57999999999999996,0.67,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,6,0,0,0.65,0.1,0.1,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,6,0,5,0.66,0.15,0.14000000000000001,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,6,0,10,0.67,0.19,0.15,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,6,0,15,0.67,0.24,0.15,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,6.5,0,0,0.63,0.15,0.15,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,6.5,0,5,0.64,0.2,0.2,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,6.5,0,10,0.64,0.26,0.2,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,6.5,0,15,0.64,0.28999999999999998,0.2,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,7,0,0,0.6,0.21,0.22,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,7,0,5,0.61,0.27,0.25,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,7,0,10,0.62,0.32,0.25,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,7,0,15,0.62,0.35,0.26,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,7.5,0,0,0.57999999999999996,0.27,0.28999999999999998,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,7.5,0,5,0.59,0.33,0.32,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,7.5,0,10,0.59,0.36,0.32,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,7.5,0,15,0.59,0.39,0.32,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,8,0,0,0.56000000000000005,0.33,0.36,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,8,0,5,0.56999999999999995,0.38,0.39,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,8,0,10,0.56999999999999995,0.4,0.4,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,8,0,15,0.56999999999999995,0.43,0.4,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,8.5,0,0,0.54,0.39,0.42,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,8.5,0,5,0.55000000000000004,0.42,0.45,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,8.5,0,10,0.55000000000000004,0.45,0.46,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,8.5,0,15,0.55000000000000004,0.47,0.45,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,9,0,0,0.52,0.43,0.48,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,9,0,5,0.53,0.45,0.51,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,9,0,10,0.53,0.48,0.51,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,9,0,15,0.53,0.5,0.51,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,9.5,0,0,0.5,0.47,0.55000000000000004,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,9.5,0,5,0.51,0.49,0.56999999999999995,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,9.5,0,10,0.51,0.52,0.57999999999999996,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,9.5,0,15,0.51,0.53,0.57999999999999996,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,10,0,0,0.49,0.52,0.6,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,10,0,5,0.49,0.53,0.62,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,10,0,10,0.49,0.55000000000000004,0.63,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,10,0,15,0.49,0.56999999999999995,0.63,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,6,0,0,0.63,0.08,0.08,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,6,0,5,0.64,0.12,0.12,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,6,0,10,0.65,0.17,0.12,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,6,0,15,0.65,0.21,0.13,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,6.5,0,0,0.61,0.13,0.12,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,6.5,0,5,0.62,0.18,0.17,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,6.5,0,10,0.62,0.24,0.18,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,6.5,0,15,0.62,0.27,0.18,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,7,0,0,0.57999999999999996,0.19,0.19,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,7,0,5,0.59,0.25,0.23,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,7,0,10,0.6,0.28999999999999998,0.23,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,7,0,15,0.6,0.33,0.23,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,7.5,0,0,0.56000000000000005,0.25,0.26,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,7.5,0,5,0.56999999999999995,0.31,0.28000000000000003,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,7.5,0,10,0.56999999999999995,0.35,0.28999999999999998,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,7.5,0,15,0.57999999999999996,0.38,0.28999999999999998,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,8,0,0,0.54,0.3,0.32,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,8,0,5,0.55000000000000004,0.36,0.35,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,8,0,10,0.55000000000000004,0.39,0.36,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,8,0,15,0.55000000000000004,0.42,0.36,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,8.5,0,0,0.52,0.36,0.39,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,8.5,0,5,0.53,0.4,0.42,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,8.5,0,10,0.53,0.43,0.43,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,8.5,0,15,0.53,0.45,0.42,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,9,0,0,0.5,0.41,0.44,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,9,0,5,0.51,0.44,0.48,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,9,0,10,0.51,0.47,0.48,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,9,0,15,0.51,0.49,0.48,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,9.5,0,0,0.49,0.45,0.5,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,9.5,0,5,0.49,0.47,0.54,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,9.5,0,10,0.49,0.5,0.54,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,9.5,0,15,0.49,0.52,0.54,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,10,0,0,0.47,0.49,0.56999999999999995,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,10,0,5,0.47,0.52,0.6,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,10,0,10,0.48,0.54,0.6,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,10,0,15,0.48,0.55000000000000004,0.6,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,6,0,0,0.61,0.06,0.06,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,6,0,5,0.62,0.1,0.1,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,6,0,10,0.63,0.15,0.1,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,6,0,15,0.63,0.19,0.11,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,6.5,0,0,0.59,0.11,0.1,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,6.5,0,5,0.6,0.16,0.15,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,6.5,0,10,0.6,0.21,0.16,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,6.5,0,15,0.61,0.24,0.16,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,7,0,0,0.56999999999999995,0.17,0.16,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,7,0,5,0.56999999999999995,0.22,0.2,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,7,0,10,0.57999999999999996,0.27,0.21,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,7,0,15,0.57999999999999996,0.31,0.21,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,7.5,0,0,0.55000000000000004,0.22,0.23,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,7.5,0,5,0.55000000000000004,0.28000000000000003,0.26,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,7.5,0,10,0.56000000000000005,0.32,0.26,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,7.5,0,15,0.56000000000000005,0.36,0.26,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,8,0,0,0.53,0.28000000000000003,0.28999999999999998,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,8,0,5,0.53,0.33,0.32,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,8,0,10,0.53,0.37,0.32,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,8,0,15,0.54,0.4,0.32,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,8.5,0,0,0.51,0.34,0.35,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,8.5,0,5,0.51,0.38,0.39,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,8.5,0,10,0.51,0.41,0.4,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,8.5,0,15,0.51,0.44,0.39,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,9,0,0,0.49,0.39,0.41,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,9,0,5,0.49,0.42,0.45,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,9,0,10,0.5,0.45,0.45,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,9,0,15,0.5,0.47,0.45,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,9.5,0,0,0.47,0.43,0.47,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,9.5,0,5,0.48,0.45,0.5,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,9.5,0,10,0.48,0.48,0.5,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,9.5,0,15,0.48,0.5,0.5,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,10,0,0,0.46,0.47,0.53,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,10,0,5,0.46,0.49,0.56000000000000005,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,10,0,10,0.46,0.52,0.56000000000000005,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,10,0,15,0.46,0.53,0.56000000000000005,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,6,0,0,0.59,0.05,0.06,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,6,0,5,0.6,0.08,7.0000000000000007E-2,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,6,0,10,0.61,0.12,0.08,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,6,0,15,0.61,0.17,0.08,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,6.5,0,0,0.56999999999999995,0.09,0.09,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,6.5,0,5,0.57999999999999996,0.13,0.12,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,6.5,0,10,0.57999999999999996,0.19,0.12,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,6.5,0,15,0.59,0.23,0.13,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,7,0,0,0.55000000000000004,0.14000000000000001,0.14000000000000001,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,7,0,5,0.56000000000000005,0.2,0.18,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,7,0,10,0.56000000000000005,0.25,0.18,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,7,0,15,0.56000000000000005,0.28000000000000003,0.18,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,7.5,0,0,0.53,0.19,0.21,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,7.5,0,5,0.54,0.26,0.24,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,7.5,0,10,0.54,0.3,0.24,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,7.5,0,15,0.54,0.33,0.24,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,8,0,0,0.51,0.26,0.26,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,8,0,5,0.52,0.32,0.3,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,8,0,10,0.52,0.35,0.3,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,8,0,15,0.52,0.38,0.3,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,8.5,0,0,0.49,0.32,0.31,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,8.5,0,5,0.5,0.36,0.35,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,8.5,0,10,0.5,0.39,0.36,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,8.5,0,15,0.5,0.42,0.36,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,9,0,0,0.48,0.36,0.37,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,9,0,5,0.48,0.39,0.41,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,9,0,10,0.48,0.43,0.42,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,9,0,15,0.48,0.45,0.42,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,9.5,0,0,0.46,0.41,0.43,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,9.5,0,5,0.46,0.43,0.48,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,9.5,0,10,0.46,0.46,0.48,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,9.5,0,15,0.47,0.48,0.48,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,10,0,0,0.44,0.45,0.5,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,10,0,5,0.45,0.47,0.54,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,10,0,10,0.45,0.5,0.54,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,10,0,15,0.45,0.51,0.54,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,6,0,0,0.57999999999999996,0.05,0.05,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,6,0,5,0.59,7.0000000000000007E-2,0.06,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,6,0,10,0.59,0.11,0.06,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,6,0,15,0.6,0.14000000000000001,7.0000000000000007E-2,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,6.5,0,0,0.55000000000000004,0.08,0.08,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,6.5,0,5,0.56000000000000005,0.12,0.1,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,6.5,0,10,0.56999999999999995,0.17,0.11,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,6.5,0,15,0.56999999999999995,0.2,0.11,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,7,0,0,0.53,0.12,0.12,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,7,0,5,0.54,0.18,0.15,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,7,0,10,0.54,0.23,0.16,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,7,0,15,0.55000000000000004,0.26,0.16,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,7.5,0,0,0.51,0.17,0.18,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,7.5,0,5,0.52,0.24,0.21,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,7.5,0,10,0.52,0.28000000000000003,0.22,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,7.5,0,15,0.53,0.31,0.22,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,8,0,0,0.49,0.23,0.24,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,8,0,5,0.5,0.3,0.27,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,8,0,10,0.5,0.32,0.27,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,8,0,15,0.51,0.36,0.27,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,8.5,0,0,0.48,0.3,0.28999999999999998,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,8.5,0,5,0.48,0.34,0.33,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,8.5,0,10,0.49,0.37,0.33,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,8.5,0,15,0.49,0.4,0.33,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,9,0,0,0.46,0.34,0.34,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,9,0,5,0.47,0.37,0.38,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,9,0,10,0.47,0.41,0.39,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,9,0,15,0.47,0.43,0.38,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,9.5,0,0,0.45,0.38,0.39,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,9.5,0,5,0.45,0.41,0.44,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,9.5,0,10,0.45,0.44,0.45,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,9.5,0,15,0.45,0.46,0.45,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,10,0,0,0.43,0.42,0.47,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,10,0,5,0.43,0.45,0.5,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,10,0,10,0.44,0.48,0.51,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,10,0,15,0.44,0.49,0.51,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,6,0,0,0.56000000000000005,0.04,0.04,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,6,0,5,0.56999999999999995,0.06,0.05,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,6,0,10,0.57999999999999996,0.09,0.05,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,6,0,15,0.57999999999999996,0.12,0.05,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,6.5,0,0,0.54,7.0000000000000007E-2,7.0000000000000007E-2,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,6.5,0,5,0.55000000000000004,0.1,0.08,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,6.5,0,10,0.55000000000000004,0.14000000000000001,0.09,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,6.5,0,15,0.55000000000000004,0.18,0.09,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,7,0,0,0.52,0.11,0.11,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,7,0,5,0.53,0.15,0.13,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,7,0,10,0.53,0.21,0.14000000000000001,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,7,0,15,0.53,0.24,0.14000000000000001,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,7.5,0,0,0.5,0.15,0.15,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,7.5,0,5,0.51,0.22,0.19,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,7.5,0,10,0.51,0.26,0.19,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,7.5,0,15,0.51,0.28999999999999998,0.19,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,8,0,0,0.48,0.21,0.21,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,8,0,5,0.49,0.27,0.24,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,8,0,10,0.49,0.3,0.25,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,8,0,15,0.49,0.34,0.25,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,8.5,0,0,0.46,0.27,0.26,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,8.5,0,5,0.47,0.32,0.3,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,8.5,0,10,0.47,0.35,0.3,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,8.5,0,15,0.47,0.38,0.3,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,9,0,0,0.45,0.33,0.31,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,9,0,5,0.45,0.36,0.35,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,9,0,10,0.46,0.4,0.36,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,9,0,15,0.46,0.42,0.36,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,9.5,0,0,0.43,0.36,0.36,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,9.5,0,5,0.44,0.39,0.41,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,9.5,0,10,0.44,0.43,0.42,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,9.5,0,15,0.44,0.44,0.41,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,10,0,0,0.42,0.4,0.43,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,10,0,5,0.42,0.44,0.47,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,10,0,10,0.42,0.46,0.48,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,10,0,15,0.42,0.47,0.47,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,6,0,0,0.55000000000000004,0.03,0.03,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,6,0,5,0.56000000000000005,0.05,0.04,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,6,0,10,0.56000000000000005,0.08,0.05,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,6,0,15,0.56000000000000005,0.1,0.05,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,6.5,0,0,0.53,0.05,0.05,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,6.5,0,5,0.53,0.08,7.0000000000000007E-2,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,6.5,0,10,0.54,0.12,0.08,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,6.5,0,15,0.54,0.16,0.08,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,7,0,0,0.51,0.09,0.08,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,7,0,5,0.51,0.13,0.11,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,7,0,10,0.52,0.17,0.12,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,7,0,15,0.52,0.21,0.12,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,7.5,0,0,0.49,0.13,0.12,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,7.5,0,5,0.49,0.19,0.16,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,7.5,0,10,0.5,0.23,0.17,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,7.5,0,15,0.5,0.27,0.17,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,8,0,0,0.47,0.19,0.18,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,8,0,5,0.47,0.25,0.21,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,8,0,10,0.48,0.28000000000000003,0.22,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,8,0,15,0.48,0.32,0.22,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,8.5,0,0,0.45,0.24,0.23,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,8.5,0,5,0.46,0.3,0.27,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,8.5,0,10,0.46,0.34,0.27,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,8.5,0,15,0.46,0.37,0.27,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,9,0,0,0.44,0.3,0.28999999999999998,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,9,0,5,0.44,0.34,0.32,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,9,0,10,0.44,0.38,0.33,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,9,0,15,0.44,0.4,0.33,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,9.5,0,0,0.42,0.35,0.34,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,9.5,0,5,0.43,0.38,0.38,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,9.5,0,10,0.43,0.42,0.39,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,9.5,0,15,0.43,0.44,0.39,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,10,0,0,0.41,0.39,0.39,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,10,0,5,0.41,0.42,0.43,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,10,0,10,0.41,0.45,0.44,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,10,0,15,0.41,0.47,0.44,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,6,0,0,0.53,0.02,0.02,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,6,0,5,0.54,0.04,0.03,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,6,0,10,0.55000000000000004,7.0000000000000007E-2,0.04,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,6,0,15,0.55000000000000004,0.09,0.04,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,6.5,0,0,0.51,0.04,0.04,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,6.5,0,5,0.52,7.0000000000000007E-2,0.06,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,6.5,0,10,0.52,0.1,7.0000000000000007E-2,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,6.5,0,15,0.53,0.13,7.0000000000000007E-2,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,7,0,0,0.49,7.0000000000000007E-2,7.0000000000000007E-2,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,7,0,5,0.5,0.11,0.09,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,7,0,10,0.5,0.15,0.11,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,7,0,15,0.5,0.18,0.11,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,7.5,0,0,0.47,0.11,0.1,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,7.5,0,5,0.48,0.17,0.14000000000000001,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,7.5,0,10,0.48,0.2,0.15,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,7.5,0,15,0.48,0.24,0.15,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,8,0,0,0.46,0.17,0.15,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,8,0,5,0.46,0.22,0.19,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,8,0,10,0.46,0.25,0.2,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,8,0,15,0.47,0.3,0.2,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,8.5,0,0,0.44,0.22,0.21,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,8.5,0,5,0.45,0.27,0.24,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,8.5,0,10,0.45,0.31,0.25,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,8.5,0,15,0.45,0.35,0.25,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,9,0,0,0.43,0.28000000000000003,0.26,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,9,0,5,0.43,0.32,0.3,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,9,0,10,0.43,0.36,0.3,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,9,0,15,0.43,0.38,0.3,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,9.5,0,0,0.41,0.33,0.31,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,9.5,0,5,0.41,0.36,0.35,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,9.5,0,10,0.42,0.4,0.36,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,9.5,0,15,0.42,0.42,0.36,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,10,0,0,0.4,0.37,0.37,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,10,0,5,0.4,0.4,0.4,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,10,0,10,0.4,0.44,0.41,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,10,0,15,0.4,0.45,0.41,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,6,0,0,0.52,0.02,0.02,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,6,0,5,0.53,0.03,0.03,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,6,0,10,0.53,0.06,0.03,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,6,0,15,0.54,7.0000000000000007E-2,0.03,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,6.5,0,0,0.5,0.04,0.03,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,6.5,0,5,0.51,0.06,0.05,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,6.5,0,10,0.51,0.09,0.06,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,6.5,0,15,0.51,0.12,0.06,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,7,0,0,0.48,0.06,0.06,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,7,0,5,0.49,0.09,0.08,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,7,0,10,0.49,0.13,0.09,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,7,0,15,0.49,0.16,0.09,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,7.5,0,0,0.46,0.1,0.09,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,7.5,0,5,0.47,0.15,0.12,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,7.5,0,10,0.47,0.18,0.13,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,7.5,0,15,0.47,0.22,0.13,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,8,0,0,0.44,0.15,0.13,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,8,0,5,0.45,0.2,0.17,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,8,0,10,0.45,0.23,0.18,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,8,0,15,0.45,0.27,0.18,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,8.5,0,0,0.43,0.2,0.18,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,8.5,0,5,0.43,0.25,0.22,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,8.5,0,10,0.44,0.28999999999999998,0.23,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,8.5,0,15,0.44,0.32,0.22,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,9,0,0,0.41,0.26,0.23,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,9,0,5,0.42,0.3,0.27,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,9,0,10,0.42,0.34,0.27,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,9,0,15,0.42,0.37,0.27,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,9.5,0,0,0.4,0.31,0.28999999999999998,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,9.5,0,5,0.4,0.34,0.33,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,9.5,0,10,0.41,0.38,0.33,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,9.5,0,15,0.41,0.4,0.33,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,10,0,0,0.39,0.35,0.34,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,10,0,5,0.39,0.39,0.38,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,10,0,10,0.39,0.42,0.39,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,10,0,15,0.39,0.44,0.38,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,6,0,0,0.51,0.02,0.02,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,6,0,5,0.51,0.03,0.02,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,6,0,10,0.52,0.05,0.02,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,6,0,15,0.52,7.0000000000000007E-2,0.02,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,6.5,0,0,0.49,0.04,0.03,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,6.5,0,5,0.49,0.05,0.04,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,6.5,0,10,0.5,0.08,0.04,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,6.5,0,15,0.5,0.1,0.04,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,7,0,0,0.47,0.06,0.05,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,7,0,5,0.47,0.08,7.0000000000000007E-2,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,7,0,10,0.48,0.11,7.0000000000000007E-2,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,7,0,15,0.48,0.14000000000000001,7.0000000000000007E-2,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,7.5,0,0,0.45,0.09,0.08,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,7.5,0,5,0.46,0.13,0.11,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,7.5,0,10,0.46,0.16,0.11,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,7.5,0,15,0.46,0.21,0.11,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,8,0,0,0.43,0.13,0.12,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,8,0,5,0.44,0.18,0.15,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,8,0,10,0.44,0.22,0.16,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,8,0,15,0.44,0.25,0.16,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,8.5,0,0,0.42,0.17,0.17,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,8.5,0,5,0.42,0.23,0.2,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,8.5,0,10,0.43,0.27,0.21,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,8.5,0,15,0.43,0.3,0.21,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,9,0,0,0.4,0.23,0.22,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,9,0,5,0.41,0.28000000000000003,0.25,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,9,0,10,0.41,0.32,0.25,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,9,0,15,0.41,0.35,0.25,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,9.5,0,0,0.39,0.28999999999999998,0.26,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,9.5,0,5,0.39,0.32,0.3,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,9.5,0,10,0.4,0.36,0.3,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,9.5,0,15,0.4,0.39,0.3,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,10,0,0,0.38,0.33,0.31,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,10,0,5,0.38,0.36,0.35,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,10,0,10,0.38,0.4,0.36,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,10,0,15,0.38,0.42,0.36,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,6,0,0,0.49,0.02,0.01,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,6,0,5,0.5,0.03,0.02,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,6,0,10,0.51,0.04,0.02,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,6,0,15,0.51,0.06,0.02,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,6.5,0,0,0.47,0.03,0.02,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,6.5,0,5,0.48,0.04,0.03,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,6.5,0,10,0.48,7.0000000000000007E-2,0.04,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,6.5,0,15,0.49,0.08,0.03,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,7,0,0,0.46,0.05,0.04,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,7,0,5,0.46,7.0000000000000007E-2,0.06,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,7,0,10,0.47,0.1,0.06,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,7,0,15,0.47,0.12,0.06,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,7.5,0,0,0.44,0.08,7.0000000000000007E-2,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,7.5,0,5,0.45,0.11,0.09,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,7.5,0,10,0.45,0.14000000000000001,0.09,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,7.5,0,15,0.45,0.18,0.09,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,8,0,0,0.42,0.12,0.11,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,8,0,5,0.43,0.16,0.13,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,8,0,10,0.43,0.2,0.14000000000000001,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,8,0,15,0.43,0.24,0.14000000000000001,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,8.5,0,0,0.41,0.16,0.15,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,8.5,0,5,0.41,0.21,0.18,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,8.5,0,10,0.41,0.25,0.19,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,8.5,0,15,0.42,0.28000000000000003,0.19,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,9,0,0,0.39,0.21,0.19,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,9,0,5,0.4,0.26,0.23,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,9,0,10,0.4,0.3,0.23,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,9,0,15,0.4,0.33,0.23,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,9.5,0,0,0.38,0.27,0.24,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,9.5,0,5,0.38,0.31,0.28000000000000003,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,9.5,0,10,0.39,0.34,0.28000000000000003,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,9.5,0,15,0.39,0.37,0.28000000000000003,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,10,0,0,0.37,0.32,0.28999999999999998,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,10,0,5,0.37,0.35,0.33,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,10,0,10,0.37,0.38,0.33,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,10,0,15,0.37,0.41,0.33,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,6,0,0,0.48,0.02,0.01,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,6,0,5,0.49,0.03,0.02,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,6,0,10,0.49,0.04,0.02,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,6,0,15,0.5,0.05,0.02,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,6.5,0,0,0.46,0.03,0.02,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,6.5,0,5,0.47,0.04,0.03,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,6.5,0,10,0.47,0.06,0.03,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,6.5,0,15,0.48,7.0000000000000007E-2,0.03,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,7,0,0,0.45,0.04,0.04,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,7,0,5,0.45,0.06,0.05,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,7,0,10,0.45,0.09,0.05,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,7,0,15,0.46,0.11,0.05,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,7.5,0,0,0.43,7.0000000000000007E-2,0.06,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,7.5,0,5,0.43,0.1,0.08,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,7.5,0,10,0.44,0.13,0.08,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,7.5,0,15,0.44,0.16,0.08,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,8,0,0,0.41,0.1,0.09,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,8,0,5,0.42,0.14000000000000001,0.12,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,8,0,10,0.42,0.18,0.12,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,8,0,15,0.42,0.22,0.12,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,8.5,0,0,0.4,0.14000000000000001,0.13,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,8.5,0,5,0.4,0.19,0.16,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,8.5,0,10,0.4,0.23,0.17,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,8.5,0,15,0.41,0.26,0.17,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,9,0,0,0.39,0.19,0.17,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,9,0,5,0.39,0.24,0.21,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,9,0,10,0.39,0.28000000000000003,0.21,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,9,0,15,0.39,0.31,0.21,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,9.5,0,0,0.37,0.24,0.22,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,9.5,0,5,0.37,0.28999999999999998,0.25,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,9.5,0,10,0.38,0.32,0.26,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,9.5,0,15,0.38,0.35,0.25,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,10,0,0,0.36,0.3,0.27,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,10,0,5,0.36,0.33,0.3,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,10,0,10,0.36,0.37,0.31,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,10,0,15,0.36,0.39,0.3,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,6,0,0,0.47,0.02,0.01,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,6,0,5,0.48,0.02,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,6,0,10,0.48,0.03,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,6,0,15,0.49,0.04,0.02,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,6.5,0,0,0.45,0.02,0.02,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,6.5,0,5,0.46,0.03,0.02,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,6.5,0,10,0.46,0.05,0.02,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,6.5,0,15,0.46,0.06,0.02,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,7,0,0,0.44,0.03,0.03,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,7,0,5,0.44,0.05,0.04,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,7,0,10,0.44,7.0000000000000007E-2,0.04,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,7,0,15,0.45,0.09,0.04,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,7.5,0,0,0.42,0.05,0.05,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,7.5,0,5,0.42,0.08,0.06,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,7.5,0,10,0.43,0.11,7.0000000000000007E-2,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,7.5,0,15,0.43,0.14000000000000001,7.0000000000000007E-2,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,8,0,0,0.4,0.08,7.0000000000000007E-2,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,8,0,5,0.41,0.12,0.09,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,8,0,10,0.41,0.15,0.11,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,8,0,15,0.41,0.19,0.11,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,8.5,0,0,0.39,0.12,0.1,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,8.5,0,5,0.39,0.17,0.14000000000000001,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,8.5,0,10,0.4,0.2,0.15,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,8.5,0,15,0.4,0.24,0.15,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,9,0,0,0.38,0.17,0.15,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,9,0,5,0.38,0.21,0.18,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,9,0,10,0.38,0.26,0.19,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,9,0,15,0.38,0.28999999999999998,0.19,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,9.5,0,0,0.36,0.22,0.19,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,9.5,0,5,0.37,0.26,0.23,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,9.5,0,10,0.37,0.31,0.24,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,9.5,0,15,0.37,0.34,0.24,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,10,0,0,0.35,0.27,0.25,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,10,0,5,0.35,0.31,0.28000000000000003,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,10,0,10,0.35,0.35,0.28999999999999998,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,10,0,15,0.36,0.37,0.28999999999999998,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,6,0,0,0.46,0.02,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,6,0,5,0.47,0.02,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,6,0,10,0.47,0.03,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,6,0,15,0.47,0.03,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,6.5,0,0,0.44,0.02,0.02,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,6.5,0,5,0.45,0.03,0.02,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,6.5,0,10,0.45,0.04,0.02,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,6.5,0,15,0.45,0.05,0.02,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,7,0,0,0.43,0.03,0.02,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,7,0,5,0.43,0.04,0.03,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,7,0,10,0.43,0.06,0.04,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,7,0,15,0.44,0.08,0.04,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,7.5,0,0,0.41,0.04,0.04,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,7.5,0,5,0.41,7.0000000000000007E-2,0.05,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,7.5,0,10,0.42,0.09,0.06,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,7.5,0,15,0.42,0.12,0.06,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,8,0,0,0.39,7.0000000000000007E-2,0.06,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,8,0,5,0.4,0.1,0.08,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,8,0,10,0.4,0.14000000000000001,0.09,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,8,0,15,0.4,0.17,0.09,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,8.5,0,0,0.38,0.11,0.09,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,8.5,0,5,0.38,0.15,0.12,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,8.5,0,10,0.39,0.18,0.13,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,8.5,0,15,0.39,0.22,0.13,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,9,0,0,0.37,0.16,0.13,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,9,0,5,0.37,0.19,0.16,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,9,0,10,0.37,0.24,0.17,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,9,0,15,0.37,0.27,0.17,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,9.5,0,0,0.35,0.2,0.17,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,9.5,0,5,0.36,0.24,0.22,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,9.5,0,10,0.36,0.28999999999999998,0.22,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,9.5,0,15,0.36,0.32,0.22,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,10,0,0,0.34,0.25,0.23,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,10,0,5,0.35,0.28999999999999998,0.26,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,10,0,10,0.35,0.33,0.27,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,10,0,15,0.35,0.36,0.27,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,6,0,0,0.45,0.01,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,6,0,5,0.46,0.02,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,6,0,10,0.46,0.02,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,6,0,15,0.46,0.03,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,6.5,0,0,0.43,0.02,0.01,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,6.5,0,5,0.44,0.02,0.02,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,6.5,0,10,0.44,0.04,0.02,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,6.5,0,15,0.44,0.05,0.02,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,7,0,0,0.42,0.02,0.02,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,7,0,5,0.42,0.04,0.03,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,7,0,10,0.42,0.05,0.03,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,7,0,15,0.43,7.0000000000000007E-2,0.03,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,7.5,0,0,0.4,0.04,0.03,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,7.5,0,5,0.41,0.06,0.05,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,7.5,0,10,0.41,0.08,0.05,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,7.5,0,15,0.41,0.11,0.05,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,8,0,0,0.39,0.06,0.05,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,8,0,5,0.39,0.09,7.0000000000000007E-2,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,8,0,10,0.39,0.12,0.08,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,8,0,15,0.39,0.15,0.08,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,8.5,0,0,0.37,0.1,0.08,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,8.5,0,5,0.38,0.13,0.1,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,8.5,0,10,0.38,0.17,0.12,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,8.5,0,15,0.38,0.2,0.12,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,9,0,0,0.36,0.13,0.11,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,9,0,5,0.36,0.18,0.15,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,9,0,10,0.36,0.21,0.16,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,9,0,15,0.37,0.25,0.15,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,9.5,0,0,0.35,0.18,0.15,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,9.5,0,5,0.35,0.22,0.19,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,9.5,0,10,0.35,0.27,0.2,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,9.5,0,15,0.35,0.3,0.2,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,10,0,0,0.34,0.23,0.2,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,10,0,5,0.34,0.27,0.24,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,10,0,10,0.34,0.31,0.25,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,10,0,15,0.34,0.34,0.24,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,6,0,0,0.44,0.01,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,6,0,5,0.45,0.02,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,6,0,10,0.45,0.02,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,6,0,15,0.45,0.03,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,6.5,0,0,0.42,0.02,0.01,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,6.5,0,5,0.43,0.02,0.02,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,6.5,0,10,0.43,0.03,0.02,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,6.5,0,15,0.43,0.04,0.02,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,7,0,0,0.41,0.02,0.02,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,7,0,5,0.41,0.04,0.02,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,7,0,10,0.42,0.05,0.03,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,7,0,15,0.42,7.0000000000000007E-2,0.03,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,7.5,0,0,0.39,0.04,0.03,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,7.5,0,5,0.4,0.06,0.04,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,7.5,0,10,0.4,7.0000000000000007E-2,0.04,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,7.5,0,15,0.4,0.1,0.04,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,8,0,0,0.38,0.06,0.04,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,8,0,5,0.38,0.08,0.06,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,8,0,10,0.38,0.11,7.0000000000000007E-2,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,8,0,15,0.38,0.14000000000000001,7.0000000000000007E-2,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,8.5,0,0,0.36,0.09,7.0000000000000007E-2,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,8.5,0,5,0.37,0.12,0.09,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,8.5,0,10,0.37,0.15,0.1,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,8.5,0,15,0.37,0.19,0.1,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,9,0,0,0.35,0.13,0.1,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,9,0,5,0.36,0.16,0.13,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,9,0,10,0.36,0.2,0.14000000000000001,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,9,0,15,0.36,0.23,0.14000000000000001,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,9.5,0,0,0.34,0.17,0.14000000000000001,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,9.5,0,5,0.34,0.21,0.17,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,9.5,0,10,0.34,0.25,0.19,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,9.5,0,15,0.34,0.28000000000000003,0.18,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,10,0,0,0.33,0.21,0.18,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,10,0,5,0.33,0.25,0.21,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,10,0,10,0.33,0.3,0.23,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,10,0,15,0.33,0.32,0.22,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,6,0,0,0.43,0.01,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,6,0,5,0.44,0.02,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,6,0,10,0.44,0.02,0.01,5,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,6,0,15,0.44,0.02,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,6.5,0,0,0.41,0.02,0.01,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,6.5,0,5,0.42,0.02,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,6.5,0,10,0.42,0.03,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,6.5,0,15,0.43,0.04,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,7,0,0,0.4,0.02,0.01,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,7,0,5,0.4,0.03,0.02,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,7,0,10,0.41,0.04,0.02,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,7,0,15,0.41,0.06,0.02,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,7.5,0,0,0.38,0.03,0.02,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,7.5,0,5,0.39,0.05,0.03,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,7.5,0,10,0.39,7.0000000000000007E-2,0.04,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,7.5,0,15,0.39,0.09,0.04,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,8,0,0,0.37,0.05,0.04,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,8,0,5,0.37,0.08,0.05,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,8,0,10,0.38,0.09,0.06,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,8,0,15,0.38,0.12,0.06,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,8.5,0,0,0.36,0.08,0.06,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,8.5,0,5,0.36,0.11,0.08,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,8.5,0,10,0.36,0.13,0.09,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,8.5,0,15,0.36,0.17,0.09,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,9,0,0,0.34,0.11,0.09,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,9,0,5,0.35,0.14000000000000001,0.11,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,9,0,10,0.35,0.19,0.12,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,9,0,15,0.35,0.22,0.12,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,9.5,0,0,0.33,0.15,0.12,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,9.5,0,5,0.34,0.19,0.15,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,9.5,0,10,0.34,0.23,0.17,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,9.5,0,15,0.34,0.26,0.17,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,10,0,0,0.32,0.19,0.16,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,10,0,5,0.32,0.24,0.2,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,10,0,10,0.32,0.28000000000000003,0.21,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,10,0,15,0.33,0.3,0.2,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,6,0,0,0.42,0.01,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,6,0,5,0.43,0.01,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,6,0,10,0.43,0.02,0.01,5,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,6,0,15,0.44,0.02,0.01,5,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,6.5,0,0,0.4,0.01,0.01,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,6.5,0,5,0.41,0.02,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,6.5,0,10,0.41,0.03,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,6.5,0,15,0.42,0.03,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,7,0,0,0.39,0.02,0.01,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,7,0,5,0.4,0.03,0.02,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,7,0,10,0.4,0.04,0.02,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,7,0,15,0.4,0.05,0.02,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,7.5,0,0,0.38,0.03,0.02,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,7.5,0,5,0.38,0.04,0.03,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,7.5,0,10,0.38,0.06,0.03,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,7.5,0,15,0.38,0.08,0.03,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,8,0,0,0.36,0.05,0.03,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,8,0,5,0.37,7.0000000000000007E-2,0.04,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,8,0,10,0.37,0.08,0.05,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,8,0,15,0.37,0.11,0.05,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,8.5,0,0,0.35,7.0000000000000007E-2,0.05,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,8.5,0,5,0.35,0.09,7.0000000000000007E-2,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,8.5,0,10,0.35,0.12,0.08,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,8.5,0,15,0.35,0.15,7.0000000000000007E-2,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,9,0,0,0.34,0.1,0.08,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,9,0,5,0.34,0.13,0.1,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,9,0,10,0.34,0.16,0.11,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,9,0,15,0.34,0.2,0.11,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,9.5,0,0,0.33,0.14000000000000001,0.11,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,9.5,0,5,0.33,0.17,0.14000000000000001,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,9.5,0,10,0.33,0.21,0.15,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,9.5,0,15,0.33,0.24,0.15,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,10,0,0,0.31,0.17,0.15,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,10,0,5,0.32,0.22,0.18,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,10,0,10,0.32,0.26,0.19,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,10,0,15,0.32,0.28000000000000003,0.19,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,6,0,0,0.41,0.01,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,6,0,5,0.42,0.01,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,6,0,10,0.42,0.02,0.01,5,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,6,0,15,0.43,0.02,0.01,5,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,6.5,0,0,0.4,0.01,0.01,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,6.5,0,5,0.4,0.02,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,6.5,0,10,0.41,0.02,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,6.5,0,15,0.41,0.03,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,7,0,0,0.38,0.02,0.01,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,7,0,5,0.39,0.02,0.02,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,7,0,10,0.39,0.03,0.02,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,7,0,15,0.39,0.04,0.02,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,7.5,0,0,0.37,0.02,0.02,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,7.5,0,5,0.37,0.03,0.02,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,7.5,0,10,0.37,0.05,0.03,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,7.5,0,15,0.38,0.06,0.03,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,8,0,0,0.35,0.03,0.03,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,8,0,5,0.36,0.05,0.04,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,8,0,10,0.36,7.0000000000000007E-2,0.04,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,8,0,15,0.36,0.09,0.04,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,8.5,0,0,0.34,0.05,0.04,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,8.5,0,5,0.35,0.08,0.06,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,8.5,0,10,0.35,0.1,7.0000000000000007E-2,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,8.5,0,15,0.35,0.13,7.0000000000000007E-2,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,9,0,0,0.33,0.08,0.06,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,9,0,5,0.33,0.11,0.08,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,9,0,10,0.34,0.15,0.1,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,9,0,15,0.34,0.17,0.09,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,9.5,0,0,0.32,0.12,0.09,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,9.5,0,5,0.32,0.15,0.12,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,9.5,0,10,0.32,0.19,0.13,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,9.5,0,15,0.32,0.22,0.13,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,10,0,0,0.31,0.16,0.13,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,10,0,5,0.31,0.2,0.16,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,10,0,10,0.31,0.24,0.17,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,10,0,15,0.31,0.26,0.17,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,6,0,0,0.4,0.01,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,6,0,5,0.41,0.01,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,6,0,10,0.42,0.02,0.01,5,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,6,0,15,0.42,0.02,0.01,5,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,6.5,0,0,0.39,0.01,0.01,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,6.5,0,5,0.4,0.02,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,6.5,0,10,0.4,0.02,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,6.5,0,15,0.4,0.03,0.01,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,7,0,0,0.37,0.02,0.01,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,7,0,5,0.38,0.02,0.01,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,7,0,10,0.38,0.03,0.01,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,7,0,15,0.38,0.04,0.01,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,7.5,0,0,0.36,0.02,0.02,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,7.5,0,5,0.37,0.03,0.02,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,7.5,0,10,0.37,0.04,0.02,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,7.5,0,15,0.37,0.05,0.02,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,8,0,0,0.35,0.03,0.02,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,8,0,5,0.35,0.05,0.03,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,8,0,10,0.35,0.06,0.04,3,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,8,0,15,0.35,0.08,0.04,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,8.5,0,0,0.34,0.05,0.04,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,8.5,0,5,0.34,7.0000000000000007E-2,0.05,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,8.5,0,10,0.34,0.09,0.06,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,8.5,0,15,0.34,0.12,0.06,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,9,0,0,0.32,7.0000000000000007E-2,0.06,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,9,0,5,0.33,0.1,7.0000000000000007E-2,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,9,0,10,0.33,0.13,0.08,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,9,0,15,0.33,0.16,0.08,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,9.5,0,0,0.31,0.1,0.08,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,9.5,0,5,0.32,0.14000000000000001,0.11,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,9.5,0,10,0.32,0.17,0.12,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,9.5,0,15,0.32,0.2,0.12,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,10,0,0,0.3,0.14000000000000001,0.11,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,10,0,5,0.3,0.18,0.14000000000000001,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,10,0,10,0.31,0.22,0.16,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,10,0,15,0.31,0.24,0.15,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",41,10,0,0,0.82,0.59,0.5,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",40,10,0,0,0.84,0.61,0.51,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",40,10,0,5,0.85,0.6,0.51,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",40,10,0,10,0.86,0.59,0.51,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",40,10,0,15,0.86,0.59,0.51,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",39,9.5,0,0,0.89,0.59,0.5,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",39,9.5,0,5,0.9,0.59,0.5,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",39,9.5,0,10,0.91,0.57999999999999996,0.5,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",39,9.5,0,15,0.91,0.56000000000000005,0.5,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",39,10,0,0,0.86,0.62,0.52,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",39,10,0,5,0.87,0.61,0.52,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",39,10,0,10,0.88,0.6,0.53,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",39,10,0,15,0.88,0.59,0.53,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",38,9.5,0,0,0.92,0.6,0.5,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",38,9.5,0,5,0.93,0.59,0.51,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",38,9.5,0,10,0.93,0.57999999999999996,0.51,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",38,9.5,0,15,0.93,0.57999999999999996,0.51,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",38,10,0,0,0.89,0.64,0.53,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",38,10,0,5,0.9,0.63,0.54,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",38,10,0,10,0.9,0.62,0.54,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",38,10,0,15,0.9,0.6,0.54,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",37,9,0,0,0.97,0.59,0.5,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",37,9,0,5,0.98,0.57999999999999996,0.5,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",37,9,0,10,0.99,0.56999999999999995,0.5,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",37,9,0,15,0.99,0.56000000000000005,0.5,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",37,9.5,0,0,0.94,0.62,0.52,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",37,9.5,0,5,0.95,0.61,0.52,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",37,9.5,0,10,0.96,0.6,0.53,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",37,9.5,0,15,0.96,0.57999999999999996,0.53,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",37,10,0,0,0.91,0.65,0.55000000000000004,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",37,10,0,5,0.92,0.66,0.55000000000000004,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",37,10,0,10,0.92,0.65,0.55000000000000004,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",37,10,0,15,0.93,0.63,0.56000000000000005,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",36,9,0,10,1.02,0.57999999999999996,0.5,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",36,9,0,15,1.02,0.56999999999999995,0.5,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",36,9.5,0,0,0.97,0.63,0.53,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",36,9.5,0,5,0.98,0.63,0.53,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",36,9.5,0,10,0.98,0.63,0.53,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",36,9.5,0,15,0.99,0.61,0.53,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",36,10,0,0,0.94,0.67,0.56000000000000005,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",36,10,0,5,0.95,0.67,0.56000000000000005,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",36,10,0,10,0.95,0.66,0.56000000000000005,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",36,10,0,15,0.95,0.66,0.56000000000000005,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",35,9,0,0,1.03,0.61,0.51,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",35,9,0,5,1.04,0.62,0.52,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",35,9,0,10,1.05,0.61,0.52,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",35,9,0,15,1.05,0.59,0.52,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",35,9.5,0,0,0.99,0.65,0.55000000000000004,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",35,9.5,0,5,1.01,0.65,0.55000000000000004,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",35,9.5,0,10,1.01,0.64,0.55000000000000004,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",35,9.5,0,15,1.01,0.65,0.55000000000000004,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",35,10,0,0,0.96,0.69,0.59,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",35,10,0,5,0.97,0.69,0.59,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",35,10,0,10,0.98,0.68,0.6,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",35,10,0,15,0.98,0.68,0.6,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",34,8.5,0,0,1.1000000000000001,0.59,0.5,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",34,8.5,0,5,1.1100000000000001,0.59,0.5,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",34,8.5,0,10,1.1200000000000001,0.57999999999999996,0.5,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",34,8.5,0,15,1.1200000000000001,0.56000000000000005,0.51,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",34,9,0,0,1.06,0.63,0.53,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",34,9,0,5,1.07,0.63,0.53,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",34,9,0,10,1.08,0.63,0.53,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",34,9,0,15,1.08,0.61,0.54,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",34,9.5,0,0,1.02,0.67,0.56999999999999995,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",34,9.5,0,5,1.04,0.67,0.56999999999999995,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",34,9.5,0,10,1.04,0.66,0.57999999999999996,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",34,9.5,0,15,1.04,0.66,0.57999999999999996,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",34,10,0,0,0.99,0.73,0.63,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",34,10,0,5,1,0.72,0.63,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",34,10,0,10,1.01,0.71,0.63,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",34,10,0,15,1.01,0.7,0.63,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",33,8.5,0,0,1.1299999999999999,0.61,0.52,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",33,8.5,0,5,1.1399999999999999,0.61,0.52,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",33,8.5,0,10,1.1499999999999999,0.61,0.51,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",33,8.5,0,15,1.1499999999999999,0.6,0.51,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",33,9,0,0,1.0900000000000001,0.65,0.55000000000000004,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",33,9,0,5,1.1000000000000001,0.64,0.55000000000000004,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",33,9,0,10,1.1100000000000001,0.64,0.55000000000000004,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",33,9,0,15,1.1100000000000001,0.63,0.55000000000000004,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",33,9.5,0,0,1.05,0.71,0.6,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",33,9.5,0,5,1.06,0.7,0.61,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",33,9.5,0,10,1.07,0.69,0.6,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",33,9.5,0,15,1.07,0.68,0.6,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",33,10,0,0,1.02,0.75,0.65,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",33,10,0,5,1.03,0.76,0.65,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",33,10,0,10,1.04,0.76,0.66,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",33,10,0,15,1.04,0.73,0.65,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",32,8,0,0,1.2,0.59,0.5,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",32,8,0,5,1.22,0.59,0.5,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",32,8,0,10,1.23,0.59,0.5,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",32,8,0,15,1.23,0.57999999999999996,0.5,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",32,8.5,0,0,1.1599999999999999,0.63,0.54,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",32,8.5,0,5,1.18,0.62,0.54,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",32,8.5,0,10,1.19,0.62,0.53,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",32,8.5,0,15,1.19,0.62,0.54,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",32,9,0,0,1.1200000000000001,0.68,0.57999999999999996,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",32,9,0,5,1.1399999999999999,0.68,0.59,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",32,9,0,10,1.1399999999999999,0.67,0.57999999999999996,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",32,9,0,15,1.1499999999999999,0.65,0.57999999999999996,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",32,9.5,0,0,1.0900000000000001,0.75,0.64,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",32,9.5,0,5,1.1000000000000001,0.74,0.65,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",32,9.5,0,10,1.1000000000000001,0.73,0.65,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",32,9.5,0,15,1.1100000000000001,0.71,0.65,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",32,10,0,0,1.05,0.78,0.68,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",32,10,0,5,1.06,0.78,0.68,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",32,10,0,10,1.07,0.77,0.69,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",32,10,0,15,1.07,0.77,0.68,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",31,8,0,0,1.24,0.61,0.52,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",31,8,0,5,1.26,0.61,0.52,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",31,8,0,10,1.27,0.61,0.52,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",31,8,0,15,1.27,0.6,0.52,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",31,8.5,0,0,1.2,0.65,0.56000000000000005,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",31,8.5,0,5,1.22,0.65,0.56000000000000005,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",31,8.5,0,10,1.22,0.64,0.56000000000000005,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",31,8.5,0,15,1.23,0.63,0.56000000000000005,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",31,9,0,0,1.1599999999999999,0.72,0.62,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",31,9,0,5,1.17,0.71,0.62,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",31,9,0,10,1.18,0.7,0.62,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",31,9,0,15,1.18,0.69,0.62,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",31,9.5,0,0,1.1200000000000001,0.77,0.67,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",31,9.5,0,5,1.1299999999999999,0.77,0.67,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",31,9.5,0,10,1.1399999999999999,0.76,0.67,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",31,9.5,0,15,1.1399999999999999,0.75,0.67,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",31,10,0,0,1.0900000000000001,0.8,0.71,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",31,10,0,5,1.1000000000000001,0.8,0.72,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",31,10,0,10,1.1000000000000001,0.79,0.72,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",31,10,0,15,1.1000000000000001,0.79,0.71,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,7.5,0,0,1.33,0.59,0.51,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,7.5,0,5,1.35,0.57999999999999996,0.51,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,7.5,0,10,1.36,0.57999999999999996,0.5,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,7.5,0,15,1.37,0.56999999999999995,0.5,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,8,0,0,1.29,0.63,0.55000000000000004,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,8,0,5,1.3,0.63,0.55000000000000004,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,8,0,10,1.31,0.62,0.55000000000000004,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,8,0,15,1.32,0.61,0.55000000000000004,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,8.5,0,0,1.24,0.7,0.61,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,8.5,0,5,1.26,0.7,0.61,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,8.5,0,10,1.26,0.69,0.61,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,8.5,0,15,1.27,0.67,0.61,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,9,0,0,1.2,0.76,0.65,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,9,0,5,1.21,0.76,0.66,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,9,0,10,1.22,0.76,0.67,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,9,0,15,1.22,0.75,0.66,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,9.5,0,0,1.1599999999999999,0.79,0.7,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,9.5,0,5,1.17,0.79,0.7,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,9.5,0,10,1.18,0.79,0.71,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,9.5,0,15,1.18,0.78,0.7,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,10,0,0,1.1200000000000001,0.81,0.75,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,10,0,5,1.1299999999999999,0.81,0.76,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,10,0,10,1.1399999999999999,0.81,0.76,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,10,0,15,1.1399999999999999,0.8,0.76,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,7.5,0,0,1.38,0.6,0.53,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,7.5,0,5,1.4,0.6,0.53,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,7.5,0,10,1.41,0.59,0.53,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,7.5,0,15,1.42,0.59,0.52,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,8,0,0,1.33,0.67,0.57999999999999996,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,8,0,5,1.35,0.66,0.57999999999999996,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,8,0,10,1.36,0.66,0.57999999999999996,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,8,0,15,1.36,0.64,0.57999999999999996,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,8.5,0,0,1.28,0.74,0.64,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,8.5,0,5,1.3,0.75,0.65,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,8.5,0,10,1.31,0.75,0.66,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,8.5,0,15,1.31,0.71,0.65,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,9,0,0,1.24,0.78,0.69,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,9,0,5,1.26,0.78,0.69,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,9,0,10,1.26,0.78,0.7,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,9,0,15,1.27,0.77,0.69,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,9.5,0,0,1.2,0.8,0.74,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,9.5,0,5,1.21,0.8,0.75,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,9.5,0,10,1.22,0.79,0.76,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,9.5,0,15,1.22,0.79,0.75,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,10,0,0,1.1599999999999999,0.82,0.78,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,10,0,5,1.17,0.82,0.78,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,10,0,10,1.18,0.81,0.79,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,10,0,15,1.18,0.81,0.79,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,7,0,0,1.48,0.59,0.51,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,7,0,5,1.51,0.57999999999999996,0.51,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,7,0,10,1.52,0.57999999999999996,0.5,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,7,0,15,1.53,0.56999999999999995,0.5,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,7.5,0,0,1.43,0.63,0.55000000000000004,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,7.5,0,5,1.45,0.63,0.56000000000000005,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,7.5,0,10,1.46,0.63,0.56000000000000005,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,7.5,0,15,1.46,0.61,0.55000000000000004,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,8,0,0,1.38,0.71,0.62,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,8,0,5,1.4,0.71,0.62,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,8,0,10,1.4,0.7,0.64,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,8,0,15,1.41,0.68,0.63,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,8.5,0,0,1.33,0.77,0.67,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,8.5,0,5,1.35,0.77,0.68,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,8.5,0,10,1.35,0.77,0.69,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,8.5,0,15,1.36,0.76,0.68,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,9,0,0,1.29,0.79,0.73,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,9,0,5,1.3,0.79,0.73,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,9,0,10,1.31,0.78,0.74,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,9,0,15,1.31,0.78,0.73,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,9.5,0,0,1.24,0.8,0.77,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,9.5,0,5,1.26,0.81,0.78,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,9.5,0,10,1.26,0.8,0.78,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,9.5,0,15,1.27,0.8,0.78,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,10,0,0,1.2,0.82,0.8,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,10,0,5,1.21,0.83,0.81,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,10,0,10,1.22,0.82,0.81,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,10,0,15,1.22,0.82,0.81,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,7,0,0,1.54,0.6,0.52,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,7,0,5,1.56,0.6,0.53,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,7,0,10,1.57,0.6,0.53,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,7,0,15,1.58,0.59,0.52,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,7.5,0,0,1.48,0.68,0.59,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,7.5,0,5,1.5,0.67,0.59,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,7.5,0,10,1.51,0.67,0.6,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,7.5,0,15,1.52,0.65,0.59,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,8,0,0,1.43,0.75,0.66,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,8,0,5,1.45,0.76,0.67,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,8,0,10,1.46,0.76,0.67,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,8,0,15,1.46,0.73,0.67,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,8.5,0,0,1.38,0.78,0.71,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,8.5,0,5,1.4,0.78,0.72,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,8.5,0,10,1.4,0.77,0.72,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,8.5,0,15,1.41,0.77,0.72,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,9,0,0,1.33,0.79,0.76,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,9,0,5,1.35,0.8,0.77,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,9,0,10,1.36,0.79,0.77,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,9,0,15,1.36,0.79,0.77,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,9.5,0,0,1.29,0.81,0.8,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,9.5,0,5,1.3,0.82,0.81,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,9.5,0,10,1.31,0.81,0.81,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,9.5,0,15,1.31,0.81,0.8,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,10,0,0,1.25,0.83,0.85,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,10,0,5,1.26,0.83,0.85,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,10,0,10,1.27,0.83,0.86,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,10,0,15,1.27,0.83,0.85,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,6.5,0,0,1.66,0.59,0.5,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,6.5,0,5,1.69,0.59,0.5,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,6.5,0,10,1.7,0.57999999999999996,0.5,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,7,0,0,1.59,0.64,0.55000000000000004,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,7,0,5,1.62,0.64,0.56000000000000005,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,7,0,10,1.63,0.63,0.56000000000000005,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,7,0,15,1.64,0.62,0.56000000000000005,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,7.5,0,0,1.54,0.73,0.62,1,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,7.5,0,5,1.56,0.72,0.64,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,7.5,0,10,1.57,0.72,0.64,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,7.5,0,15,1.58,0.69,0.64,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,8,0,0,1.49,0.77,0.69,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,8,0,5,1.5,0.77,0.7,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,8,0,10,1.51,0.77,0.7,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,8,0,15,1.52,0.76,0.7,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,8.5,0,0,1.43,0.78,0.75,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,8.5,0,5,1.45,0.78,0.77,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,8.5,0,10,1.46,0.78,0.77,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,8.5,0,15,1.46,0.78,0.76,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,9,0,0,1.38,0.8,0.79,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,9,0,5,1.4,0.81,0.8,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,9,0,10,1.41,0.8,0.8,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,9,0,15,1.41,0.8,0.79,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,9.5,0,0,1.34,0.82,0.83,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,9.5,0,5,1.35,0.82,0.84,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,9.5,0,10,1.36,0.82,0.85,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,9.5,0,15,1.36,0.82,0.84,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,10,0,0,1.29,0.84,0.86,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,10,0,5,1.31,0.84,0.87,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,10,0,10,1.31,0.84,0.88,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,10,0,15,1.32,0.83,0.87,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,6.5,0,0,1.72,0.61,0.52,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,6.5,0,5,1.75,0.61,0.53,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,6.5,0,10,1.77,0.61,0.53,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,6.5,0,15,1.78,0.6,0.52,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,7,0,0,1.66,0.69,0.59,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,7,0,5,1.68,0.69,0.6,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,7,0,10,1.7,0.68,0.61,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,7,0,15,1.7,0.66,0.6,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,7.5,0,0,1.6,0.76,0.67,1,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,7.5,0,5,1.62,0.76,0.68,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,7.5,0,10,1.63,0.76,0.69,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,7.5,0,15,1.64,0.75,0.69,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,8,0,0,1.54,0.77,0.73,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,8,0,5,1.56,0.78,0.74,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,8,0,10,1.57,0.77,0.74,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,8,0,15,1.58,0.77,0.74,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,8.5,0,0,1.49,0.79,0.78,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,8.5,0,5,1.51,0.8,0.79,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,8.5,0,10,1.52,0.79,0.79,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,8.5,0,15,1.52,0.79,0.79,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,9,0,0,1.44,0.81,0.82,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,9,0,5,1.46,0.82,0.83,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,9,0,10,1.46,0.81,0.83,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,9,0,15,1.47,0.81,0.82,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,9.5,0,0,1.39,0.83,0.86,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,9.5,0,5,1.41,0.83,0.87,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,9.5,0,10,1.41,0.83,0.87,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,9.5,0,15,1.42,0.82,0.87,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,10,0,0,1.34,0.85,0.88,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,10,0,5,1.36,0.85,0.89,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,10,0,10,1.37,0.85,0.89,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,10,0,15,1.37,0.84,0.89,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,6.5,0,0,1.79,0.65,0.56000000000000005,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,6.5,0,5,1.82,0.65,0.56000000000000005,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,6.5,0,10,1.84,0.65,0.56999999999999995,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,6.5,0,15,1.85,0.63,0.56999999999999995,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,7,0,0,1.73,0.75,0.64,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,7,0,5,1.75,0.75,0.66,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,7,0,10,1.77,0.74,0.67,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,7,0,15,1.78,0.72,0.66,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,7.5,0,0,1.67,0.77,0.71,1,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,7.5,0,5,1.69,0.77,0.72,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,7.5,0,10,1.7,0.77,0.72,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,7.5,0,15,1.71,0.76,0.73,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,8,0,0,1.61,0.78,0.78,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,8,0,5,1.63,0.79,0.78,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,8,0,10,1.64,0.78,0.78,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,8,0,15,1.64,0.78,0.78,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,8.5,0,0,1.55,0.8,0.81,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,8.5,0,5,1.57,0.81,0.82,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,8.5,0,10,1.58,0.8,0.82,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,8.5,0,15,1.58,0.8,0.82,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,9,0,0,1.5,0.82,0.86,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,9,0,5,1.52,0.83,0.87,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,9,0,10,1.52,0.82,0.87,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,9,0,15,1.53,0.82,0.86,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,9.5,0,0,1.45,0.84,0.88,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,9.5,0,5,1.46,0.84,0.89,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,9.5,0,10,1.47,0.84,0.9,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,9.5,0,15,1.47,0.84,0.89,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,10,0,0,1.4,0.86,0.88,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,10,0,5,1.42,0.87,0.89,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,10,0,10,1.42,0.86,0.9,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,10,0,15,1.42,0.86,0.9,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,6,0,0,1.94,0.62,0.51,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,6,0,5,1.98,0.62,0.52,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,6,0,10,2,0.62,0.52,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,6,0,15,2.0099999999999998,0.61,0.52,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,6.5,0,0,1.87,0.71,0.6,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,6.5,0,5,1.9,0.71,0.61,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,6.5,0,10,1.92,0.7,0.62,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,6.5,0,15,1.93,0.69,0.63,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,7,0,0,1.8,0.76,0.7,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,7,0,5,1.83,0.76,0.71,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,7,0,10,1.85,0.76,0.71,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,7,0,15,1.85,0.76,0.71,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,7.5,0,0,1.74,0.78,0.76,1,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,7.5,0,5,1.76,0.78,0.77,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,7.5,0,10,1.78,0.78,0.78,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,7.5,0,15,1.78,0.77,0.78,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,8,0,0,1.68,0.8,0.81,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,8,0,5,1.7,0.8,0.81,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,8,0,10,1.71,0.8,0.81,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,8,0,15,1.72,0.79,0.81,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,8.5,0,0,1.62,0.82,0.85,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,8.5,0,5,1.64,0.82,0.86,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,8.5,0,10,1.65,0.82,0.86,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,8.5,0,15,1.65,0.81,0.86,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,9,0,0,1.56,0.83,0.88,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,9,0,5,1.58,0.84,0.88,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,9,0,10,1.59,0.83,0.89,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,9,0,15,1.59,0.83,0.89,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,9.5,0,0,1.51,0.86,0.88,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,9.5,0,5,1.53,0.86,0.9,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,9.5,0,10,1.54,0.86,0.91,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,9.5,0,15,1.54,0.86,0.91,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,10,0,0,1.46,0.87,0.89,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,10,0,5,1.48,0.88,0.91,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,10,0,10,1.48,0.88,0.91,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,10,0,15,1.49,0.87,0.92,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,6,0,0,2.0299999999999998,0.69,0.56000000000000005,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,6,0,5,2.0699999999999998,0.69,0.56000000000000005,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,6,0,10,2.09,0.69,0.56999999999999995,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,6,0,15,2.1,0.67,0.56999999999999995,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,6.5,0,0,1.96,0.75,0.67,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,6.5,0,5,1.99,0.75,0.68,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,6.5,0,10,2.0099999999999998,0.74,0.69,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,6.5,0,15,2.02,0.74,0.68,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,7,0,0,1.88,0.78,0.74,1,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,7,0,5,1.91,0.78,0.75,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,7,0,10,1.93,0.78,0.75,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,7,0,15,1.94,0.77,0.75,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,7.5,0,0,1.82,0.8,0.8,1,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,7.5,0,5,1.84,0.81,0.8,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,7.5,0,10,1.86,0.8,0.8,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,7.5,0,15,1.87,0.8,0.8,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,8,0,0,1.75,0.81,0.84,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,8,0,5,1.77,0.82,0.85,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,8,0,10,1.79,0.81,0.85,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,8,0,15,1.79,0.81,0.85,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,8.5,0,0,1.69,0.83,0.87,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,8.5,0,5,1.71,0.84,0.87,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,8.5,0,10,1.72,0.83,0.88,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,8.5,0,15,1.73,0.83,0.87,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,9,0,0,1.63,0.85,0.88,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,9,0,5,1.65,0.86,0.89,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,9,0,10,1.66,0.86,0.9,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,9,0,15,1.67,0.86,0.91,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,9.5,0,0,1.58,0.87,0.89,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,9.5,0,5,1.6,0.87,0.91,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,9.5,0,10,1.61,0.87,0.91,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,9.5,0,15,1.61,0.87,0.92,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,10,0,0,1.53,0.88,0.9,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,10,0,5,1.54,0.88,0.91,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,10,0,10,1.55,0.88,0.92,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,10,0,15,1.55,0.88,0.93,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,6,0,0,2.13,0.73,0.61,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,6,0,5,2.17,0.73,0.62,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,6,0,10,2.19,0.72,0.64,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,6,0,15,2.2000000000000002,0.72,0.64,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,6.5,0,0,2.0499999999999998,0.76,0.72,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,6.5,0,5,2.08,0.77,0.73,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,6.5,0,10,2.1,0.76,0.73,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,6.5,0,15,2.12,0.75,0.74,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,7,0,0,1.98,0.79,0.79,1,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,7,0,5,2.0099999999999998,0.8,0.8,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,7,0,10,2.02,0.79,0.8,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,7,0,15,2.0299999999999998,0.78,0.8,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,7.5,0,0,1.9,0.81,0.83,1,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,7.5,0,5,1.93,0.81,0.83,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,7.5,0,10,1.94,0.81,0.83,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,7.5,0,15,1.95,0.81,0.84,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,8,0,0,1.84,0.82,0.86,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,8,0,5,1.86,0.83,0.86,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,8,0,10,1.87,0.83,0.86,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,8,0,15,1.88,0.82,0.86,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,8.5,0,0,1.77,0.85,0.88,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,8.5,0,5,1.79,0.86,0.89,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,8.5,0,10,1.81,0.85,0.9,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,8.5,0,15,1.81,0.85,0.9,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,9,0,0,1.71,0.86,0.89,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,9,0,5,1.73,0.87,0.9,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,9,0,10,1.74,0.87,0.92,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,9,0,15,1.75,0.87,0.92,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,9.5,0,0,1.66,0.88,0.89,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,9.5,0,5,1.67,0.88,0.91,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,9.5,0,10,1.68,0.88,0.91,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,9.5,0,15,1.68,0.87,0.93,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,10,0,0,1.6,0.89,0.91,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,10,0,5,1.62,0.89,0.93,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,10,0,10,1.63,0.89,0.94,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,10,0,15,1.63,0.89,0.94,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,6,0,0,2.2400000000000002,0.75,0.69,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,6,0,5,2.2799999999999998,0.75,0.7,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,6,0,10,2.2999999999999998,0.74,0.71,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,6,0,15,2.3199999999999998,0.74,0.7,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,6.5,0,0,2.15,0.78,0.78,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,6.5,0,5,2.19,0.78,0.79,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,6.5,0,10,2.21,0.78,0.79,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,6.5,0,15,2.2200000000000002,0.77,0.78,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,7,0,0,2.0699999999999998,0.81,0.82,1,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,7,0,5,2.11,0.81,0.82,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,7,0,10,2.12,0.81,0.81,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,7,0,15,2.13,0.8,0.82,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,7.5,0,0,2,0.83,0.84,1,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,7.5,0,5,2.0299999999999998,0.84,0.85,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,7.5,0,10,2.04,0.83,0.84,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,7.5,0,15,2.0499999999999998,0.83,0.85,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,8,0,0,1.93,0.84,0.87,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,8,0,5,1.95,0.86,0.87,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,8,0,10,1.96,0.85,0.87,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,8,0,15,1.97,0.85,0.88,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,8.5,0,0,1.86,0.86,0.89,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,8.5,0,5,1.88,0.87,0.9,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,8.5,0,10,1.9,0.87,0.91,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,8.5,0,15,1.9,0.87,0.92,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,9,0,0,1.8,0.88,0.89,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,9,0,5,1.82,0.88,0.91,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,9,0,10,1.83,0.88,0.92,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,9,0,15,1.83,0.87,0.93,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,9.5,0,0,1.74,0.89,0.91,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,9.5,0,5,1.76,0.89,0.93,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,9.5,0,10,1.77,0.89,0.94,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,9.5,0,15,1.77,0.89,0.94,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,10,0,0,1.68,0.89,0.92,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,10,0,5,1.7,0.9,0.93,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,10,0,10,1.71,0.89,0.93,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,10,0,15,1.71,0.89,0.94,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,6,0,0,2.36,0.77,0.74,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,6,0,5,2.4,0.77,0.75,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,6,0,10,2.42,0.76,0.74,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,6,0,15,2.44,0.75,0.75,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,6.5,0,0,2.27,0.8,0.79,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,6.5,0,5,2.2999999999999998,0.8,0.8,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,6.5,0,10,2.3199999999999998,0.8,0.79,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,6.5,0,15,2.34,0.79,0.8,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,7,0,0,2.1800000000000002,0.83,0.83,1,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,7,0,5,2.2200000000000002,0.83,0.83,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,7,0,10,2.23,0.83,0.83,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,7,0,15,2.2400000000000002,0.82,0.83,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,7.5,0,0,2.1,0.84,0.86,1,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,7.5,0,5,2.13,0.85,0.86,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,7.5,0,10,2.15,0.85,0.86,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,7.5,0,15,2.16,0.84,0.87,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,8,0,0,2.0299999999999998,0.85,0.88,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,8,0,5,2.06,0.86,0.88,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,8,0,10,2.0699999999999998,0.87,0.89,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,8,0,15,2.08,0.87,0.9,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,8.5,0,0,1.96,0.87,0.9,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,8.5,0,5,1.98,0.88,0.91,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,8.5,0,10,2,0.88,0.92,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,8.5,0,15,2,0.87,0.93,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,9,0,0,1.89,0.88,0.91,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,9,0,5,1.91,0.89,0.93,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,9,0,10,1.93,0.89,0.94,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,9,0,15,1.93,0.89,0.94,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,9.5,0,0,1.83,0.89,0.91,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,9.5,0,5,1.85,0.9,0.92,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,9.5,0,10,1.86,0.9,0.93,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,9.5,0,15,1.86,0.9,0.94,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,10,0,0,1.77,0.9,0.92,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,10,0,5,1.79,0.91,0.93,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,10,0,10,1.8,0.9,0.93,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,10,0,15,1.8,0.89,0.94,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,6,0,0,2.4900000000000002,0.79,0.76,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,6,0,5,2.5299999999999998,0.79,0.76,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,6,0,10,2.56,0.79,0.77,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,6,0,15,2.57,0.78,0.77,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,6.5,0,0,2.39,0.82,0.81,1,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,6.5,0,5,2.4300000000000002,0.82,0.81,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,6.5,0,10,2.4500000000000002,0.82,0.81,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,6.5,0,15,2.4700000000000002,0.82,0.82,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,7,0,0,2.2999999999999998,0.84,0.84,1,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,7,0,5,2.34,0.85,0.85,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,7,0,10,2.36,0.84,0.84,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,7,0,15,2.37,0.84,0.85,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,7.5,0,0,2.2200000000000002,0.85,0.87,1,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,7.5,0,5,2.25,0.86,0.88,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,7.5,0,10,2.27,0.87,0.88,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,7.5,0,15,2.2799999999999998,0.87,0.89,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,8,0,0,2.14,0.87,0.89,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,9,0,5,2.02,0.9,0.92,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,10,0,0,1.87,0.9,0.93,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,7.5,0,5,2.38,0.87,0.9,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,9.5,0,5,2.0699999999999998,0.91,0.92,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,6,0,5,2.85,0.82,0.81,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,8.5,0,10,2.37,0.91,0.92,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,6,0,10,3.07,0.83,0.84,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,6.5,0,5,2.92,0.86,0.87,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,9,0,10,2.44,0.9,0.92,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,6,0,10,3.29,0.85,0.87,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,8,0,10,2.81,0.91,0.89,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,8.5,0,5,2.69,0.91,0.91,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,6.5,0,10,3.4,0.9,0.88,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,7.5,0,10,3.14,0.91,0.89,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,9.5,0,10,2.72,0.9,0.97,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,7,0,15,3.55,0.91,0.89,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,8,0,10,3.28,0.9,0.94,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,9.5,0,10,2.94,0.89,0.97,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,7,0,10,3.86,0.91,0.92,1,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,9,0,15,3.33,0.89,0.96,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,7,0,15,4.26,0.91,0.95,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,9,0,0,3.6,0.89,0.97,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,10,0,15,3.42,0.89,0.97,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,6,0,15,1.93,0.59,0.48,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,6,0,10,1.64,0.51,0.39,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,6.5,0,15,1.53,0.52,0.43,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,7,0,10,1.41,0.54,0.47,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,6,0,0,1.4,0.46,0.31,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,6.5,0,10,1.38,0.48,0.39,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,6,0,15,1.4,0.46,0.33,4,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,7.5,0,10,1.24,0.54,0.45,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,7.5,0,0,1.18,0.53,0.44,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,7,0,15,1.22,0.48,0.39,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,6,0,5,1.26,0.42,0.27,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,7.5,0,15,1.1399999999999999,0.5,0.42,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,8.5,0,0,1.03,0.56000000000000005,0.47,1,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,7.5,0,5,1.1000000000000001,0.5,0.4,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,6,0,15,1.22,0.4,0.26,4,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,7.5,0,5,1.07,0.48,0.38,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,6.5,0,0,1.1000000000000001,0.39,0.27,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,7,0,5,1.08,0.44,0.32,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,8.5,0,15,0.98,0.51,0.45,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,6.5,0,5,1.0900000000000001,0.39,0.26,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,9.5,0,0,0.87,0.56999999999999995,0.49,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,6,0,5,1.1100000000000001,0.32,0.2,4,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,7.5,0,15,1,0.45,0.37,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,6,0,15,1.1000000000000001,0.33,0.21,5,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,7,0,5,1,0.41,0.28999999999999998,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,9.5,0,0,0.83,0.55000000000000004,0.46,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,10,0,15,0.82,0.56000000000000005,0.48,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,7,0,15,0.99,0.41,0.28000000000000003,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,6,0,0,1.02,0.25,0.14000000000000001,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,6.5,0,0,0.98,0.3,0.19,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,9,0,0,0.82,0.5,0.41,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,6,0,5,1.01,0.26,0.15,4,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,7.5,0,0,0.89,0.38,0.28000000000000003,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,8.5,0,0,0.83,0.46,0.37,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,6.5,0,0,0.94,0.28000000000000003,0.16,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,8,0,5,0.85,0.43,0.31,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,9.5,0,0,0.76,0.5,0.43,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,7,0,10,0.9,0.35,0.23,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,8,0,0,0.82,0.4,0.28999999999999998,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,9.5,0,5,0.75,0.5,0.43,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,8,0,5,0.82,0.4,0.28999999999999998,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,9,0,10,0.77,0.48,0.39,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,7,0,5,0.86,0.32,0.2,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,8.5,0,15,0.78,0.45,0.33,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,10,0,5,0.7,0.52,0.44,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,6,0,10,0.92,0.23,0.12,5,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,8.5,0,5,0.75,0.42,0.3,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,10,0,15,0.69,0.52,0.43,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",32,9,0,10,0.85,0.47,0.5,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",30,8.5,0,10,0.93,0.46,0.51,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",30,9,0,15,0.9,0.51,0.56000000000000005,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",29,9,0,5,0.93,0.49,0.6,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",29,10,0,15,0.87,0.57999999999999996,0.69,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",27,8,0,15,1.08,0.49,0.55000000000000004,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",27,10,0,5,0.93,0.57999999999999996,0.74,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",26,9,0,0,1.03,0.53,0.67,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",26,10,0,5,0.96,0.57999999999999996,0.76,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",25,8,0,15,1.17,0.53,0.63,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",24,7,0,5,1.31,0.43,0.53,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",24,9,0,0,1.1100000000000001,0.56000000000000005,0.72,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",24,10,0,5,1.04,0.61,0.81,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",23,7.5,0,0,1.3,0.47,0.64,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",23,9,0,10,1.18,0.59,0.77,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",22,7,0,10,1.43,0.5,0.63,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",22,8,0,15,1.33,0.56999999999999995,0.74,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",21,7,0,0,1.47,0.47,0.65,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",21,7.5,0,0,1.42,0.51,0.72,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",21,9,0,15,1.29,0.61,0.83,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",20,7.5,0,10,1.51,0.56000000000000005,0.75,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",20,9,0,5,1.34,0.6,0.85,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",19,6,0,10,1.81,0.47,0.6,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",19,8,0,10,1.53,0.59,0.81,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",19,8.5,0,15,1.48,0.61,0.84,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",18,7,0,15,1.76,0.55000000000000004,0.77,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",18,8.5,0,0,1.54,0.59,0.86,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",18,10,0,15,1.4,0.66,0.89,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",17,7.5,0,5,1.77,0.56000000000000005,0.83,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",17,8.5,0,15,1.65,0.61,0.88,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",17,10,0,0,1.46,0.66,0.93,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",16,7.5,0,15,1.9,0.57999999999999996,0.85,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",16,9.5,0,5,1.62,0.64,0.92,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",15,6,0,15,2.2999999999999998,0.53,0.78,3,0.81]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",15,7.5,0,0,1.98,0.55000000000000004,0.87,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",15,9,0,15,1.8,0.64,0.9,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",14,6.5,0,5,2.33,0.52,0.83,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",14,9.5,0,0,1.84,0.64,0.94,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",13,6,0,10,2.64,0.52,0.84,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",13,8,0,0,2.2000000000000002,0.59,0.92,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",13,8.5,0,5,2.14,0.62,0.93,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",12,7,0,0,2.57,0.54,0.9,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",12,8,0,10,2.4300000000000002,0.6,0.91,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",12,10,0,0,2.0699999999999998,0.67,0.95,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",11,7,0,15,2.88,0.57999999999999996,0.91,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",11,8.5,0,0,2.5099999999999998,0.61,0.95,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",11,9.5,0,10,2.37,0.67,0.95,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",10,7,0,0,3.09,0.55000000000000004,0.93,1,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",10,9,0,15,2.7,0.66,0.95,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",20,6,0,0,1.67,0.39,0.54,3,0.81]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",25,6.5,0,0,1.29,0.34,0.41,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",26,6.5,0,5,1.25,0.35,0.39,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",26,6.5,0,15,1.27,0.4,0.39,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",28,6,0,5,1.21,0.25,0.24,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",28,7.5,0,0,1.06,0.36,0.41,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",29,7,0,0,1.07,0.28999999999999998,0.33,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",30,7,0,0,1.03,0.27,0.28999999999999998,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",30,8,0,0,0.96,0.36,0.4,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",31,6.5,0,10,1.06,0.28000000000000003,0.22,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",31,8,0,15,0.94,0.44,0.41,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",32,7.5,0,15,0.95,0.38,0.31,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",32,8,0,15,0.91,0.42,0.38,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",33,8,0,10,0.88,0.37,0.35,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",34,6,0,5,1,0.11,0.09,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",34,7,0,0,0.91,0.18,0.18,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",34,9.5,0,5,0.77,0.44,0.48,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",35,6.5,0,15,0.94,0.23,0.13,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",35,8,0,15,0.84,0.36,0.28999999999999998,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",35,9,0,10,0.77,0.41,0.41,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",36,6.5,0,15,0.92,0.21,0.11,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",36,8,0,15,0.81,0.35,0.26,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",37,6,0,10,0.93,0.1,0.06,5,0.82]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",37,8,0,0,0.78,0.22,0.21,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",37,8.5,0,5,0.76,0.32,0.3,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",38,6.5,0,0,0.85,0.05,0.05,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",38,7.5,0,10,0.8,0.23,0.17,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",38,9.5,0,0,0.68,0.34,0.34,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",39,7,0,15,0.81,0.19,0.11,4,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",39,8.5,0,0,0.71,0.23,0.22,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",39,9.5,0,10,0.67,0.39,0.36,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",40,7,0,0,0.77,7.0000000000000007E-2,7.0000000000000007E-2,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",40,9,0,15,0.68,0.36,0.27,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",41,7,0,5,0.76,0.09,7.0000000000000007E-2,4,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",41,8.5,0,0,0.68,0.19,0.17,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",41,10,0,5,0.61,0.37,0.35,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",42,6,0,15,0.82,0.06,0.02,5,0.81]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",42,9,0,5,0.64,0.27,0.23,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",43,6,0,0,0.78,0.02,0.01,5,0.81]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",43,7.5,0,5,0.7,0.1,0.08,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",43,10,0,5,0.59,0.33,0.3,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",44,6,0,5,0.77,0.02,0.01,5,0.82]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",44,7.5,0,0,0.68,0.06,0.05,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",44,9,0,5,0.61,0.23,0.19,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",45,7,0,5,0.7,0.05,0.04,4,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",45,9,0,10,0.6,0.24,0.18,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",46,6.5,0,10,0.72,0.04,0.02,5,0.82]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",46,8,0,10,0.63,0.13,0.08,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",46,9,0,5,0.59,0.19,0.15,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",47,6.5,0,10,0.7,0.04,0.02,5,0.82]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",47,8,0,10,0.62,0.12,7.0000000000000007E-2,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",47,9.5,0,10,0.56000000000000005,0.26,0.19,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",48,7.5,0,15,0.64,0.1,0.04,4,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",48,8,0,10,0.61,0.11,0.06,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",48,10,0,10,0.53,0.28000000000000003,0.21,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",49,7,0,10,0.65,0.04,0.02,4,0.83]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",49,9.5,0,15,0.53,0.24,0.15,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",49,10,0,10,0.52,0.26,0.2,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",50,9,0,0,0.54,0.09,7.0000000000000007E-2,3,0.85]
[7,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",50,10,0,15,0.51,0.27,0.18,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",40,10,0,15,1.42,0.59,0.52,3,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",38,10,0,5,1.49,0.65,0.55000000000000004,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",36,9,0,10,1.69,0.6,0.51,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",35,8.5,0,10,1.8,0.57999999999999996,0.5,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",35,9.5,0,10,1.68,0.67,0.57999999999999996,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",34,9.5,0,10,1.73,0.69,0.61,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",33,9.5,0,15,1.78,0.72,0.64,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",32,8,0,10,2.04,0.59,0.51,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",31,8.5,0,0,1.99,0.69,0.59,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",31,10,0,15,1.83,0.79,0.75,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",30,7.5,0,15,2.27,0.57999999999999996,0.52,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",30,9.5,0,10,1.95,0.79,0.74,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",29,7.5,0,15,2.35,0.61,0.56000000000000005,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",29,10,0,15,1.96,0.81,0.82,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",28,7,0,15,2.5299999999999998,0.57999999999999996,0.52,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",28,9,0,10,2.17,0.78,0.77,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",27,7,0,15,2.62,0.61,0.55000000000000004,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",27,9.5,0,15,2.17,0.8,0.84,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",26,8,0,0,2.46,0.78,0.73,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",26,8,0,10,2.5099999999999998,0.77,0.74,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",25,7,0,0,2.75,0.74,0.63,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",25,7.5,0,15,2.72,0.76,0.72,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",25,10,0,0,2.23,0.84,0.89,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",24,7.5,0,0,2.76,0.78,0.75,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",24,9,0,0,2.4900000000000002,0.82,0.87,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",24,9.5,0,15,2.4500000000000002,0.84,0.9,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",23,7.5,0,0,2.88,0.79,0.8,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",23,9.5,0,0,2.5099999999999998,0.85,0.9,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",22,6,0,0,3.37,0.72,0.59,3,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",22,8.5,0,5,2.84,0.83,0.87,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",21,6,0,5,3.59,0.74,0.67,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",21,6.5,0,0,3.4,0.77,0.76,2,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",21,9.5,0,5,2.78,0.89,0.92,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",20,6,0,5,3.77,0.76,0.73,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",20,8,0,5,3.24,0.85,0.87,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",20,10,0,10,2.83,0.9,0.93,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",19,6.5,0,5,3.82,0.8,0.8,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",19,7.5,0,5,3.54,0.85,0.86,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",19,9.5,0,5,3.07,0.9,0.92,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",18,7,0,10,3.91,0.84,0.85,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",18,9.5,0,10,3.25,0.9,0.92,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",17,6.5,0,15,4.33,0.83,0.84,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",17,7,0,5,4.0999999999999996,0.85,0.86,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",17,9,0,10,3.57,0.91,0.91,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",16,7,0,10,4.4000000000000004,0.88,0.91,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",16,8,0,15,4.09,0.91,0.91,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",16,10,0,10,3.54,0.89,0.93,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",15,8,0,0,4.26,0.91,0.9,1,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",15,8.5,0,10,4.1900000000000004,0.91,0.9,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",15,10,0,15,3.78,0.9,0.94,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",14,7.5,0,10,4.84,0.91,0.89,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",14,10,0,0,3.98,0.9,0.96,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",13,6,0,10,5.87,0.88,0.87,"/",0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",13,9,0,5,4.6399999999999997,0.9,0.95,1,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",12,6,0,15,6.4,0.88,0.88,"/",0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",12,7,0,0,5.73,0.9,0.89,"/",0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",12,9,0,15,5.07,0.9,0.97,"/",0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",11,6.5,0,5,6.59,0.89,0.9,"/",0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",11,8.5,0,0,5.61,0.9,0.98,"/",0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",11,8.5,0,15,5.73,0.9,0.96,"/",0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",10,6,0,15,7.67,0.89,0.9,"/",0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",10,9,0,0,5.96,0.9,0.97,"/",0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",25,6,0,0,2.96,0.56999999999999995,0.47,3,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",28,6,0,0,2.64,0.52,0.41,3,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",28,6,0,15,2.73,0.5,0.4,5,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",30,7,0,0,2.29,0.55000000000000004,0.48,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",31,6.5,0,0,2.2999999999999998,0.51,0.4,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",32,6.5,0,0,2.23,0.5,0.38,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",33,6.5,0,5,2.2000000000000002,0.49,0.37,4,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",33,7.5,0,0,2.0099999999999998,0.53,0.46,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",34,6.5,0,0,2.1,0.48,0.34,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",35,6,0,0,2.11,0.42,0.28000000000000003,4,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",35,8,0,5,1.85,0.55000000000000004,0.47,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",36,6,0,15,2.13,0.42,0.3,6,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",37,6.5,0,5,1.96,0.45,0.32,4,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",37,8,0,0,1.73,0.52,0.45,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",37,8.5,0,0,1.67,0.56000000000000005,0.48,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",38,8,0,0,1.68,0.52,0.43,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",39,6,0,15,1.97,0.39,0.26,6,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",39,8,0,10,1.67,0.5,0.43,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",40,7,0,0,1.72,0.43,0.32,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",40,7.5,0,10,1.7,0.46,0.38,4,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",40,9,0,15,1.52,0.52,0.46,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",41,6.5,0,10,1.79,0.4,0.27,5,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",41,9,0,0,1.46,0.53,0.45,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",42,7,0,15,1.69,0.42,0.31,5,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",42,9,0,5,1.44,0.53,0.45,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",42,9,0,10,1.45,0.52,0.45,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",43,7,0,0,1.6,0.38,0.26,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",43,9,0,15,1.42,0.51,0.45,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",44,6.5,0,5,1.65,0.34,0.22,5,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",44,7.5,0,15,1.55,0.43,0.32,5,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",44,10,0,10,1.29,0.54,0.46,3,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",45,6,0,15,1.71,0.3,0.18,7,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",45,8,0,5,1.44,0.44,0.35,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",45,9,0,15,1.36,0.49,0.43,4,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",46,7.5,0,10,1.47,0.41,0.28999999999999998,4,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",46,8,0,15,1.43,0.44,0.34,4,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",46,10,0,5,1.23,0.53,0.46,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",47,8.5,0,0,1.32,0.44,0.34,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",47,9,0,10,1.3,0.48,0.41,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",48,7,0,0,1.43,0.31,0.2,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",48,8.5,0,15,1.32,0.45,0.35,4,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",48,10,0,0,1.17,0.51,0.44,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",49,6.5,0,10,1.5,0.3,0.18,6,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",49,8.5,0,5,1.28,0.43,0.33,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",50,6.5,0,5,1.45,0.27,0.16,5,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",50,8,0,10,1.31,0.4,0.28999999999999998,4,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",50,9.5,0,5,1.17,0.47,0.39,3,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",36,10,0,15,0.87,0.48,0.52,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",32,9,0,5,1.05,0.45,0.51,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",31,9,0,0,1.07,0.44,0.51,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",31,10,0,15,1.01,0.56000000000000005,0.65,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",29,8.5,0,0,1.19,0.43,0.52,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",29,9,0,10,1.1599999999999999,0.51,0.62,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",28,8,0,15,1.3,0.48,0.54,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",27,8.5,0,0,1.28,0.48,0.6,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",27,9.5,0,5,1.2,0.56000000000000005,0.71,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",27,10,0,15,1.1599999999999999,0.6,0.74,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",26,9,0,0,1.28,0.53,0.69,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",25,8.5,0,5,1.39,0.53,0.69,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",25,9,0,10,1.35,0.56999999999999995,0.73,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",24,8,0,5,1.5,0.51,0.68,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",24,9.5,0,15,1.35,0.6,0.77,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",23,7,0,10,1.71,0.48,0.62,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",23,8,0,15,1.58,0.55000000000000004,0.72,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",22,6.5,0,0,1.82,0.4,0.56000000000000005,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",22,8,0,10,1.65,0.56000000000000005,0.75,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",22,9.5,0,0,1.46,0.59,0.83,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",21,8,0,0,1.7,0.54,0.75,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",21,9.5,0,10,1.54,0.63,0.84,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",21,9.5,0,15,1.54,0.63,0.83,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",20,8,0,10,1.81,0.56999999999999995,0.78,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",20,9.5,0,0,1.6,0.61,0.85,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",19,7,0,10,2.06,0.54,0.75,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",19,9,0,5,1.76,0.61,0.85,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",19,10,0,10,1.65,0.65,0.88,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",18,7,0,0,2.14,0.51,0.78,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",18,8.5,0,10,1.94,0.61,0.84,2,0.85]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",17,6,0,5,2.4900000000000002,0.49,0.71,3,0.81]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",17,7,0,10,2.31,0.56000000000000005,0.79,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",17,10,0,10,1.84,0.66,0.91,1,0.87]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",16,6,0,10,2.67,0.51,0.75,3,0.81]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",16,8,0,5,2.25,0.59,0.86,2,0.84]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",15,6,0,15,2.86,0.53,0.77,3,0.81]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",15,7.5,0,10,2.5099999999999998,0.56999999999999995,0.85,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",15,9,0,15,2.2400000000000002,0.64,0.9,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",14,6.5,0,15,2.93,0.54,0.81,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",14,7.5,0,15,2.7,0.59,0.86,2,0.83]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",14,9,0,10,2.4,0.63,0.92,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",13,6,0,15,3.3,0.52,0.81,3,0.81]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",13,8.5,0,15,2.68,0.62,0.92,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",13,9.5,0,15,2.4900000000000002,0.65,0.94,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",12,6.5,0,10,3.4,0.54,0.85,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",12,8.5,0,5,2.89,0.61,0.94,1,0.85]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",11,6.5,0,0,3.64,0.51,0.9,2,0.82]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",11,8,0,10,3.29,0.6,0.93,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",11,9.5,0,0,2.91,0.65,0.95,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",10,6,0,5,4.22,0.49,0.9,2,0.81]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",10,8,0,0,3.57,0.57999999999999996,0.95,1,0.84]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",10,9.5,0,10,3.24,0.67,0.94,1,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",25,6,0,5,1.69,0.33,0.37,4,0.81]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",26,6,0,10,1.64,0.34,0.34,5,0.81]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",27,6.5,0,0,1.48,0.3,0.34,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",27,7,0,5,1.44,0.39,0.44,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",29,6,0,15,1.48,0.31,0.24,5,0.81]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",29,7.5,0,5,1.29,0.39,0.43,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",30,7,0,5,1.3,0.32,0.34,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",31,6,0,15,1.38,0.27,0.18,5,0.81]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",31,7.5,0,0,1.2,0.31,0.34,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",32,6,0,0,1.3,0.11,0.12,4,0.81]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",32,7.5,0,10,1.18,0.37,0.34,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",33,7,0,0,1.17,0.21,0.21,3,0.82]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",33,8,0,5,1.0900000000000001,0.36,0.36,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",34,7.5,0,5,1.1000000000000001,0.3,0.28000000000000003,3,0.83]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",34,9,0,10,0.99,0.43,0.47,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",34,9.5,0,0,0.95,0.42,0.47,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",35,8.5,0,5,0.99,0.36,0.36,3,0.85]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",36,6,0,0,1.1599999999999999,0.06,0.06,5,0.81]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",36,7.5,0,5,1.04,0.26,0.23,4,0.83]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",36,10,0,5,0.87,0.44,0.49,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",37,6.5,0,15,1.1100000000000001,0.19,0.11,5,0.82]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",37,8,0,10,0.98,0.32,0.27,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",37,9.5,0,15,0.88,0.45,0.43,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",38,7.5,0,15,1,0.27,0.19,4,0.83]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",38,8,0,15,0.96,0.32,0.24,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",39,7,0,0,0.99,0.09,0.08,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",39,8.5,0,0,0.88,0.25,0.23,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",39,9,0,15,0.87,0.38,0.32,3,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",40,7.5,0,0,0.93,0.12,0.12,4,0.83]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",40,9,0,0,0.83,0.28000000000000003,0.25,3,0.85]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",41,6,0,0,1.02,0.02,0.02,5,0.81]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",41,6.5,0,15,1,0.11,0.05,5,0.82]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",41,9,0,0,0.81,0.26,0.23,3,0.85]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",42,6,0,0,0.99,0.02,0.02,5,0.81]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",42,7.5,0,0,0.88,0.09,0.08,4,0.83]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",42,10,0,5,0.75,0.36,0.33,2,0.87]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",43,6,0,0,0.97,0.02,0.02,6,0.81]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",43,8,0,0,0.83,0.12,0.1,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",43,9.5,0,0,0.75,0.27,0.24,2,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",44,7.5,0,5,0.85,0.1,0.08,4,0.83]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",44,9.5,0,0,0.73,0.25,0.22,3,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",45,6,0,5,0.94,0.02,0.01,6,0.81]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",45,7,0,15,0.88,0.1,0.04,5,0.82]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",45,9,0,5,0.75,0.22,0.19,3,0.85]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",46,7,0,0,0.84,0.03,0.02,4,0.82]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",46,9,0,10,0.73,0.24,0.18,3,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",47,6,0,5,0.9,0.02,0.01,7,0.81]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",47,7.5,0,10,0.8,0.09,0.05,4,0.83]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",47,8.5,0,0,0.73,0.11,0.09,3,0.84]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",48,6.5,0,10,0.85,0.03,0.02,6,0.82]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",48,8,0,5,0.75,0.09,7.0000000000000007E-2,4,0.84]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",48,9.5,0,10,0.68,0.25,0.19,3,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",49,6,0,0,0.85,0.01,0.01,6,0.81]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",49,8,0,10,0.74,0.1,0.06,4,0.84]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",49,9.5,0,5,0.66,0.2,0.16,3,0.86]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",50,6.5,0,10,0.82,0.03,0.01,6,0.82]
[7,"UNILATERAL","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",50,9,0,10,0.68,0.17,0.12,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",40,10,0,15,1.76,0.59,0.52,3,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",39,9.5,0,5,1.86,0.59,0.51,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",37,10,0,10,1.9,0.66,0.56999999999999995,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",36,9.5,0,5,2.0099999999999998,0.64,0.55000000000000004,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",35,9.5,0,15,2.08,0.65,0.57999999999999996,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",34,9,0,15,2.2200000000000002,0.63,0.56000000000000005,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",33,8.5,0,15,2.37,0.61,0.53,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",33,9.5,0,10,2.2000000000000002,0.73,0.64,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",32,9,0,15,2.36,0.69,0.62,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",31,8.5,0,10,2.52,0.67,0.59,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",31,10,0,10,2.27,0.81,0.75,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",30,9.5,0,15,2.4300000000000002,0.8,0.74,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",30,10,0,10,2.34,0.82,0.78,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",29,8,0,15,2.8,0.68,0.62,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",28,8,0,0,2.83,0.75,0.66,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",28,9,0,0,2.65,0.8,0.77,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",27,7.5,0,0,3.04,0.72,0.63,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",27,9.5,0,5,2.68,0.83,0.84,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",26,7,0,0,3.28,0.68,0.59,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",26,8,0,0,3.06,0.79,0.73,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",26,10,0,0,2.66,0.85,0.9,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",25,8,0,5,3.22,0.79,0.78,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",25,9,0,0,2.96,0.83,0.87,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",24,7,0,10,3.63,0.77,0.7,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",24,7.5,0,0,3.43,0.79,0.75,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",24,9.5,0,5,3.01,0.85,0.91,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",23,6.5,0,0,3.85,0.76,0.65,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",23,9,0,10,3.27,0.85,0.92,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",22,6.5,0,5,4.09,0.78,0.72,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",22,7,0,5,3.93,0.8,0.79,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",22,9,0,0,3.36,0.86,0.9,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",21,6,0,5,4.45,0.76,0.67,3,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",21,8.5,0,5,3.69,0.86,0.91,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",20,6,0,10,4.7300000000000004,0.78,0.74,4,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",20,6.5,0,0,4.43,0.81,0.79,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",20,9,0,10,3.76,0.9,0.94,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",20,10,0,5,3.5,0.9,0.93,1,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",19,7.5,0,10,4.42,0.86,0.89,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",19,9.5,0,10,3.82,0.9,0.92,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",18,6.5,0,10,5.05,0.83,0.84,"/",0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",18,7.5,0,5,4.63,0.86,0.89,2,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",18,9.5,0,10,4.04,0.9,0.91,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",17,7,0,10,5.13,0.87,0.89,"/",0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",17,8,0,10,4.76,0.9,0.91,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",16,6,0,15,5.95,0.84,0.85,"/",0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",16,8,0,15,5.07,0.91,0.9,"/",0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",16,8.5,0,10,4.87,0.91,0.9,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",15,7,0,15,5.84,0.9,0.9,"/",0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",15,8,0,15,5.41,0.91,0.89,"/",0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",15,10,0,15,4.6900000000000004,0.9,0.94,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",14,8,0,0,5.67,0.91,0.89,"/",0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",14,8.5,0,15,5.58,0.9,0.92,"/",0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",14,9.5,0,15,5.19,0.9,0.95,"/",0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",13,7,0,15,6.74,0.9,0.88,"/",0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",13,9.5,0,0,5.5,0.9,0.97,"/",0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",13,10,0,15,5.4,0.89,0.96,"/",0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",12,9,0,5,6.24,0.9,0.98,"/",0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",12,9,0,15,6.28,0.9,0.97,"/",0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",11,7,0,0,7.75,0.91,0.92,"/",0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",11,9.5,0,0,6.51,0.9,0.96,"/",0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",10,6,0,5,9.35,0.89,0.9,"/",0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",10,8,0,0,7.94,0.91,0.97,"/",0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Adecuado/a",10,10,0,10,7.02,0.89,0.97,"/",0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",26,6,0,0,3.53,0.54,0.44,3,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",28,6,0,5,3.34,0.52,0.41,4,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",29,7,0,15,3.02,0.55000000000000004,0.49,4,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",31,6.5,0,5,2.9,0.51,0.4,4,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",31,7,0,15,2.83,0.53,0.45,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",33,6,0,15,2.89,0.45,0.33,6,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",33,6.5,0,0,2.69,0.48,0.37,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",34,6,0,10,2.78,0.44,0.32,6,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",35,6,0,5,2.67,0.44,0.3,5,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",35,7.5,0,15,2.41,0.49,0.44,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",36,7,0,0,2.37,0.48,0.36,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",36,7.5,0,5,2.3199999999999998,0.5,0.43,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",37,7,0,0,2.31,0.47,0.35,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",37,8.5,0,10,2.11,0.54,0.48,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",38,7,0,0,2.25,0.46,0.34,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",39,6,0,0,2.36,0.36,0.24,4,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",39,6.5,0,5,2.31,0.43,0.28999999999999998,5,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",39,9,0,10,1.93,0.55000000000000004,0.48,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",40,6.5,0,10,2.27,0.41,0.28000000000000003,5,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",40,8.5,0,10,1.95,0.51,0.44,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",41,6.5,0,15,2.23,0.41,0.27,6,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",41,7.5,0,10,2.0499999999999998,0.46,0.37,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",41,9,0,10,1.84,0.53,0.45,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",42,7,0,10,2.08,0.43,0.31,5,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",42,9,0,15,1.8,0.52,0.45,4,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",42,10,0,10,1.68,0.56999999999999995,0.49,3,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",43,7,0,10,2.0299999999999998,0.41,0.28999999999999998,5,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",43,10,0,15,1.64,0.55000000000000004,0.47,3,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",44,6,0,15,2.16,0.32,0.19,7,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",44,8.5,0,15,1.78,0.47,0.41,4,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",45,6,0,0,2.0499999999999998,0.26,0.15,5,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",45,7.5,0,15,1.88,0.42,0.31,5,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",45,8,0,15,1.81,0.45,0.36,5,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",46,6,0,15,2.0699999999999998,0.31,0.18,8,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",46,8,0,0,1.73,0.42,0.32,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",46,9,0,15,1.64,0.48,0.42,4,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",47,7,0,5,1.84,0.36,0.23,4,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",47,7.5,0,15,1.8,0.41,0.28000000000000003,5,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",47,9.5,0,0,1.53,0.49,0.43,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",48,6.5,0,15,1.9,0.33,0.19,6,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",48,9,0,5,1.57,0.47,0.39,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",49,7,0,0,1.74,0.32,0.2,4,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",49,8.5,0,10,1.6,0.44,0.34,4,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",49,10,0,0,1.42,0.51,0.44,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",50,6,0,5,1.87,0.24,0.12,7,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",50,8.5,0,0,1.53,0.41,0.31,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","Definido por el usuario","Insuficiente",50,10,0,10,1.41,0.51,0.44,3,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",19,7.5,0,5,0.82,0.47,0.57999999999999996,1,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",18,8.5,0,5,0.8,0.65,0.85,1,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",18,9,0,10,0.77,0.67,0.89,1,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",17,8,0,5,0.88,0.64,0.84,1,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",17,9,0,15,0.81,0.67,0.86,1,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",16,7.5,0,0,0.98,0.57999999999999996,0.78,1,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",16,9.5,0,10,0.83,0.68,0.85,1,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",15,7,0,5,1.0900000000000001,0.59,0.82,1,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",15,8,0,10,1,0.63,0.86,1,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",15,9.5,0,0,0.89,0.69,0.84,1,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",14,7,0,10,1.1599999999999999,0.6,0.88,1,0.82]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",14,9,0,5,0.99,0.67,0.83,1,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",14,10,0,10,0.91,0.71,0.85,1,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",13,7,0,0,1.26,0.61,0.85,1,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",13,8.5,0,10,1.1000000000000001,0.65,0.83,1,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",12,6,0,5,1.5,0.56000000000000005,0.86,2,0.81]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",12,8.5,0,0,1.2,0.65,0.83,1,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",12,9.5,0,15,1.1000000000000001,0.7,0.88,1,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",11,7.5,0,5,1.42,0.6,0.83,1,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",11,8,0,15,1.35,0.65,0.85,1,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",11,10,0,0,1.17,0.73,0.98,1,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",10,6.5,0,15,1.7,0.56999999999999995,0.82,1,0.81]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",10,9.5,0,5,1.33,0.71,0.94,1,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",10,10,0,15,1.27,0.73,0.92,1,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",18,6.5,0,5,0.95,0.39,0.45,2,0.82]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",19,9,0,10,0.73,0.68,0.87,1,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",19,9.5,0,15,0.69,0.68,0.89,1,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",20,8,0,15,0.74,0.56999999999999995,0.63,1,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",20,10,0,5,0.64,0.7,0.88,1,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",21,6.5,0,15,0.81,0.34,0.34,2,0.81]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",21,8,0,0,0.72,0.4,0.44,1,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",21,10,0,15,0.6,0.7,0.88,1,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",22,7.5,0,5,0.71,0.33,0.34,2,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",22,8.5,0,15,0.65,0.55000000000000004,0.56999999999999995,1,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",23,7,0,10,0.71,0.28000000000000003,0.27,2,0.82]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",23,7,0,15,0.71,0.32,0.31,2,0.82]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",23,9,0,5,0.6,0.49,0.55000000000000004,1,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",24,7.5,0,0,0.66,0.22,0.22,2,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",24,8.5,0,10,0.6,0.43,0.45,1,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",25,6.5,0,0,0.69,0.14000000000000001,0.14000000000000001,2,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",25,8,0,15,0.6,0.36,0.36,2,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",25,9.5,0,0,0.54,0.42,0.44,1,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,6,0,10,0.69,0.15,0.15,3,0.81]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,8,0,0,0.57999999999999996,0.21,0.22,2,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,9.5,0,15,0.51,0.51,0.5,1,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",27,6.5,0,0,0.64,0.13,0.12,2,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",27,9.5,0,0,0.5,0.32,0.34,1,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",27,10,0,0,0.48,0.39,0.4,1,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,7,0,15,0.57999999999999996,0.2,0.18,2,0.82]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,8.5,0,0,0.52,0.21,0.22,2,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",29,7,0,0,0.56999999999999995,0.14000000000000001,0.12,2,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",29,8.5,0,5,0.5,0.22,0.22,2,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",30,6,0,5,0.6,0.1,0.08,3,0.81]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",30,7,0,5,0.55000000000000004,0.15,0.13,2,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",30,8.5,0,0,0.48,0.19,0.18,2,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",30,10,0,5,0.43,0.32,0.33,1,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",31,8,0,5,0.48,0.18,0.16,2,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",31,9,0,5,0.45,0.22,0.23,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",32,6,0,0,0.56000000000000005,0.08,0.06,3,0.82]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",32,7.5,0,5,0.49,0.16,0.13,2,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",32,9.5,0,5,0.42,0.24,0.25,1,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",33,7.5,0,10,0.47,0.17,0.14000000000000001,2,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",33,9,0,10,0.42,0.22,0.22,2,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",33,9.5,0,15,0.4,0.27,0.27,1,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",34,7,0,10,0.48,0.13,0.09,3,0.82]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",34,9,0,0,0.41,0.18,0.16,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",34,10,0,10,0.38,0.27,0.26,1,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",35,8.5,0,5,0.41,0.18,0.15,2,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",35,10,0,15,0.36,0.28000000000000003,0.26,1,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",36,6.5,0,0,0.48,7.0000000000000007E-2,0.05,3,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",36,9,0,15,0.38,0.21,0.19,2,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,6,0,5,0.49,7.0000000000000007E-2,0.04,4,0.81]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,7.5,0,15,0.42,0.15,0.1,2,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,9.5,0,10,0.36,0.22,0.19,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,6,0,15,0.47,0.08,0.04,4,0.81]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,7.5,0,5,0.41,0.11,7.0000000000000007E-2,2,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,9,0,15,0.36,0.2,0.16,2,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,7,0,10,0.42,0.09,0.06,3,0.82]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,8,0,15,0.38,0.15,0.1,2,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,9.5,0,5,0.34,0.18,0.15,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,6.5,0,15,0.42,0.08,0.05,3,0.81]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,8.5,0,10,0.36,0.14000000000000001,0.1,2,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,7,0,0,0.4,7.0000000000000007E-2,0.04,3,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,8,0,15,0.36,0.12,0.09,2,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,10,0,0,0.31,0.17,0.14000000000000001,2,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,6,0,10,0.43,0.06,0.03,4,0.81]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,9,0,0,0.33,0.12,0.09,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,10,0,15,0.3,0.21,0.17,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,7.5,0,0,0.37,7.0000000000000007E-2,0.04,3,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,10,0,0,0.3,0.16,0.11,2,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,6,0,0,0.41,0.04,0.02,4,0.82]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,7,0,15,0.37,0.08,0.04,3,0.82]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,6,0,5,0.4,0.04,0.02,4,0.81]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,7,0,0,0.37,0.05,0.03,3,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,8,0,0,0.34,7.0000000000000007E-2,0.05,2,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,6.5,0,5,0.37,0.05,0.02,4,0.82]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,8,0,5,0.33,0.08,0.05,2,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,9,0,0,0.3,0.1,0.06,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,6.5,0,5,0.36,0.04,0.02,4,0.82]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,8,0,5,0.32,0.08,0.05,3,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,9.5,0,5,0.28000000000000003,0.12,0.08,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,7.5,0,10,0.33,7.0000000000000007E-2,0.04,3,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,8.5,0,5,0.3,0.09,0.05,2,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,10,0,5,0.27,0.13,0.09,2,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,7,0,5,0.33,0.05,0.02,3,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,9.5,0,10,0.27,0.12,0.08,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,7,0,10,0.33,0.05,0.03,3,0.82]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,8.5,0,15,0.28999999999999998,0.09,0.06,2,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,10,0,10,0.26,0.13,0.09,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",23,9.5,0,10,1.37,0.69,0.51,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",22,10,0,10,1.38,0.75,0.59,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",20,8.5,0,10,1.69,0.73,0.54,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",19,8,0,5,1.85,0.72,0.51,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",19,9.5,0,10,1.65,0.83,0.7,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",18,7.5,0,0,2.0299999999999998,0.71,0.5,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",18,10,0,10,1.69,0.81,0.71,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",17,8,0,10,2.0699999999999998,0.8,0.64,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",17,9.5,0,15,1.84,0.8,0.71,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",16,6.5,0,10,2.48,0.71,0.5,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",16,9,0,0,2.0299999999999998,0.83,0.73,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",16,10,0,15,1.89,0.79,0.71,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",15,7.5,0,15,2.4300000000000002,0.82,0.71,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",15,10,0,15,2.0099999999999998,0.78,0.72,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",14,8,0,0,2.5099999999999998,0.83,0.75,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",14,8,0,10,2.5099999999999998,0.81,0.73,2,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",14,9.5,0,15,2.2400000000000002,0.78,0.72,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",13,7.5,0,15,2.8,0.8,0.72,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",13,10,0,0,2.33,0.8,0.77,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",12,7,0,0,3.17,0.82,0.77,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",12,8.5,0,0,2.81,0.8,0.74,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",12,9,0,15,2.7,0.8,0.77,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",11,7,0,0,3.46,0.8,0.74,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",11,9,0,0,2.96,0.83,0.81,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",10,6,0,0,4.1500000000000004,0.81,0.77,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",10,8.5,0,5,3.38,0.85,0.85,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",10,9,0,0,3.25,0.86,0.87,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",15,6,0,0,2.77,0.67,0.47,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",18,7,0,0,2.11,0.66,0.44,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",19,6.5,0,0,2.09,0.6,0.38,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",20,6.5,0,0,1.99,0.57999999999999996,0.35,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",21,6,0,5,1.98,0.54,0.28999999999999998,3,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",21,7.5,0,0,1.74,0.62,0.4,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",21,8.5,0,0,1.61,0.68,0.49,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",22,7.5,0,5,1.66,0.6,0.38,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",23,6.5,0,10,1.73,0.52,0.3,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",23,7.5,0,5,1.59,0.57999999999999996,0.35,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",24,6.5,0,15,1.65,0.49,0.28000000000000003,3,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",24,7,0,5,1.59,0.52,0.31,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",24,9,0,10,1.36,0.62,0.43,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",25,6.5,0,5,1.59,0.46,0.24,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",25,9,0,15,1.3,0.6,0.41,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,6.5,0,10,1.53,0.44,0.23,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,7,0,10,1.47,0.48,0.27,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,9.5,0,10,1.21,0.61,0.41,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",27,6,0,15,1.53,0.38,0.18,4,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",27,8,0,10,1.3,0.53,0.33,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,6,0,0,1.48,0.31,0.16,4,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,6.5,0,10,1.42,0.4,0.2,3,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,8,0,15,1.25,0.51,0.31,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,10,0,10,1.0900000000000001,0.61,0.41,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",29,7.5,0,15,1.26,0.46,0.25,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",29,9.5,0,15,1.08,0.56999999999999995,0.37,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",30,6.5,0,15,1.32,0.36,0.18,4,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",30,7.5,0,10,1.22,0.43,0.23,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",30,9.5,0,15,1.05,0.55000000000000004,0.36,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",31,7,0,15,1.23,0.37,0.19,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",31,8,0,15,1.1299999999999999,0.46,0.26,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",32,6.5,0,0,1.24,0.28000000000000003,0.14000000000000001,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",32,8.5,0,0,1.06,0.45,0.26,2,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",32,8.5,0,15,1.05,0.47,0.27,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",32,10,0,15,0.95,0.56000000000000005,0.34,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",33,8.5,0,0,1.02,0.43,0.24,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",34,6,0,0,1.22,0.25,0.12,4,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",34,6,0,15,1.22,0.27,0.13,4,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",34,9,0,0,0.96,0.46,0.25,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",34,10,0,0,0.89,0.52,0.3,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",35,7.5,0,0,1.05,0.32,0.17,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",35,9.5,0,5,0.9,0.48,0.27,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",36,6,0,0,1.1499999999999999,0.23,0.11,4,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",36,7.5,0,0,1.02,0.31,0.16,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",36,9.5,0,0,0.87,0.45,0.25,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,7,0,5,1.03,0.28999999999999998,0.14000000000000001,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,9.5,0,5,0.85,0.46,0.25,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,6,0,10,1.1000000000000001,0.23,0.11,4,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,8,0,5,0.93,0.34,0.19,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,8.5,0,5,0.89,0.38,0.21,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,6.5,0,5,1.02,0.24,0.12,4,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,8,0,10,0.9,0.34,0.18,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,10,0,5,0.78,0.46,0.25,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,7.5,0,15,0.91,0.28999999999999998,0.15,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,8.5,0,5,0.85,0.32,0.18,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,9.5,0,10,0.79,0.4,0.21,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,7,0,5,0.93,0.24,0.12,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,9,0,15,0.79,0.36,0.19,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,7,0,10,0.91,0.24,0.12,3,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,9,0,0,0.78,0.31,0.17,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,6,0,10,0.97,0.19,0.08,4,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,6.5,0,15,0.92,0.22,0.1,4,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,9,0,10,0.76,0.32,0.17,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,6.5,0,0,0.9,0.2,0.09,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,7.5,0,10,0.83,0.24,0.12,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,10,0,5,0.69,0.36,0.19,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,6,0,10,0.93,0.18,7.0000000000000007E-2,4,0.81]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,8,0,0,0.78,0.24,0.12,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,9.5,0,10,0.7,0.32,0.17,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,7.5,0,5,0.8,0.23,0.11,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,9.5,0,0,0.69,0.28999999999999998,0.16,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,10,0,15,0.66,0.34,0.18,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,7,0,15,0.81,0.22,0.1,4,0.82]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,9,0,15,0.69,0.28000000000000003,0.15,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,7,0,0,0.79,0.19,0.09,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,7.5,0,15,0.76,0.23,0.11,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,9,0,15,0.68,0.28000000000000003,0.15,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,8,0,0,0.72,0.23,0.11,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,8.5,0,0,0.69,0.24,0.13,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,6.5,0,0,0.8,0.16,7.0000000000000007E-2,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,8,0,5,0.7,0.23,0.11,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,10,0,0,0.61,0.3,0.16,2,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",25,9.5,0,5,0.75,0.46,0.52,1,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",23,9.5,0,0,0.81,0.49,0.57999999999999996,1,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",22,9,0,0,0.88,0.46,0.56999999999999995,1,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",22,10,0,15,0.82,0.69,0.8,1,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",21,10,0,10,0.86,0.69,0.87,1,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",20,8,0,5,1.05,0.47,0.6,2,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",20,9.5,0,10,0.94,0.68,0.87,1,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",19,8,0,15,1.1100000000000001,0.59,0.69,2,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",18,7,0,10,1.27,0.48,0.57999999999999996,2,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",18,9.5,0,5,1.04,0.66,0.87,1,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",17,7.5,0,0,1.28,0.5,0.68,2,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",17,8.5,0,10,1.19,0.63,0.89,1,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",17,9,0,15,1.1399999999999999,0.64,0.85,1,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",16,7,0,15,1.43,0.56999999999999995,0.74,2,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",16,9,0,5,1.21,0.65,0.84,1,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",16,10,0,15,1.1299999999999999,0.67,0.83,1,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",15,8.5,0,10,1.35,0.63,0.83,1,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",15,9,0,15,1.3,0.64,0.84,1,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",14,6.5,0,5,1.7,0.54,0.8,2,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",14,7.5,0,15,1.57,0.59,0.84,2,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",14,10,0,10,1.29,0.69,0.84,1,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",13,8,0,0,1.6,0.6,0.84,1,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",13,9.5,0,15,1.44,0.67,0.85,1,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",12,6.5,0,0,1.97,0.55000000000000004,0.85,2,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",12,7.5,0,10,1.82,0.57999999999999996,0.83,1,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",12,10,0,0,1.49,0.7,0.92,1,0.88]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",11,7,0,15,2.08,0.56000000000000005,0.82,2,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",11,8.5,0,0,1.82,0.64,0.87,1,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",11,9.5,0,10,1.7,0.69,0.95,1,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",10,7,0,0,2.2599999999999998,0.55000000000000004,0.82,1,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",10,8.5,0,15,2.02,0.65,0.93,1,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",10,10,0,0,1.79,0.7,0.93,1,0.88]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",19,6.5,0,5,1.25,0.33,0.37,2,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",19,7,0,5,1.2,0.39,0.48,2,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",21,6,0,5,1.19,0.19,0.21,3,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",21,8,0,0,0.99,0.39,0.45,2,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",22,7,0,10,1.04,0.32,0.34,2,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",23,7.5,0,5,0.95,0.28999999999999998,0.31,2,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",23,8,0,15,0.92,0.43,0.45,2,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",24,7,0,10,0.95,0.24,0.25,2,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",25,7,0,5,0.91,0.19,0.2,2,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",25,7.5,0,10,0.88,0.27,0.27,2,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,6,0,0,0.95,0.13,0.12,3,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,7.5,0,10,0.84,0.24,0.24,2,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,9,0,0,0.74,0.3,0.33,2,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,10,0,5,0.69,0.48,0.54,1,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",27,8,0,0,0.77,0.2,0.21,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",27,9.5,0,10,0.69,0.43,0.46,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,6.5,0,0,0.84,0.14000000000000001,0.12,3,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,7.5,0,5,0.78,0.19,0.18,2,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,9.5,0,0,0.66,0.28999999999999998,0.32,2,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",29,6.5,0,10,0.82,0.16,0.15,3,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",29,9.5,0,5,0.64,0.3,0.33,2,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",30,6,0,15,0.83,0.14000000000000001,0.11,4,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",30,8.5,0,5,0.67,0.21,0.21,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",30,8.5,0,10,0.67,0.24,0.23,2,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",31,7,0,5,0.74,0.15,0.13,3,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",31,8,0,15,0.68,0.22,0.21,2,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",31,10,0,5,0.57999999999999996,0.28999999999999998,0.3,2,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",32,7.5,0,0,0.68,0.15,0.12,3,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",32,8.5,0,5,0.63,0.2,0.2,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",32,9.5,0,15,0.59,0.28000000000000003,0.3,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",33,7.5,0,5,0.66,0.16,0.13,3,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",33,9.5,0,0,0.56000000000000005,0.22,0.22,2,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",34,6,0,5,0.73,0.09,0.06,4,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",34,9,0,5,0.56999999999999995,0.2,0.2,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",35,6,0,10,0.71,0.09,0.06,4,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",35,6.5,0,0,0.68,0.08,0.06,3,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",35,9,0,10,0.56000000000000005,0.21,0.2,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",36,6,0,5,0.69,0.08,0.05,4,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",36,7.5,0,10,0.61,0.14000000000000001,0.11,3,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",36,10,0,10,0.5,0.25,0.24,2,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,6.5,0,10,0.65,0.09,7.0000000000000007E-2,4,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,8,0,5,0.56999999999999995,0.15,0.11,3,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,9.5,0,10,0.51,0.22,0.21,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,7,0,10,0.6,0.11,7.0000000000000007E-2,3,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,8,0,10,0.55000000000000004,0.15,0.11,3,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,6.5,0,15,0.61,0.09,0.06,4,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,8,0,15,0.54,0.16,0.11,3,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,9,0,10,0.5,0.18,0.16,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,7,0,15,0.56999999999999995,0.1,7.0000000000000007E-2,3,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,8.5,0,15,0.51,0.16,0.12,2,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,10,0,15,0.45,0.23,0.21,2,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,6.5,0,10,0.57999999999999996,0.08,0.05,4,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,8.5,0,5,0.49,0.13,0.1,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,7,0,0,0.54,7.0000000000000007E-2,0.04,3,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,8,0,10,0.5,0.11,0.08,3,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,10,0,0,0.43,0.17,0.14000000000000001,2,0.88]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,7,0,15,0.53,0.09,0.05,4,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,8.5,0,0,0.47,0.11,7.0000000000000007E-2,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,9.5,0,10,0.44,0.17,0.13,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,7,0,0,0.51,0.06,0.04,4,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,9,0,15,0.44,0.15,0.1,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,6,0,0,0.55000000000000004,0.04,0.02,5,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,7,0,10,0.51,7.0000000000000007E-2,0.04,4,0.84]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,9,0,0,0.43,0.11,0.08,2,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,6,0,15,0.54,0.06,0.02,5,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,9,0,5,0.42,0.12,0.08,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,6,0,0,0.53,0.04,0.02,5,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,7.5,0,5,0.47,7.0000000000000007E-2,0.04,3,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,8,0,15,0.45,0.1,0.06,3,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,6.5,0,5,0.5,0.05,0.02,5,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,8,0,0,0.44,7.0000000000000007E-2,0.04,3,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,9.5,0,5,0.39,0.12,0.08,2,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,7.5,0,5,0.45,0.06,0.04,3,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,8,0,5,0.43,7.0000000000000007E-2,0.05,3,0.85]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,9.5,0,0,0.38,0.11,7.0000000000000007E-2,2,0.87]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,6.5,0,5,0.48,0.04,0.02,5,0.83]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,9,0,5,0.39,0.09,0.06,2,0.86]
[7,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,10,0,5,0.36,0.13,0.09,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",21,9,0,10,2.19,0.72,0.54,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",20,8.5,0,10,2.38,0.72,0.53,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",20,9.5,0,5,2.21,0.78,0.62,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",19,9,0,15,2.42,0.79,0.65,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",18,8,0,5,2.73,0.75,0.56000000000000005,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",18,9.5,0,5,2.4500000000000002,0.83,0.71,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",17,9,0,0,2.66,0.85,0.71,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",17,9.5,0,15,2.61,0.8,0.72,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",16,7.5,0,10,3.21,0.81,0.64,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",16,9,0,10,2.87,0.8,0.72,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",15,7.5,0,15,3.43,0.82,0.72,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",15,8,0,10,3.29,0.82,0.72,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",14,7,0,0,3.75,0.84,0.69,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",14,8,0,15,3.54,0.8,0.72,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",14,9,0,15,3.28,0.79,0.72,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",13,6.5,0,15,4.29,0.82,0.73,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",13,9,0,0,3.48,0.79,0.72,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",13,10,0,15,3.3,0.8,0.79,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",12,6.5,0,15,4.6500000000000004,0.81,0.75,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",12,8.5,0,15,3.97,0.79,0.74,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",11,6,0,0,5.19,0.82,0.79,"/",0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",11,8,0,15,4.5,0.8,0.77,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",11,10,0,0,3.84,0.86,0.87,2,0.88]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",10,6,0,10,5.8,0.79,0.73,"/",0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",10,8.5,0,0,4.6900000000000004,0.85,0.84,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",10,9.5,0,15,4.43,0.85,0.9,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",16,6.5,0,0,3.42,0.67,0.47,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",18,6.5,0,15,3.1,0.61,0.4,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",18,7,0,15,2.98,0.65,0.46,3,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",19,7.5,0,0,2.66,0.65,0.44,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",20,7,0,0,2.63,0.61,0.38,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",21,7,0,0,2.5099999999999998,0.57999999999999996,0.35,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",22,6,0,5,2.62,0.5,0.25,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",22,7.5,0,5,2.3199999999999998,0.59,0.37,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",22,9,0,5,2.08,0.68,0.49,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",23,6.5,0,5,2.4,0.5,0.28000000000000003,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",23,8.5,0,10,2.0699999999999998,0.61,0.41,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",24,7,0,5,2.21,0.52,0.3,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",24,8.5,0,5,1.98,0.6,0.39,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",24,9.5,0,0,1.82,0.64,0.46,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",25,7.5,0,5,2.0499999999999998,0.53,0.32,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",25,9,0,5,1.83,0.6,0.4,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,6,0,5,2.21,0.38,0.18,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,8.5,0,10,1.83,0.56000000000000005,0.35,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",27,6,0,10,2.14,0.37,0.17,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",27,6.5,0,5,2.0499999999999998,0.4,0.2,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",27,9.5,0,10,1.65,0.59,0.39,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,6,0,10,2.0699999999999998,0.35,0.16,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,8,0,10,1.77,0.5,0.3,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,10,0,15,1.53,0.59,0.41,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",29,6.5,0,10,1.92,0.36,0.18,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",29,7.5,0,10,1.77,0.44,0.24,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",29,9.5,0,10,1.53,0.56000000000000005,0.36,2,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",30,7,0,15,1.79,0.39,0.2,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",30,8.5,0,10,1.59,0.5,0.3,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",31,7,0,0,1.7,0.33,0.17,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",31,7,0,10,1.73,0.36,0.18,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",31,9,0,15,1.49,0.52,0.31,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",32,7,0,15,1.68,0.34,0.17,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",32,8.5,0,0,1.47,0.44,0.25,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",32,10,0,15,1.34,0.55000000000000004,0.34,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",33,8,0,5,1.49,0.39,0.21,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",33,8.5,0,15,1.45,0.45,0.25,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",34,6,0,0,1.68,0.26,0.12,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",34,7.5,0,15,1.52,0.36,0.18,3,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",34,10,0,5,1.26,0.53,0.3,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",35,6,0,15,1.66,0.26,0.13,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",35,9,0,10,1.32,0.45,0.24,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",35,9.5,0,15,1.27,0.49,0.27,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",36,7.5,0,0,1.41,0.31,0.16,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",36,9.5,0,0,1.22,0.45,0.24,3,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,6,0,0,1.55,0.22,0.1,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,8.5,0,5,1.28,0.38,0.21,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,9,0,0,1.23,0.4,0.22,3,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,6.5,0,0,1.44,0.24,0.12,4,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,8,0,0,1.28,0.32,0.17,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,6,0,5,1.48,0.21,0.1,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,8,0,5,1.26,0.32,0.17,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,8.5,0,0,1.2,0.34,0.19,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,6.5,0,5,1.38,0.23,0.11,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,7.5,0,5,1.28,0.26,0.14000000000000001,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,9.5,0,5,1.1100000000000001,0.38,0.2,3,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,7,0,10,1.31,0.25,0.12,4,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,8,0,5,1.2,0.28000000000000003,0.15,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,9.5,0,5,1.08,0.37,0.19,3,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,7,0,5,1.27,0.24,0.11,4,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,9,0,10,1.1000000000000001,0.33,0.17,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,10,0,5,1.02,0.39,0.2,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,8,0,15,1.1499999999999999,0.27,0.15,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,10,0,10,1,0.37,0.19,2,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,6,0,10,1.32,0.19,0.08,5,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,8.5,0,10,1.08,0.28000000000000003,0.15,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,10,0,15,0.98,0.36,0.19,3,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,7.5,0,10,1.1399999999999999,0.24,0.12,4,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,10,0,0,0.94,0.32,0.17,2,0.88]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,6,0,10,1.26,0.18,0.08,5,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,7,0,15,1.17,0.23,0.1,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,9,0,10,1,0.28000000000000003,0.15,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,7,0,0,1.1200000000000001,0.21,0.09,4,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,9,0,15,0.98,0.28000000000000003,0.15,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,6.5,0,5,1.1499999999999999,0.19,0.08,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,6.5,0,10,1.1599999999999999,0.19,0.08,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,9,0,0,0.95,0.26,0.15,3,0.87]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,6.5,0,15,1.1399999999999999,0.19,0.08,4,0.83]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,8.5,0,5,0.97,0.26,0.13,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,9.5,0,15,0.91,0.28999999999999998,0.16,3,0.86]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,7.5,0,10,1.03,0.22,0.1,4,0.84]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,8,0,15,0.99,0.24,0.12,3,0.85]
[7,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,10,0,5,0.86,0.31,0.16,3,0.87]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,8.5,0,5,0.76,0.41,0.87,1,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,9.5,0,5,0.77,0.45,0.91,1,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,10,0,15,0.76,0.5,0.9,1,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,9.5,0,0,0.81,0.43,0.92,1,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,9.5,0,0,0.86,0.43,0.94,1,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,10,0,10,0.86,0.49,0.95,1,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,9.5,0,5,0.94,0.46,0.94,1,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,8.5,0,5,1.08,0.43,0.93,1,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,9,0,10,1.06,0.46,0.93,1,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,7.5,0,5,1.25,0.4,0.89,1,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,9.5,0,10,1.1299999999999999,0.48,0.94,1,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,9,0,10,1.27,0.47,0.93,1,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",10,6,0,15,1.54,0.35,0.89,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",11,6.5,0,10,1.34,0.37,0.89,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",11,7.5,0,0,1.22,0.37,0.88,1,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",13,6.5,0,10,1.1399999999999999,0.36,0.85,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",14,6.5,0,10,1.05,0.36,0.85,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",15,6.5,0,0,0.94,0.28000000000000003,0.8,2,0.86]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",16,6.5,0,15,0.93,0.37,0.8,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",16,8,0,0,0.82,0.37,0.81,1,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",17,7,0,10,0.84,0.38,0.81,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",18,6,0,0,0.81,0.26,0.63,2,0.86]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",18,8.5,0,15,0.73,0.45,0.87,1,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",18,9.5,0,5,0.68,0.45,0.89,1,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",19,6.5,0,10,0.78,0.34,0.68,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",19,9.5,0,10,0.65,0.47,0.89,1,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",19,10,0,15,0.64,0.49,0.9,1,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",20,8,0,10,0.68,0.42,0.79,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",20,10,0,0,0.59,0.44,0.89,1,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",21,6.5,0,10,0.7,0.34,0.56999999999999995,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",21,7.5,0,15,0.67,0.41,0.73,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",21,10,0,10,0.57999999999999996,0.49,0.88,1,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",22,7.5,0,0,0.61,0.34,0.66,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",22,8.5,0,10,0.6,0.42,0.77,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,6.5,0,5,0.63,0.3,0.48,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,8.5,0,15,0.57999999999999996,0.44,0.75,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",23,9,0,0,0.54,0.39,0.75,1,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,7,0,15,0.6,0.37,0.53,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,8.5,0,5,0.54,0.41,0.72,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,6,0,15,0.62,0.28999999999999998,0.32,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,8,0,10,0.54,0.41,0.62,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,9,0,15,0.51,0.47,0.74,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,6,0,5,0.56999999999999995,0.19,0.28000000000000003,3,0.86]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,7.5,0,15,0.54,0.38,0.51,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",26,9.5,0,10,0.48,0.46,0.75,1,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,6,0,15,0.56999999999999995,0.28999999999999998,0.25,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,9,0,15,0.48,0.46,0.67,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,9.5,0,15,0.46,0.49,0.72,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,7,0,10,0.51,0.3,0.37,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,10,0,0,0.42,0.43,0.7,1,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,6.5,0,15,0.51,0.27,0.27,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",29,8.5,0,0,0.44,0.33,0.5,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,6,0,0,0.48,7.0000000000000007E-2,0.13,3,0.86]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,7,0,0,0.46,0.14000000000000001,0.27,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,8,0,15,0.46,0.39,0.43,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,10,0,10,0.4,0.47,0.67,1,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,8,0,5,0.43,0.3,0.39,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,9.5,0,15,0.4,0.46,0.57999999999999996,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,6.5,0,5,0.45,0.13,0.18,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,7.5,0,10,0.44,0.28999999999999998,0.28999999999999998,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,10,0,5,0.38,0.42,0.59,1,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,7,0,15,0.44,0.27,0.21,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,8.5,0,5,0.39,0.32,0.39,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,9.5,0,10,0.38,0.41,0.51,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,7,0,5,0.42,0.16,0.18,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,8.5,0,15,0.39,0.37,0.36,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,7,0,10,0.41,0.2,0.16,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,8.5,0,0,0.36,0.21,0.3,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,9,0,5,0.36,0.32,0.38,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,6,0,15,0.43,0.14000000000000001,0.05,5,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,9,0,10,0.36,0.34,0.36,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,6,0,0,0.39,0.03,0.03,4,0.86]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,7.5,0,10,0.38,0.21,0.17,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,9.5,0,5,0.33,0.33,0.38,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,6,0,10,0.4,0.08,0.04,5,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,7.5,0,0,0.35,0.08,0.1,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,9.5,0,10,0.33,0.35,0.37,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,7,0,5,0.36,0.08,0.09,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,8,0,10,0.35,0.22,0.18,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,6.5,0,10,0.37,0.09,0.04,4,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,8,0,15,0.34,0.25,0.16,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,8.5,0,5,0.33,0.2,0.2,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,6.5,0,15,0.36,0.1,0.04,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,8,0,10,0.33,0.19,0.14000000000000001,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,9.5,0,15,0.31,0.35,0.28000000000000003,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,7.5,0,15,0.34,0.18,0.08,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,8.5,0,15,0.32,0.26,0.17,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,10,0,10,0.28999999999999998,0.33,0.31,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,7,0,15,0.34,0.11,0.05,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,9,0,15,0.3,0.28000000000000003,0.19,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,10,0,15,0.28000000000000003,0.35,0.28999999999999998,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,9,0,0,0.28000000000000003,0.11,0.13,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,6,0,0,0.32,0.01,0.01,4,0.86]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,6.5,0,15,0.33,0.05,0.02,5,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,9.5,0,0,0.27,0.13,0.16,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,6.5,0,0,0.31,0.02,0.01,4,0.86]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,8,0,0,0.28999999999999998,0.04,0.05,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,8.5,0,15,0.28999999999999998,0.2,0.1,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,6.5,0,0,0.3,0.02,0.01,4,0.86]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,8,0,0,0.28000000000000003,0.03,0.04,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,9.5,0,0,0.26,0.11,0.13,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,7.5,0,5,0.28999999999999998,0.04,0.03,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,9.5,0,0,0.25,0.09,0.11,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,6,0,5,0.31,0.01,0.01,6,0.86]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,7,0,15,0.3,0.05,0.02,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,9,0,5,0.26,0.1,0.09,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,7,0,0,0.28000000000000003,0.01,0.01,4,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,8,0,5,0.27,0.05,0.03,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,9,0,15,0.26,0.18,0.08,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",35,9.5,0,15,0.8,0.61,0.51,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",33,9,0,15,0.87,0.63,0.51,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",31,8.5,0,10,0.95,0.64,0.52,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",31,10,0,5,0.86,0.74,0.71,1,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",30,9.5,0,10,0.93,0.73,0.7,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",29,8,0,0,1,0.64,0.51,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,8,0,10,1.08,0.69,0.6,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",28,9.5,0,5,0.98,0.77,0.73,1,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,8,0,10,1.1200000000000001,0.7,0.63,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",27,9,0,0,1.02,0.75,0.72,1,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,8,0,10,1.1599999999999999,0.71,0.65,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",26,9.5,0,5,1.06,0.78,0.76,1,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,7.5,0,10,1.24,0.7,0.64,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",25,10,0,10,1.08,0.82,0.82,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,7.5,0,10,1.29,0.71,0.67,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",24,9,0,5,1.17,0.77,0.77,1,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,8,0,15,1.32,0.74,0.73,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",23,9,0,10,1.24,0.79,0.79,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,7,0,10,1.45,0.69,0.66,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,8.5,0,10,1.33,0.77,0.78,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",22,10,0,10,1.23,0.85,0.89,1,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,6.5,0,5,1.54,0.66,0.64,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",21,9,0,10,1.36,0.8,0.85,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,6,0,10,1.69,0.64,0.6,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,7.5,0,10,1.55,0.73,0.77,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",20,10,0,15,1.36,0.88,0.87,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,6,0,10,1.78,0.66,0.64,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",19,7.5,0,10,1.63,0.74,0.79,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,6,0,15,1.91,0.69,0.69,4,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,7,0,15,1.79,0.74,0.8,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",18,9,0,15,1.6,0.86,0.85,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,7,0,0,1.8,0.69,0.79,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,8,0,15,1.79,0.82,0.85,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",17,9,0,15,1.69,0.85,0.86,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,6.5,0,15,2.08,0.73,0.82,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,8.5,0,0,1.77,0.82,0.84,1,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",16,9.5,0,15,1.75,0.87,0.89,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,8,0,5,1.98,0.82,0.84,1,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",15,8,0,15,2.0299999999999998,0.83,0.84,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,6,0,0,2.2999999999999998,0.65,0.81,2,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,7,0,15,2.31,0.79,0.86,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",14,10,0,5,1.91,0.9,0.95,1,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,7.5,0,0,2.29,0.8,0.85,1,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,8,0,0,2.23,0.82,0.89,1,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",13,9.5,0,15,2.15,0.88,0.96,1,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,7,0,0,2.5499999999999998,0.78,0.86,1,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",12,9.5,0,0,2.25,0.87,0.97,1,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,7,0,5,2.85,0.78,0.92,1,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,8.5,0,5,2.63,0.85,0.96,1,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",11,10,0,5,2.4300000000000002,0.88,0.95,1,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,6.5,0,0,3.13,0.75,0.93,1,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Adecuado/a",10,8.5,0,5,2.89,0.84,0.95,1,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",22,6,0,5,1.51,0.62,0.47,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",24,6.5,0,10,1.37,0.64,0.48,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",25,6.5,0,5,1.29,0.59,0.43,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",27,6,0,10,1.25,0.43,0.28999999999999998,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,6,0,10,1.21,0.4,0.26,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",28,7.5,0,10,1.1100000000000001,0.61,0.49,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,6,0,15,1.1399999999999999,0.36,0.23,5,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",30,8,0,15,1.02,0.6,0.49,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",31,6,0,10,1.0900000000000001,0.37,0.22,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,6.5,0,10,1.03,0.39,0.26,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",32,7.5,0,10,0.97,0.48,0.37,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,6.5,0,10,1,0.39,0.24,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",33,8.5,0,15,0.9,0.56999999999999995,0.46,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,6.5,0,5,0.95,0.36,0.23,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",34,7.5,0,5,0.9,0.46,0.33,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,6,0,5,0.95,0.32,0.19,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",35,8,0,10,0.86,0.48,0.37,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,6,0,0,0.89,0.31,0.18,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,8.5,0,10,0.82,0.52,0.39,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",36,9,0,0,0.77,0.56000000000000005,0.42,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,7,0,0,0.83,0.38,0.25,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",37,9.5,0,0,0.73,0.56999999999999995,0.43,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,6,0,5,0.87,0.31,0.17,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,8,0,0,0.76,0.45,0.31,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",38,10,0,10,0.71,0.57999999999999996,0.47,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,6.5,0,0,0.8,0.33,0.18,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,8,0,5,0.76,0.44,0.31,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",39,10,0,0,0.68,0.56999999999999995,0.43,1,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,7.5,0,10,0.78,0.39,0.26,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",40,8.5,0,0,0.71,0.48,0.32,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,6.5,0,15,0.81,0.32,0.19,5,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,7,0,0,0.75,0.36,0.2,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",41,9,0,10,0.7,0.48,0.35,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,7,0,5,0.75,0.36,0.21,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",42,8.5,0,15,0.71,0.42,0.3,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,6,0,5,0.77,0.26,0.12,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,6.5,0,10,0.76,0.32,0.17,5,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,8.5,0,5,0.67,0.44,0.3,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",43,10,0,5,0.62,0.52,0.38,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,8,0,10,0.69,0.4,0.26,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",44,10,0,10,0.62,0.49,0.36,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,6,0,5,0.74,0.24,0.11,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,8.5,0,10,0.65,0.42,0.28000000000000003,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",45,9.5,0,10,0.62,0.45,0.33,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,7,0,10,0.7,0.33,0.18,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,9,0,15,0.63,0.41,0.28999999999999998,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",46,10,0,10,0.59,0.45,0.35,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,7,0,10,0.68,0.32,0.17,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",47,9,0,10,0.61,0.42,0.28999999999999998,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,6.5,0,15,0.69,0.25,0.14000000000000001,6,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",48,7.5,0,10,0.65,0.35,0.2,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,6,0,0,0.65,0.12,0.06,4,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,7.5,0,15,0.64,0.33,0.19,5,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",49,8,0,15,0.62,0.37,0.22,4,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,6,0,15,0.69,0.18,0.09,7,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,8,0,0,0.57999999999999996,0.31,0.18,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,9.5,0,15,0.56000000000000005,0.41,0.28999999999999998,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 105w","3 módulos de 18 LEDs c/u -Total 54 LEDs-\r DRIVER: MEANWELL ELG-100-48B","Insuficiente",50,10,0,15,0.55000000000000004,0.42,0.31,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",26,8,0,15,0.87,0.41,0.59,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",26,9.5,0,5,0.78,0.43,0.74,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",25,9.5,0,0,0.8,0.41,0.73,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",24,9.5,0,5,0.85,0.43,0.78,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",24,10,0,15,0.84,0.5,0.8,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",23,9.5,0,15,0.9,0.48,0.8,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",22,9.5,0,5,0.92,0.44,0.83,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",21,9.5,0,10,0.98,0.47,0.84,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",20,10,0,0,0.97,0.44,0.88,1,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",19,9,0,15,1.1200000000000001,0.46,0.86,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",18,7.5,0,15,1.29,0.42,0.8,2,0.83]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",18,8.5,0,10,1.2,0.43,0.85,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",17,8,0,15,1.32,0.44,0.84,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",17,10,0,10,1.17,0.48,0.9,1,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",16,9,0,15,1.33,0.46,0.89,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",15,9,0,5,1.39,0.43,0.91,1,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",15,9.5,0,10,1.37,0.47,0.91,1,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",14,8.5,0,10,1.55,0.44,0.9,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",14,10,0,0,1.39,0.46,0.94,1,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",13,9.5,0,10,1.57,0.48,0.93,1,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",12,9,0,5,1.73,0.45,0.93,1,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",11,7.5,0,15,2.11,0.43,0.92,2,0.83]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",11,9,0,5,1.89,0.45,0.94,1,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",11,10,0,15,1.82,0.5,0.95,1,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",10,9.5,0,5,2.0299999999999998,0.46,0.94,1,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",10,7,0,0,2.27,0.34,0.92,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",11,8,0,0,1.96,0.39,0.91,1,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",13,6,0,5,1.89,0.3,0.83,3,0.86]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",13,6.5,0,5,1.84,0.34,0.84,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",14,7,0,10,1.69,0.39,0.85,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",15,7,0,5,1.55,0.36,0.84,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",16,6.5,0,5,1.5,0.32,0.8,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",17,7,0,0,1.34,0.31,0.77,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",17,8.5,0,0,1.24,0.38,0.84,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",18,7.5,0,0,1.23,0.34,0.76,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",19,7,0,15,1.26,0.39,0.73,3,0.83]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",20,7.5,0,0,1.1100000000000001,0.34,0.74,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",20,9,0,0,1.02,0.39,0.84,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",21,7.5,0,0,1.05,0.34,0.7,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",22,8.5,0,0,0.96,0.37,0.77,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",23,6,0,15,1.1100000000000001,0.32,0.43,5,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",24,6,0,15,1.06,0.3,0.38,5,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",24,8.5,0,0,0.88,0.38,0.71,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",25,7,0,0,0.91,0.27,0.48,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",25,8,0,5,0.88,0.38,0.63,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",26,8,0,0,0.83,0.33,0.57999999999999996,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",27,7,0,15,0.89,0.35,0.43,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",27,9.5,0,0,0.74,0.42,0.7,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",28,7.5,0,10,0.82,0.35,0.45,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",28,8.5,0,0,0.75,0.35,0.56000000000000005,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",29,6,0,15,0.88,0.28000000000000003,0.22,5,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",29,9.5,0,0,0.69,0.39,0.63,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",30,6,0,10,0.84,0.22,0.18,5,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",30,8.5,0,0,0.7,0.32,0.48,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",30,10,0,15,0.67,0.48,0.67,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",31,7,0,0,0.73,0.14000000000000001,0.26,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",31,7.5,0,10,0.74,0.31,0.35,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",31,10,0,0,0.63,0.4,0.61,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",32,7,0,15,0.75,0.28999999999999998,0.26,4,0.83]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",32,8.5,0,0,0.66,0.28999999999999998,0.42,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",33,7,0,0,0.69,0.11,0.21,4,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",33,7.5,0,0,0.67,0.16,0.26,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",33,9,0,15,0.65,0.41,0.47,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",34,6,0,0,0.7,0.04,7.0000000000000007E-2,5,0.86]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",34,9,0,0,0.6,0.28999999999999998,0.4,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",35,6,0,5,0.7,0.08,7.0000000000000007E-2,6,0.86]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",35,8,0,5,0.63,0.25,0.28999999999999998,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",35,9,0,5,0.6,0.33,0.41,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",36,6,0,0,0.67,0.03,0.05,5,0.86]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",36,8,0,5,0.61,0.24,0.26,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",36,10,0,5,0.55000000000000004,0.38,0.48,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",37,6.5,0,5,0.65,0.09,0.09,5,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",37,8,0,0,0.57999999999999996,0.15,0.22,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",37,9.5,0,5,0.55000000000000004,0.34,0.4,2,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",38,7,0,5,0.61,0.11,0.12,4,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",38,9.5,0,0,0.53,0.27,0.34,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",39,6,0,10,0.64,0.09,0.04,7,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",39,7,0,15,0.61,0.21,0.11,5,0.83]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",39,9,0,10,0.54,0.31,0.3,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",40,6.5,0,0,0.57999999999999996,0.03,0.04,5,0.86]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",40,7.5,0,10,0.57999999999999996,0.18,0.13,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",41,6,0,5,0.6,0.04,0.02,6,0.86]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",41,6.5,0,10,0.6,0.1,0.04,6,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",41,8.5,0,0,0.51,0.13,0.18,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",42,6.5,0,15,0.59,0.1,0.04,6,0.83]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",42,8,0,5,0.53,0.14000000000000001,0.14000000000000001,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",42,9.5,0,15,0.49,0.34,0.28000000000000003,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",43,7,0,10,0.55000000000000004,0.1,0.05,5,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",43,8,0,15,0.53,0.22,0.12,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",43,9.5,0,5,0.47,0.25,0.26,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",44,7,0,15,0.55000000000000004,0.12,0.05,5,0.83]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",44,9,0,10,0.48,0.24,0.2,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",44,10,0,15,0.46,0.34,0.28000000000000003,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",45,7,0,5,0.52,0.05,0.04,5,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",45,8.5,0,15,0.49,0.23,0.13,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",46,6,0,10,0.55000000000000004,0.03,0.01,7,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",46,9,0,0,0.45,0.1,0.13,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",46,10,0,15,0.44,0.31,0.24,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",47,7.5,0,0,0.47,0.03,0.03,4,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",47,8,0,10,0.48,0.13,7.0000000000000007E-2,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",48,6.5,0,0,0.49,0.02,0.01,5,0.86]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",48,7.5,0,15,0.49,0.1,0.04,5,0.83]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",48,9.5,0,0,0.42,0.12,0.14000000000000001,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",49,7,0,0,0.47,0.02,0.02,5,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",49,8,0,0,0.44,0.04,0.03,4,0.85]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",49,9,0,15,0.44,0.21,0.11,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",50,8,0,5,0.44,0.06,0.04,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",50,9,0,0,0.41,7.0000000000000007E-2,7.0000000000000007E-2,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",50,10,0,0,0.39,0.13,0.14000000000000001,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",35,10,0,10,1.28,0.69,0.61,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",34,10,0,10,1.32,0.7,0.65,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",33,9.5,0,5,1.38,0.71,0.62,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",32,9.5,0,10,1.44,0.71,0.66,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",31,9,0,10,1.53,0.7,0.64,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",30,8,0,10,1.67,0.63,0.53,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",29,8,0,15,1.74,0.66,0.57999999999999996,4,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",29,9,0,10,1.63,0.73,0.68,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",28,7.5,0,10,1.84,0.64,0.53,4,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",28,9,0,10,1.69,0.74,0.7,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",27,8.5,0,15,1.82,0.72,0.69,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",26,7.5,0,0,1.9,0.67,0.62,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",26,9,0,5,1.8,0.75,0.73,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",26,9.5,0,10,1.77,0.78,0.78,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",25,8,0,0,1.92,0.7,0.67,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",25,9.5,0,15,1.86,0.8,0.81,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",24,7,0,5,2.17,0.66,0.62,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",24,10,0,5,1.85,0.81,0.84,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",23,7.5,0,10,2.23,0.71,0.69,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",23,8.5,0,0,2.04,0.73,0.74,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",22,6.5,0,15,2.5,0.68,0.62,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",22,8,0,10,2.27,0.75,0.75,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",22,9.5,0,15,2.11,0.85,0.87,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",21,6,0,5,2.61,0.62,0.56999999999999995,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",21,8,0,15,2.4,0.77,0.79,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",21,9.5,0,10,2.19,0.84,0.88,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",20,6.5,0,15,2.75,0.69,0.68,4,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",20,9,0,15,2.38,0.84,0.86,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",20,10,0,15,2.2599999999999998,0.87,0.87,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",19,7,0,10,2.78,0.71,0.76,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",19,8.5,0,15,2.58,0.83,0.86,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",18,6.5,0,15,3.06,0.71,0.76,4,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",18,9,0,0,2.54,0.83,0.83,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",17,6,0,0,3.13,0.64,0.69,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",17,7.5,0,0,2.9,0.73,0.82,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",17,8,0,15,2.97,0.82,0.83,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",16,6.5,0,0,3.24,0.67,0.78,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",16,8,0,0,3.01,0.8,0.82,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",16,9.5,0,0,2.79,0.86,0.88,1,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",15,7.5,0,5,3.37,0.79,0.83,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",15,8,0,0,3.2,0.8,0.84,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",15,9.5,0,0,2.98,0.87,0.93,1,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",14,8,0,5,3.51,0.82,0.86,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",14,9,0,5,3.33,0.85,0.93,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",13,6.5,0,5,4.0999999999999996,0.74,0.84,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",13,8.5,0,10,3.73,0.84,0.94,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",13,10,0,5,3.41,0.88,0.96,1,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",12,6.5,0,5,4.4400000000000004,0.76,0.86,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",12,8.5,0,5,3.99,0.84,0.96,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",12,10,0,10,3.74,0.88,0.96,1,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",11,7,0,5,4.72,0.77,0.93,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",11,9.5,0,15,4.21,0.87,0.96,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",11,10,0,5,4.03,0.87,0.96,1,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",10,7.5,0,10,5.14,0.81,0.95,"/",0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Adecuado/a",10,9,0,5,4.67,0.85,0.95,1,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",25,6,0,5,2.19,0.55000000000000004,0.37,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",26,7,0,0,1.95,0.64,0.49,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",27,6,0,15,2.1,0.45,0.32,7,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",28,7,0,15,1.91,0.56999999999999995,0.44,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",29,7,0,0,1.75,0.54,0.38,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",30,7,0,15,1.78,0.51,0.38,5,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",30,7.5,0,15,1.73,0.56000000000000005,0.44,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",32,6.5,0,0,1.62,0.4,0.25,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",32,8,0,0,1.5,0.57999999999999996,0.43,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",33,6,0,15,1.72,0.32,0.21,8,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",33,8.5,0,0,1.42,0.6,0.47,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",34,7.5,0,0,1.45,0.46,0.33,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",35,6,0,0,1.52,0.32,0.18,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",35,6.5,0,15,1.57,0.34,0.23,6,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",35,9,0,0,1.31,0.61,0.47,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",36,7,0,0,1.41,0.39,0.26,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",36,8.5,0,0,1.3,0.53,0.4,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",37,7.5,0,5,1.37,0.41,0.3,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",37,9.5,0,5,1.23,0.59,0.48,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",38,6,0,0,1.4,0.3,0.16,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",38,7.5,0,0,1.3,0.4,0.28000000000000003,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",39,6,0,0,1.36,0.3,0.15,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",39,8,0,0,1.24,0.44,0.31,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",39,8,0,15,1.3,0.41,0.31,4,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",40,6.5,0,0,1.3,0.33,0.18,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",40,7.5,0,0,1.24,0.39,0.26,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",40,9.5,0,0,1.1200000000000001,0.54,0.39,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",41,7,0,5,1.27,0.36,0.22,5,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",41,8.5,0,0,1.1499999999999999,0.47,0.33,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",41,9.5,0,0,1.0900000000000001,0.52,0.38,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",42,7,0,0,1.2,0.35,0.2,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",42,9,0,5,1.1100000000000001,0.48,0.35,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",43,7,0,5,1.21,0.35,0.2,5,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",43,8,0,10,1.1599999999999999,0.4,0.27,4,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",43,10,0,5,1.04,0.52,0.4,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",44,6,0,5,1.24,0.25,0.12,7,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",44,8.5,0,5,1.0900000000000001,0.43,0.28999999999999998,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",44,10,0,10,1.02,0.5,0.38,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",45,7.5,0,5,1.1200000000000001,0.37,0.22,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",45,9.5,0,15,1.03,0.43,0.33,4,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",46,6,0,5,1.19,0.24,0.1,7,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",46,7,0,10,1.1499999999999999,0.33,0.18,6,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",46,9,0,5,1.02,0.45,0.3,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",47,6.5,0,15,1.17,0.27,0.15,8,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",47,9,0,10,1.01,0.42,0.3,4,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",48,6.5,0,0,1.08,0.21,0.1,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",48,8,0,10,1.04,0.38,0.23,4,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",48,8.5,0,15,1.02,0.4,0.26,5,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",49,6.5,0,10,1.1100000000000001,0.22,0.13,7,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",49,8,0,0,0.98,0.35,0.21,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",49,9.5,0,10,0.94,0.42,0.3,4,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",50,7.5,0,5,1.01,0.31,0.17,5,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 140w","Definido por el usuario","Insuficiente",50,8,0,10,1,0.36,0.22,5,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",33,9.5,0,15,0.78,0.43,0.55000000000000004,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",32,9.5,0,15,0.8,0.44,0.59,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",30,8.5,0,15,0.91,0.41,0.53,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",29,9.5,0,15,0.89,0.46,0.66,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",28,8.5,0,15,0.97,0.43,0.61,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",27,8,0,15,1.04,0.4,0.57999999999999996,3,0.83]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",26,8,0,15,1.08,0.41,0.62,3,0.83]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",25,8,0,15,1.1200000000000001,0.42,0.66,3,0.83]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",25,9.5,0,0,0.99,0.41,0.74,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",24,10,0,5,1.03,0.46,0.8,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",23,9.5,0,15,1.1200000000000001,0.48,0.79,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",23,10,0,15,1.0900000000000001,0.49,0.82,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",21,8,0,15,1.33,0.44,0.76,3,0.83]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",21,10,0,10,1.18,0.48,0.85,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",20,9.5,0,15,1.28,0.47,0.84,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",20,10,0,15,1.25,0.49,0.86,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",19,10,0,15,1.31,0.49,0.88,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",18,8.5,0,15,1.51,0.44,0.83,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",17,7.5,0,15,1.7,0.42,0.8,3,0.83]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",17,10,0,15,1.47,0.49,0.89,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",16,8,0,15,1.75,0.44,0.83,2,0.83]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",16,10,0,5,1.54,0.47,0.92,1,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",15,9,0,15,1.76,0.46,0.9,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",14,9,0,0,1.82,0.41,0.93,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",13,8.5,0,10,2.0699999999999998,0.44,0.92,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",12,7,0,15,2.4700000000000002,0.4,0.88,2,0.83]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",12,9,0,0,2.12,0.42,0.94,1,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",12,9.5,0,5,2.1,0.46,0.94,1,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",11,9,0,5,2.35,0.45,0.94,1,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",10,7.5,0,15,2.88,0.43,0.93,2,0.83]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",10,9.5,0,5,2.52,0.46,0.94,1,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",11,6,0,0,2.71,0.28000000000000003,0.87,3,0.86]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",11,6.5,0,5,2.7,0.34,0.9,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",12,6.5,0,10,2.52,0.36,0.85,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",13,6,0,10,2.4,0.32,0.81,4,0.85]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",14,6.5,0,10,2.16,0.36,0.81,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",15,7,0,5,1.93,0.36,0.82,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",16,7,0,5,1.81,0.36,0.8,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",17,6,0,15,1.86,0.33,0.71,4,0.83]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",17,8,0,0,1.58,0.37,0.82,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",19,6,0,5,1.61,0.28999999999999998,0.62,4,0.85]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",20,6,0,0,1.49,0.25,0.55000000000000004,4,0.86]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",20,7,0,5,1.45,0.34,0.71,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",21,7,0,15,1.42,0.38,0.67,4,0.83]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",21,8,0,0,1.28,0.36,0.77,2,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",22,7,0,15,1.35,0.38,0.63,4,0.83]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",23,6,0,5,1.33,0.27,0.44,5,0.85]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",24,6.5,0,10,1.26,0.32,0.49,5,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",25,6,0,10,1.25,0.27,0.37,6,0.85]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",25,7,0,0,1.1299999999999999,0.28000000000000003,0.5,3,0.85]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",26,6,0,5,1.18,0.21,0.32,5,0.85]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",26,8,0,0,1.03,0.33,0.6,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",27,7.5,0,15,1.07,0.37,0.52,4,0.83]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",28,6,0,0,1.06,0.11,0.24,5,0.86]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",28,7.5,0,5,1.01,0.32,0.47,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",29,7.5,0,15,1,0.36,0.44,4,0.83]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",29,8.5,0,0,0.9,0.34,0.53,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",30,7.5,0,15,0.96,0.35,0.41,4,0.83]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",31,6.5,0,0,0.94,0.1,0.22,5,0.85]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",31,7.5,0,10,0.92,0.31,0.37,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",31,9,0,0,0.82,0.34,0.52,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",32,8,0,0,0.84,0.25,0.37,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",33,6,0,15,0.96,0.23,0.14000000000000001,7,0.83]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",33,7.5,0,5,0.85,0.25,0.3,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",34,6,0,5,0.9,0.1,0.1,6,0.85]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",34,6.5,0,10,0.89,0.2,0.17,6,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",34,8.5,0,0,0.77,0.25,0.37,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",35,7,0,5,0.83,0.17,0.2,5,0.85]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",35,8,0,15,0.8,0.33,0.31,4,0.83]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",36,6,0,5,0.85,0.08,7.0000000000000007E-2,7,0.85]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",36,6,0,10,0.87,0.14000000000000001,7.0000000000000007E-2,7,0.85]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",36,9,0,5,0.72,0.32,0.4,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",36,9.5,0,15,0.71,0.4,0.46,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",37,7.5,0,5,0.76,0.19,0.2,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",37,9.5,0,0,0.67,0.28999999999999998,0.38,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",38,6,0,5,0.81,0.06,0.05,7,0.85]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",38,7,0,15,0.78,0.22,0.14000000000000001,6,0.83]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",38,9.5,0,5,0.67,0.33,0.39,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",39,7,0,0,0.73,0.06,0.09,5,0.85]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",39,8,0,5,0.7,0.2,0.22,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",40,6.5,0,5,0.74,7.0000000000000007E-2,0.06,6,0.85]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",40,8,0,10,0.7,0.23,0.2,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",40,8.5,0,0,0.66,0.16,0.22,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",41,6.5,0,10,0.74,0.11,0.05,7,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",41,8,0,5,0.67,0.17,0.18,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",41,10,0,10,0.61,0.35,0.38,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",42,7.5,0,10,0.68,0.16,0.12,5,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",42,8.5,0,10,0.64,0.25,0.21,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",42,10,0,5,0.59,0.31,0.34,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",43,7,0,10,0.69,0.11,0.06,6,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",43,9,0,10,0.61,0.26,0.23,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",43,10,0,10,0.57999999999999996,0.33,0.34,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",44,8.5,0,15,0.62,0.25,0.17,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",44,10,0,15,0.56999999999999995,0.35,0.31,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",45,6.5,0,10,0.67,7.0000000000000007E-2,0.02,7,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",45,8.5,0,5,0.59,0.15,0.15,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",45,9.5,0,15,0.56999999999999995,0.3,0.24,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",46,8,0,10,0.61,0.15,0.1,5,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",46,8.5,0,15,0.59,0.23,0.14000000000000001,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",47,6,0,5,0.65,0.02,0.01,8,0.85]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",47,9,0,0,0.55000000000000004,0.1,0.13,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",47,10,0,10,0.53,0.28000000000000003,0.25,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",48,7.5,0,0,0.57999999999999996,0.03,0.03,5,0.85]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",48,9,0,15,0.55000000000000004,0.24,0.15,4,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",49,6,0,0,0.61,0.01,0.01,8,0.86]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",49,7,0,10,0.6,0.06,0.02,7,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",49,9.5,0,0,0.51,0.11,0.13,3,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",50,6.5,0,15,0.61,0.04,0.01,8,0.83]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",50,8,0,0,0.54,0.04,0.04,5,0.84]
[12,"UNILATERAL","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",50,9,0,10,0.53,0.17,0.12,4,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",37,10,0,5,1.49,0.65,0.54,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",35,10,0,0,1.55,0.7,0.59,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",33,9.5,0,10,1.73,0.72,0.62,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",32,9,0,5,1.81,0.7,0.57999999999999996,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",31,8.5,0,10,1.95,0.66,0.55000000000000004,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",31,9.5,0,0,1.79,0.75,0.7,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",30,9.5,0,10,1.91,0.76,0.73,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",29,8.5,0,5,2.0499999999999998,0.72,0.67,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",29,10,0,10,1.92,0.79,0.78,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",28,9,0,10,2.1,0.75,0.73,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",28,10,0,10,1.99,0.79,0.79,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",27,8.5,0,5,2.2000000000000002,0.73,0.7,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",27,10,0,10,2.06,0.8,0.81,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",26,9,0,15,2.27,0.77,0.77,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",26,10,0,15,2.16,0.82,0.84,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",25,10,0,0,2.17,0.8,0.82,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",24,7.5,0,5,2.61,0.7,0.69,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",24,8.5,0,0,2.4300000000000002,0.74,0.74,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",23,6.5,0,5,2.88,0.64,0.56999999999999995,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",23,8,0,5,2.65,0.73,0.74,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",23,9.5,0,5,2.46,0.8,0.84,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",22,7.5,0,15,2.93,0.74,0.75,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",22,8.5,0,10,2.74,0.78,0.81,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",22,10,0,10,2.5299999999999998,0.86,0.88,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",21,7,0,10,3.12,0.7,0.72,4,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",21,9.5,0,15,2.74,0.85,0.88,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",21,10,0,10,2.65,0.86,0.87,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",20,9,0,0,2.84,0.8,0.84,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",20,10,0,15,2.8,0.87,0.86,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",19,6.5,0,15,3.6,0.7,0.74,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",19,9,0,15,3.11,0.85,0.84,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",18,6.5,0,0,3.58,0.67,0.73,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",18,8,0,15,3.47,0.82,0.84,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",18,10,0,0,3.01,0.86,0.87,1,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",17,6,0,10,4.09,0.68,0.75,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",17,9,0,0,3.34,0.84,0.85,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",17,10,0,15,3.29,0.87,0.9,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",16,7.5,0,0,3.83,0.76,0.81,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",16,8,0,10,3.87,0.82,0.83,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",15,6,0,0,4.4000000000000004,0.65,0.78,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",15,7,0,15,4.42,0.78,0.82,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",15,9,0,0,3.78,0.86,0.89,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",14,7,0,0,4.4800000000000004,0.75,0.84,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",14,8,0,0,4.26,0.82,0.85,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",14,9,0,15,4.22,0.86,0.94,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",13,6.5,0,0,4.95,0.72,0.84,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",13,9,0,0,4.3600000000000003,0.86,0.96,1,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",12,6.5,0,5,5.51,0.76,0.85,"/",0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",12,8,0,5,5.08,0.82,0.94,"/",0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",12,9.5,0,5,4.7,0.87,0.96,1,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",11,6,0,0,6,0.71,0.86,"/",0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",11,8.5,0,5,5.4,0.85,0.97,"/",0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",11,10,0,5,5,0.87,0.95,"/",0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",10,7,0,5,6.44,0.78,0.95,"/",0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",10,8,0,0,5.97,0.83,0.97,"/",0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Adecuado/a",10,10,0,5,5.5,0.88,0.96,"/",0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",24,6.5,0,0,2.68,0.63,0.48,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",26,6,0,15,2.71,0.51,0.36,7,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",28,6,0,15,2.5099999999999998,0.42,0.28999999999999998,8,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",29,6.5,0,15,2.35,0.47,0.35,6,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",29,7,0,10,2.2599999999999998,0.54,0.4,4,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",31,6,0,15,2.27,0.37,0.23,8,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",31,7,0,15,2.14,0.46,0.35,5,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",32,6.5,0,15,2.14,0.39,0.27,6,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",33,6,0,0,2,0.34,0.2,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",33,7,0,15,2.0099999999999998,0.42,0.3,5,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",33,8,0,15,1.9,0.54,0.42,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",34,7,0,15,1.95,0.41,0.28999999999999998,5,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",35,6.5,0,0,1.84,0.36,0.22,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",35,7.5,0,15,1.84,0.44,0.32,5,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",36,7,0,5,1.79,0.39,0.27,5,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",36,7,0,15,1.84,0.37,0.27,6,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",37,6,0,0,1.78,0.31,0.17,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",37,8.5,0,0,1.58,0.5,0.37,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",37,9.5,0,5,1.53,0.59,0.47,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",38,7.5,0,0,1.61,0.4,0.28000000000000003,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",38,9.5,0,10,1.51,0.56000000000000005,0.45,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",39,6.5,0,15,1.75,0.33,0.2,7,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",39,8,0,0,1.53,0.44,0.31,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",39,9.5,0,15,1.48,0.53,0.43,4,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",40,7.5,0,5,1.57,0.39,0.27,4,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",40,9.5,0,0,1.39,0.53,0.4,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",41,6.5,0,0,1.57,0.33,0.17,5,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",41,7,0,15,1.62,0.35,0.22,6,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",41,9.5,0,0,1.35,0.52,0.38,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",42,6.5,0,0,1.53,0.32,0.16,5,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",42,8,0,0,1.42,0.42,0.28000000000000003,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",43,6,0,5,1.58,0.28000000000000003,0.13,7,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",43,6.5,0,0,1.5,0.3,0.15,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",43,8.5,0,0,1.36,0.44,0.3,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",43,10,0,0,1.26,0.51,0.39,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",44,8,0,5,1.39,0.4,0.26,4,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",44,10,0,5,1.26,0.5,0.38,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",45,6,0,0,1.46,0.23,0.1,6,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",45,8.5,0,5,1.32,0.43,0.28999999999999998,4,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",45,9.5,0,5,1.26,0.47,0.34,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",46,7,0,5,1.4,0.33,0.18,5,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",46,9,0,10,1.28,0.44,0.3,4,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",47,6,0,5,1.44,0.22,0.1,8,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",47,7,0,5,1.37,0.33,0.17,6,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",47,9,0,5,1.24,0.44,0.3,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",48,6.5,0,10,1.4,0.27,0.14000000000000001,8,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",48,7.5,0,5,1.31,0.35,0.2,5,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",48,10,0,15,1.17,0.43,0.33,4,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",49,7.5,0,10,1.3,0.34,0.19,6,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",49,8,0,10,1.27,0.37,0.23,5,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",50,6.5,0,10,1.35,0.23,0.13,8,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",50,7.5,0,15,1.29,0.33,0.19,6,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED 200w","6 módulos de 18 LEDs c/u -Total 108 LEDs-\r DRIVER: MEANWELL ELG-200-48B","Insuficiente",50,9.5,0,10,1.1499999999999999,0.42,0.3,4,0.84]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",16,7,0,5,0.81,0.47,0.72,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",16,7.5,0,15,0.77,0.47,0.75,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",15,6.5,0,15,0.88,0.43,0.75,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",15,8.5,0,10,0.77,0.47,0.75,1,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",14,8,0,0,0.86,0.49,0.72,1,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",13,6,0,0,1.08,0.41,0.76,2,0.82]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",13,7.5,0,15,0.94,0.48,0.79,1,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",13,8,0,0,0.93,0.48,0.7,1,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",13,10,0,10,0.81,0.56000000000000005,0.88,1,0.84]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",12,8,0,5,1,0.49,0.78,1,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",12,9,0,15,0.92,0.54,0.86,1,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",11,6.5,0,5,1.22,0.44,0.76,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",11,9,0,0,1.02,0.52,0.86,1,0.84]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",11,9.5,0,5,0.99,0.55000000000000004,0.94,1,0.84]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",10,6.5,0,15,1.32,0.47,0.82,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",10,8.5,0,5,1.1599999999999999,0.54,0.93,1,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",15,6,0,0,0.94,0.33,0.53,2,0.82]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",15,9.5,0,10,0.72,0.5,0.81,1,0.84]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",16,8.5,0,15,0.72,0.47,0.76,1,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",17,6,0,10,0.81,0.41,0.43,3,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",17,9,0,0,0.66,0.5,0.78,1,0.84]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",18,6.5,0,5,0.74,0.38,0.44,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",18,7.5,0,0,0.7,0.41,0.59,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",18,10,0,10,0.57999999999999996,0.5,0.8,1,0.84]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",19,6,0,0,0.74,0.15,0.21,3,0.82]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",19,8,0,5,0.63,0.49,0.67,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",20,6,0,5,0.7,0.2,0.26,3,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",20,7.5,0,10,0.62,0.48,0.52,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",20,9.5,0,5,0.54,0.51,0.84,1,0.84]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",20,10,0,5,0.53,0.52,0.85,1,0.84]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",21,8,0,5,0.56999999999999995,0.43,0.52,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",21,9,0,10,0.53,0.49,0.72,1,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",22,6.5,0,5,0.61,0.2,0.23,3,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",22,8.5,0,15,0.52,0.49,0.56999999999999995,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",22,9.5,0,5,0.49,0.5,0.71,1,0.84]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",23,6.5,0,10,0.57999999999999996,0.25,0.24,3,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",23,8.5,0,5,0.5,0.41,0.46,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",24,6,0,15,0.56999999999999995,0.22,0.2,3,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",24,7,0,5,0.54,0.2,0.21,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",24,8.5,0,10,0.48,0.44,0.45,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",25,7,0,10,0.51,0.24,0.22,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",25,7.5,0,15,0.49,0.35,0.31,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",25,10,0,10,0.42,0.5,0.63,1,0.84]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,7.5,0,0,0.48,0.14000000000000001,0.17,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,9,0,10,0.43,0.41,0.42,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,9.5,0,15,0.41,0.5,0.5,1,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",27,7.5,0,10,0.46,0.24,0.21,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",27,9.5,0,0,0.4,0.28999999999999998,0.32,1,0.84]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,6,0,10,0.49,0.1,0.12,4,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,8.5,0,5,0.41,0.24,0.23,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",29,6,0,15,0.47,0.11,0.12,4,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",29,6.5,0,0,0.47,0.06,0.08,3,0.82]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",29,9,0,15,0.38,0.36,0.33,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",30,6,0,5,0.46,7.0000000000000007E-2,0.08,4,0.82]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",30,8,0,15,0.4,0.24,0.21,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",30,10,0,10,0.35,0.37,0.37,1,0.84]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",31,6.5,0,15,0.43,0.1,0.12,3,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",31,7.5,0,5,0.4,0.1,0.13,3,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",31,9.5,0,15,0.35,0.33,0.31,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",32,7,0,10,0.4,0.09,0.13,3,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",32,8,0,15,0.37,0.18,0.19,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",33,6.5,0,15,0.4,0.09,0.09,4,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",33,7,0,15,0.39,0.1,0.12,3,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",33,9,0,10,0.34,0.19,0.21,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",34,7.5,0,0,0.37,0.08,0.08,3,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",34,8,0,15,0.35,0.16,0.16,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",35,6,0,10,0.4,7.0000000000000007E-2,0.05,4,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",35,7,0,0,0.37,0.06,0.06,3,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",35,8.5,0,5,0.33,0.12,0.14000000000000001,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",35,10,0,0,0.3,0.15,0.18,2,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",36,7.5,0,10,0.34,0.1,0.1,3,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",36,10,0,5,0.28999999999999998,0.17,0.19,2,0.84]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,7,0,15,0.34,0.1,0.08,3,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,8.5,0,5,0.31,0.11,0.12,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,9.5,0,10,0.28999999999999998,0.16,0.19,2,0.84]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,7.5,0,5,0.33,0.08,7.0000000000000007E-2,3,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,9,0,15,0.28999999999999998,0.15,0.16,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,6,0,5,0.36,0.05,0.04,5,0.82]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,8.5,0,0,0.3,0.09,0.08,2,0.84]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,9,0,5,0.28999999999999998,0.11,0.13,2,0.84]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,6,0,15,0.34,7.0000000000000007E-2,0.03,5,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,9,0,10,0.28000000000000003,0.13,0.13,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,6,0,0,0.34,0.04,0.02,4,0.82]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,6.5,0,5,0.33,0.05,0.04,4,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,8,0,15,0.28999999999999998,0.11,0.09,3,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,6.5,0,10,0.32,0.06,0.04,4,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,7.5,0,0,0.3,0.06,0.05,3,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,9.5,0,10,0.26,0.13,0.13,2,0.84]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,7,0,5,0.3,0.06,0.04,4,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,8,0,10,0.28000000000000003,0.08,7.0000000000000007E-2,3,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,9.5,0,0,0.25,0.09,0.09,2,0.84]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,7,0,10,0.28999999999999998,7.0000000000000007E-2,0.04,4,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,9,0,5,0.26,0.09,0.08,2,0.84]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,10,0,10,0.24,0.13,0.14000000000000001,2,0.84]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,8.5,0,10,0.26,0.09,7.0000000000000007E-2,3,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,10,0,15,0.23,0.15,0.14000000000000001,2,0.84]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,6,0,5,0.3,0.04,0.02,5,0.82]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,8.5,0,15,0.25,0.1,7.0000000000000007E-2,3,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,10,0,10,0.23,0.13,0.11,2,0.84]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,7.5,0,15,0.26,0.08,0.04,3,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,9.5,0,15,0.23,0.12,0.1,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,6,0,15,0.28999999999999998,0.05,0.02,6,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,7.5,0,10,0.26,0.06,0.04,4,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,9,0,15,0.23,0.11,0.08,2,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,6.5,0,15,0.27,0.06,0.02,5,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,7.5,0,15,0.25,7.0000000000000007E-2,0.04,4,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,6.5,0,0,0.27,0.03,0.02,4,0.82]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,8,0,0,0.24,0.05,0.03,3,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,8.5,0,15,0.23,0.08,0.05,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",22,9.5,0,15,1.1399999999999999,0.73,0.54,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",21,9.5,0,15,1.19,0.78,0.6,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",20,9,0,10,1.29,0.78,0.61,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",19,8.5,0,15,1.4,0.79,0.62,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",19,9.5,0,10,1.32,0.8,0.7,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",18,8,0,10,1.53,0.75,0.61,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",17,7,0,10,1.73,0.67,0.53,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",17,9,0,0,1.52,0.8,0.74,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",16,7,0,5,1.84,0.68,0.57999999999999996,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",16,8,0,10,1.72,0.77,0.73,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",16,9.5,0,0,1.57,0.79,0.73,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",15,7.5,0,0,1.9,0.77,0.72,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",15,9,0,15,1.72,0.79,0.7,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",14,6,0,0,2.27,0.62,0.51,4,0.82]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",14,7,0,10,2.1,0.73,0.73,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",14,9,0,0,1.85,0.79,0.72,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",13,6,0,15,2.42,0.71,0.67,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",13,9,0,5,1.99,0.79,0.71,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",12,6,0,0,2.65,0.73,0.71,4,0.82]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",12,7.5,0,5,2.37,0.75,0.73,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",12,8,0,15,2.29,0.78,0.73,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",11,6.5,0,5,2.78,0.7,0.73,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",11,8,0,0,2.5099999999999998,0.77,0.74,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",11,9.5,0,5,2.2799999999999998,0.86,0.85,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",10,7,0,5,2.95,0.74,0.74,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",10,8,0,5,2.76,0.81,0.8,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",10,9.5,0,0,2.5099999999999998,0.86,0.91,2,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",16,6,0,15,1.97,0.62,0.45,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",18,7,0,0,1.64,0.59,0.42,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",19,6.5,0,0,1.61,0.53,0.32,4,0.82]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",19,7.5,0,15,1.49,0.68,0.49,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",21,6.5,0,10,1.45,0.52,0.28000000000000003,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",21,7.5,0,5,1.36,0.57999999999999996,0.37,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",22,6.5,0,10,1.39,0.51,0.27,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",22,8,0,10,1.25,0.61,0.39,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",23,6,0,10,1.38,0.45,0.22,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",23,7,0,5,1.28,0.51,0.28000000000000003,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",23,9.5,0,10,1.0900000000000001,0.69,0.49,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",24,7,0,10,1.23,0.5,0.27,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",24,8.5,0,10,1.1100000000000001,0.56999999999999995,0.37,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",25,7,0,0,1.18,0.44,0.23,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",25,7,0,15,1.17,0.48,0.26,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",25,8.5,0,15,1.07,0.53,0.33,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,7.5,0,0,1.1000000000000001,0.46,0.25,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,8.5,0,0,1.03,0.54,0.31,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",27,6.5,0,0,1.1399999999999999,0.33,0.16,4,0.82]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",27,8,0,5,1.02,0.5,0.28000000000000003,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",27,9.5,0,0,0.93,0.56999999999999995,0.35,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,6,0,0,1.1299999999999999,0.26,0.12,4,0.82]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,8,0,0,0.99,0.46,0.25,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,9.5,0,5,0.9,0.54,0.33,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",29,6.5,0,0,1.06,0.28000000000000003,0.14000000000000001,4,0.82]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",29,9,0,10,0.89,0.5,0.3,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",29,9.5,0,15,0.87,0.49,0.31,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",30,7.5,0,5,0.95,0.38,0.19,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",30,9,0,0,0.86,0.49,0.27,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",31,6,0,5,1.02,0.25,0.11,5,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",31,8.5,0,5,0.86,0.46,0.24,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",31,9.5,0,5,0.81,0.49,0.28000000000000003,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",32,6.5,0,0,0.96,0.25,0.12,4,0.82]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",32,8,0,5,0.86,0.4,0.2,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",33,6,0,5,0.96,0.23,0.1,5,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",33,8,0,10,0.84,0.39,0.2,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",33,9.5,0,10,0.76,0.47,0.27,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",34,6.5,0,10,0.9,0.28000000000000003,0.12,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",34,7.5,0,5,0.84,0.33,0.16,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",34,10,0,10,0.72,0.47,0.27,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",35,7,0,10,0.84,0.3,0.13,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",35,8.5,0,10,0.76,0.41,0.21,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",35,9.5,0,5,0.72,0.45,0.23,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",36,7,0,10,0.82,0.28000000000000003,0.12,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",36,8.5,0,10,0.74,0.39,0.2,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",36,10,0,10,0.68,0.45,0.25,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,8,0,15,0.74,0.33,0.16,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,10,0,15,0.66,0.45,0.23,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,6,0,10,0.83,0.19,0.08,5,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,9,0,15,0.68,0.39,0.19,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,10,0,15,0.64,0.43,0.22,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,7.5,0,15,0.73,0.28999999999999998,0.13,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,9.5,0,0,0.65,0.35,0.18,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,6,0,15,0.79,0.19,7.0000000000000007E-2,5,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,7,0,15,0.73,0.24,0.1,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,9,0,15,0.65,0.34,0.16,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,7,0,0,0.72,0.18,0.08,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,8,0,15,0.67,0.27,0.13,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,6.5,0,5,0.73,0.17,7.0000000000000007E-2,5,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,6.5,0,15,0.72,0.2,0.08,5,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,9,0,0,0.62,0.26,0.13,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,7,0,0,0.69,0.17,0.08,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,8,0,5,0.64,0.21,0.11,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,10,0,0,0.56999999999999995,0.31,0.15,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,7.5,0,10,0.65,0.2,0.09,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,9,0,0,0.59,0.24,0.12,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,10,0,5,0.56000000000000005,0.31,0.15,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,7.5,0,0,0.64,0.18,0.08,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,9.5,0,10,0.56000000000000005,0.28000000000000003,0.14000000000000001,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,6,0,0,0.69,0.1,0.04,5,0.82]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,8.5,0,15,0.57999999999999996,0.24,0.12,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,9,0,0,0.56999999999999995,0.23,0.12,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,6.5,0,10,0.65,0.15,0.06,5,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,8.5,0,5,0.56999999999999995,0.21,0.11,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,10,0,5,0.52,0.28000000000000003,0.14000000000000001,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,8,0,10,0.57999999999999996,0.2,0.09,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,8.5,0,5,0.56000000000000005,0.21,0.1,3,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,6,0,5,0.65,0.09,0.04,5,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,7.5,0,5,0.57999999999999996,0.16,7.0000000000000007E-2,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,10,0,10,0.5,0.28000000000000003,0.14000000000000001,3,0.84]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,7.5,0,10,0.56999999999999995,0.16,7.0000000000000007E-2,4,0.83]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL120 120W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,8,0,5,0.55000000000000004,0.17,0.08,4,0.83]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",21,8,0,5,0.78,0.42,0.53,2,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",20,7.5,0,10,0.85,0.44,0.53,2,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",20,9.5,0,15,0.75,0.49,0.85,2,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",19,9,0,15,0.82,0.47,0.83,2,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",18,7,0,15,0.98,0.43,0.57999999999999996,2,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",18,8,0,15,0.92,0.46,0.77,2,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",18,10,0,15,0.81,0.49,0.8,1,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",17,8.5,0,15,0.94,0.45,0.78,2,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",17,9.5,0,10,0.88,0.47,0.8,1,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",16,8.5,0,5,1,0.44,0.75,2,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",15,6.5,0,5,1.22,0.41,0.71,2,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",15,7,0,5,1.17,0.43,0.79,2,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",15,10,0,5,0.97,0.48,0.81,1,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",14,7,0,10,1.26,0.41,0.76,2,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",14,9,0,5,1.1000000000000001,0.45,0.78,1,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",14,9.5,0,5,1.07,0.48,0.81,1,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",13,8,0,10,1.27,0.46,0.78,2,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",13,9,0,15,1.19,0.51,0.83,1,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",12,7,0,15,1.47,0.45,0.8,2,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",12,9.5,0,5,1.25,0.52,0.89,1,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",12,10,0,15,1.22,0.52,0.93,1,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",11,8,0,5,1.49,0.48,0.84,2,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",11,10,0,0,1.32,0.53,0.94,1,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",10,8,0,0,1.64,0.48,0.86,1,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",10,10,0,15,1.46,0.53,0.93,1,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",12,6,0,15,1.58,0.38,0.81,3,0.87]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",15,6,0,10,1.26,0.39,0.62,3,0.87]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",16,6,0,10,1.19,0.38,0.53,3,0.87]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",19,6,0,0,0.99,0.14000000000000001,0.23,3,0.87]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",20,6,0,15,0.95,0.34,0.32,3,0.87]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",20,10,0,15,0.73,0.5,0.83,1,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",21,9,0,5,0.74,0.45,0.7,2,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",21,9.5,0,10,0.72,0.48,0.8,2,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",22,7,0,0,0.8,0.17,0.24,3,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",22,8.5,0,0,0.72,0.36,0.47,2,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",23,6,0,15,0.83,0.24,0.25,4,0.87]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",23,8.5,0,5,0.69,0.39,0.48,2,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",24,6,0,0,0.79,0.08,0.11,4,0.87]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",24,7.5,0,5,0.71,0.24,0.27,3,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",24,8,0,15,0.69,0.42,0.4,2,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",24,10,0,10,0.61,0.48,0.68,2,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",25,8,0,10,0.66,0.33,0.35,2,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",25,9.5,0,15,0.6,0.47,0.56000000000000005,2,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,7,0,10,0.68,0.2,0.21,3,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,7.5,0,10,0.66,0.25,0.24,3,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,10,0,10,0.56000000000000005,0.46,0.57999999999999996,2,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",27,6.5,0,15,0.68,0.17,0.19,4,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",27,8.5,0,10,0.59,0.31,0.33,2,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,6.5,0,0,0.65,7.0000000000000007E-2,0.1,4,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,7,0,10,0.63,0.15,0.18,3,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,8.5,0,15,0.56999999999999995,0.33,0.32,2,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",29,6,0,10,0.65,0.09,0.12,5,0.87]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",29,8.5,0,0,0.55000000000000004,0.16,0.19,2,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",29,9,0,10,0.54,0.28999999999999998,0.31,2,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",30,6,0,15,0.63,0.1,0.11,5,0.87]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",30,9,0,15,0.52,0.31,0.31,2,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",30,10,0,0,0.48,0.24,0.28999999999999998,2,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",31,7.5,0,15,0.55000000000000004,0.15,0.19,3,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",31,9.5,0,5,0.48,0.21,0.26,2,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",32,6.5,0,15,0.56999999999999995,0.09,0.11,4,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",32,7.5,0,0,0.53,0.09,0.11,3,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",32,9.5,0,15,0.47,0.28000000000000003,0.28999999999999998,2,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",33,7,0,5,0.53,0.08,0.1,4,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",33,8,0,15,0.5,0.15,0.19,3,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",34,6,0,10,0.56000000000000005,0.08,7.0000000000000007E-2,5,0.87]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",34,6.5,0,15,0.54,0.09,0.09,4,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",34,8.5,0,5,0.47,0.13,0.16,3,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",35,7,0,0,0.5,7.0000000000000007E-2,7.0000000000000007E-2,4,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",35,8,0,10,0.47,0.13,0.15,3,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",36,6,0,0,0.52,0.05,0.04,5,0.87]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",36,7.5,0,15,0.48,0.11,0.12,3,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",36,9,0,0,0.43,0.11,0.14000000000000001,2,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",36,9.5,0,10,0.42,0.18,0.2,2,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,7.5,0,0,0.46,0.08,0.08,3,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,9,0,15,0.42,0.16,0.19,2,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,6,0,0,0.5,0.05,0.04,5,0.87]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,9,0,0,0.41,0.11,0.12,2,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,9.5,0,0,0.39,0.12,0.15,2,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,6.5,0,15,0.47,0.09,0.06,5,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,8,0,0,0.42,0.08,0.08,3,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,6,0,0,0.47,0.04,0.03,5,0.87]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,8,0,5,0.41,0.09,0.09,3,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,10,0,5,0.37,0.14000000000000001,0.17,2,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,6.5,0,5,0.44,0.06,0.05,5,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,8,0,0,0.4,0.08,7.0000000000000007E-2,3,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,10,0,5,0.36,0.14000000000000001,0.16,2,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,7.5,0,5,0.41,0.08,0.06,4,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,9.5,0,0,0.36,0.11,0.11,2,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,6,0,10,0.44,0.06,0.03,6,0.87]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,7,0,15,0.41,0.08,0.05,4,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,9.5,0,10,0.35,0.14000000000000001,0.13,2,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,7,0,0,0.4,0.05,0.04,4,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,8,0,10,0.38,0.09,7.0000000000000007E-2,3,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,6,0,5,0.42,0.04,0.03,6,0.87]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,6.5,0,10,0.41,0.06,0.03,5,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,8.5,0,0,0.35,7.0000000000000007E-2,0.06,3,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,9.5,0,10,0.34,0.12,0.11,3,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,8,0,5,0.36,7.0000000000000007E-2,0.06,4,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,8.5,0,10,0.35,0.09,7.0000000000000007E-2,3,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,6,0,0,0.4,0.03,0.02,6,0.87]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,8.5,0,15,0.34,0.1,7.0000000000000007E-2,3,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,9.5,0,5,0.32,0.1,0.09,3,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,7,0,15,0.37,7.0000000000000007E-2,0.04,5,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,9,0,10,0.32,0.09,7.0000000000000007E-2,3,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,10,0,15,0.31,0.14000000000000001,0.11,2,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,7,0,5,0.36,0.05,0.03,5,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,9,0,15,0.32,0.1,0.08,3,0.85]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,6.5,0,10,0.37,0.05,0.02,6,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,7.5,0,15,0.34,0.08,0.04,4,0.86]
[12,"UNILATERAL","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,9,0,5,0.31,0.08,0.06,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",23,10,0,15,1.49,0.72,0.55000000000000004,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",21,9.5,0,10,1.67,0.78,0.59,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",19,8,0,5,2,0.66,0.52,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",19,9.5,0,0,1.81,0.8,0.67,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",18,8.5,0,10,2.06,0.8,0.66,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",18,9,0,0,1.97,0.79,0.68,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",17,8,0,15,2.25,0.78,0.68,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",17,9.5,0,10,2.06,0.78,0.72,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",16,7.5,0,5,2.4500000000000002,0.73,0.66,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",16,9.5,0,5,2.17,0.78,0.7,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",15,6.5,0,0,2.76,0.61,0.52,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",15,7.5,0,15,2.64,0.74,0.72,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",14,6.5,0,5,2.98,0.7,0.65,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",14,7.5,0,0,2.77,0.76,0.77,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",14,8.5,0,0,2.61,0.76,0.72,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",13,7,0,5,3.11,0.72,0.75,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",13,8.5,0,5,2.83,0.76,0.71,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",13,9,0,0,2.72,0.77,0.7,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",12,7,0,5,3.37,0.71,0.72,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",12,8.5,0,5,3.07,0.78,0.73,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",12,10,0,5,2.82,0.84,0.82,2,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",11,8,0,10,3.47,0.78,0.76,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",11,9,0,5,3.25,0.83,0.81,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",10,6,0,5,4.32,0.66,0.73,4,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",10,8,0,0,3.76,0.78,0.78,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Adecuado/a",10,10,0,10,3.4,0.84,0.91,2,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",17,6.5,0,0,2.44,0.55000000000000004,0.39,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",18,6.5,0,0,2.2999999999999998,0.53,0.35,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",19,6,0,5,2.2799999999999998,0.48,0.26,4,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",19,7.5,0,15,2.08,0.66,0.48,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",20,7.5,0,5,1.96,0.59,0.41,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",21,6,0,10,2.0699999999999998,0.47,0.24,5,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",22,6,0,10,1.97,0.47,0.22,5,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",22,7.5,0,15,1.8,0.53,0.33,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",22,8.5,0,5,1.67,0.62,0.42,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",23,7.5,0,15,1.72,0.5,0.3,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",23,9,0,10,1.57,0.64,0.44,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",24,6.5,0,15,1.76,0.46,0.23,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",24,8.5,0,15,1.55,0.54,0.36,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",24,9.5,0,15,1.46,0.64,0.46,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",25,6.5,0,10,1.68,0.43,0.21,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",25,8,0,15,1.53,0.5,0.28999999999999998,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,6,0,15,1.68,0.37,0.18,5,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,7,0,15,1.57,0.45,0.24,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,8.5,0,10,1.43,0.5,0.3,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",26,10,0,15,1.32,0.61,0.42,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",27,8,0,15,1.42,0.48,0.27,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,6,0,0,1.53,0.27,0.12,5,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,7.5,0,0,1.39,0.41,0.21,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,9,0,0,1.27,0.5,0.3,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",28,9.5,0,15,1.26,0.49,0.32,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",29,8,0,0,1.3,0.43,0.22,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",29,9.5,0,0,1.19,0.51,0.3,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",30,6.5,0,0,1.38,0.27,0.12,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",30,9,0,5,1.2,0.49,0.27,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",30,9.5,0,0,1.1499999999999999,0.5,0.3,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",31,6.5,0,0,1.34,0.27,0.12,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",31,9.5,0,5,1.1200000000000001,0.48,0.27,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",32,6,0,5,1.35,0.24,0.1,5,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",32,7,0,0,1.25,0.28999999999999998,0.13,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",32,10,0,10,1.07,0.47,0.28000000000000003,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",33,7,0,5,1.23,0.28999999999999998,0.13,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",33,8,0,5,1.1499999999999999,0.37,0.18,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",33,10,0,5,1.03,0.47,0.27,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",34,7,0,10,1.2,0.31,0.14000000000000001,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",34,8.5,0,5,1.0900000000000001,0.4,0.21,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",35,6.5,0,15,1.2,0.27,0.11,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",35,7,0,5,1.1599999999999999,0.28000000000000003,0.12,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",35,9,0,10,1.03,0.42,0.22,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",36,6,0,5,1.2,0.21,0.09,5,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",36,8.5,0,15,1.03,0.39,0.2,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,6,0,10,1.17,0.21,0.09,5,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,6.5,0,0,1.1200000000000001,0.19,0.09,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,6.5,0,5,1.1299999999999999,0.22,0.09,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,6.5,0,10,1.1399999999999999,0.24,0.1,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,6.5,0,15,1.1399999999999999,0.26,0.1,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,7,0,0,1.0900000000000001,0.22,0.1,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,7,0,5,1.0900000000000001,0.24,0.11,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,7,0,10,1.1000000000000001,0.27,0.11,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,7,0,15,1.1100000000000001,0.28000000000000003,0.12,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,7.5,0,0,1.05,0.24,0.11,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,7.5,0,5,1.06,0.27,0.12,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,7.5,0,10,1.07,0.28999999999999998,0.13,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,7.5,0,15,1.07,0.3,0.14000000000000001,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,8,0,0,1.02,0.27,0.13,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,8,0,5,1.03,0.3,0.14000000000000001,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,8,0,10,1.03,0.32,0.15,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,8,0,15,1.04,0.33,0.16,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,8.5,0,0,0.99,0.31,0.15,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,8.5,0,5,1,0.33,0.16,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,8.5,0,10,1,0.35,0.17,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,8.5,0,15,1.01,0.36,0.18,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,9,0,0,0.96,0.35,0.17,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,9,0,5,0.97,0.37,0.18,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,9,0,10,0.98,0.38,0.19,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,9,0,15,0.98,0.39,0.19,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,9.5,0,0,0.93,0.38,0.18,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,9.5,0,5,0.94,0.4,0.2,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,9.5,0,10,0.95,0.41,0.2,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,9.5,0,15,0.95,0.41,0.21,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,10,0,0,0.91,0.41,0.21,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,10,0,5,0.92,0.43,0.22,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,10,0,10,0.92,0.43,0.22,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",37,10,0,15,0.93,0.43,0.23,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,6,0,0,1.1299999999999999,0.17,7.0000000000000007E-2,5,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,6,0,5,1.1399999999999999,0.18,7.0000000000000007E-2,5,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,6,0,10,1.1399999999999999,0.2,0.08,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,6,0,15,1.1499999999999999,0.22,0.09,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,6.5,0,0,1.0900000000000001,0.19,0.08,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,6.5,0,5,1.1000000000000001,0.21,0.09,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,6.5,0,10,1.1100000000000001,0.23,0.09,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,6.5,0,15,1.1100000000000001,0.25,0.1,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,7,0,0,1.06,0.21,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,7,0,5,1.07,0.23,0.1,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,7,0,10,1.07,0.25,0.11,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,7,0,15,1.08,0.27,0.12,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,7.5,0,0,1.02,0.23,0.11,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,7.5,0,5,1.03,0.26,0.12,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,7.5,0,10,1.04,0.28000000000000003,0.12,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,7.5,0,15,1.04,0.28999999999999998,0.13,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,8,0,0,0.99,0.26,0.12,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,8,0,5,1,0.28999999999999998,0.14000000000000001,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,8,0,10,1.01,0.3,0.15,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,8,0,15,1.01,0.32,0.15,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,8.5,0,0,0.96,0.28999999999999998,0.15,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,8.5,0,5,0.97,0.32,0.16,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,8.5,0,10,0.98,0.34,0.17,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,8.5,0,15,0.98,0.34,0.17,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,9,0,0,0.94,0.33,0.16,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,9,0,5,0.94,0.36,0.17,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,9,0,10,0.95,0.37,0.18,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,9,0,15,0.95,0.38,0.19,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,9.5,0,0,0.91,0.36,0.18,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,9.5,0,5,0.92,0.38,0.19,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,9.5,0,10,0.92,0.39,0.19,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,9.5,0,15,0.93,0.4,0.2,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,10,0,0,0.89,0.39,0.2,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,10,0,5,0.89,0.41,0.21,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,10,0,10,0.9,0.42,0.21,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",38,10,0,15,0.9,0.42,0.22,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,6,0,0,1.1000000000000001,0.16,0.06,5,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,6,0,5,1.1100000000000001,0.17,7.0000000000000007E-2,5,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,6,0,10,1.1100000000000001,0.19,7.0000000000000007E-2,5,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,6,0,15,1.1200000000000001,0.2,0.08,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,6.5,0,0,1.06,0.18,0.08,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,6.5,0,5,1.07,0.2,0.09,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,6.5,0,10,1.08,0.22,0.09,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,6.5,0,15,1.08,0.24,0.1,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,7,0,0,1.03,0.2,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,7,0,5,1.04,0.22,0.1,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,7,0,10,1.04,0.24,0.1,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,7,0,15,1.05,0.26,0.11,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,7.5,0,0,1,0.22,0.1,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,7.5,0,5,1.01,0.25,0.11,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,7.5,0,10,1.01,0.27,0.12,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,7.5,0,15,1.02,0.28000000000000003,0.12,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,8,0,0,0.97,0.25,0.12,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,8,0,5,0.98,0.27,0.13,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,8,0,10,0.98,0.28999999999999998,0.14000000000000001,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,8,0,15,0.99,0.31,0.14000000000000001,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,8.5,0,0,0.94,0.28000000000000003,0.14000000000000001,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,8.5,0,5,0.94,0.31,0.15,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,8.5,0,10,0.95,0.32,0.16,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,8.5,0,15,0.95,0.33,0.16,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,9,0,0,0.91,0.32,0.16,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,9,0,5,0.92,0.34,0.17,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,9,0,10,0.93,0.36,0.17,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,9,0,15,0.93,0.37,0.18,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,9.5,0,0,0.89,0.35,0.17,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,9.5,0,5,0.89,0.37,0.18,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,9.5,0,10,0.9,0.38,0.19,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,9.5,0,15,0.9,0.39,0.19,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,10,0,0,0.86,0.38,0.19,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,10,0,5,0.87,0.39,0.2,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,10,0,10,0.88,0.4,0.2,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",39,10,0,15,0.88,0.41,0.21,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,6,0,0,1.07,0.15,0.06,5,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,6,0,5,1.08,0.17,0.06,5,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,6,0,10,1.08,0.18,7.0000000000000007E-2,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,6,0,15,1.0900000000000001,0.19,7.0000000000000007E-2,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,6.5,0,0,1.03,0.18,0.08,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,6.5,0,5,1.04,0.19,0.08,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,6.5,0,10,1.05,0.2,0.08,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,6.5,0,15,1.05,0.22,0.09,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,7,0,0,1,0.2,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,7,0,5,1.01,0.21,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,7,0,10,1.02,0.22,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,7,0,15,1.02,0.24,0.1,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,7.5,0,0,0.97,0.21,0.1,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,7.5,0,5,0.98,0.23,0.1,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,7.5,0,10,0.99,0.24,0.11,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,7.5,0,15,0.99,0.26,0.11,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,8,0,0,0.94,0.23,0.11,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,8,0,5,0.95,0.25,0.12,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,8,0,10,0.96,0.27,0.13,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,8,0,15,0.96,0.28000000000000003,0.13,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,8.5,0,0,0.91,0.26,0.13,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,8.5,0,5,0.92,0.28000000000000003,0.13,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,8.5,0,10,0.93,0.3,0.14000000000000001,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,8.5,0,15,0.93,0.31,0.15,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,9,0,0,0.89,0.28000000000000003,0.13,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,9,0,5,0.9,0.31,0.14000000000000001,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,9,0,10,0.9,0.32,0.15,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,9,0,15,0.91,0.33,0.16,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,9.5,0,0,0.86,0.32,0.15,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,9.5,0,5,0.87,0.34,0.16,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,9.5,0,10,0.88,0.36,0.17,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,9.5,0,15,0.88,0.37,0.18,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,10,0,0,0.84,0.35,0.17,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,10,0,5,0.85,0.38,0.18,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,10,0,10,0.85,0.39,0.19,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",40,10,0,15,0.86,0.39,0.2,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,6,0,0,1.05,0.15,0.06,5,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,6,0,5,1.05,0.16,0.06,5,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,6,0,10,1.06,0.17,0.06,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,6,0,15,1.06,0.18,7.0000000000000007E-2,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,6.5,0,0,1.01,0.18,7.0000000000000007E-2,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,6.5,0,5,1.02,0.18,0.08,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,6.5,0,10,1.02,0.2,0.08,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,6.5,0,15,1.03,0.21,0.08,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,7,0,0,0.98,0.19,0.08,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,7,0,5,0.99,0.2,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,7,0,10,0.99,0.22,0.09,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,7,0,15,1,0.23,0.09,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,7.5,0,0,0.95,0.2,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,7.5,0,5,0.96,0.22,0.1,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,7.5,0,10,0.96,0.23,0.1,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,7.5,0,15,0.97,0.25,0.11,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,8,0,0,0.92,0.22,0.1,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,8,0,5,0.93,0.24,0.11,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,8,0,10,0.93,0.26,0.12,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,8,0,15,0.94,0.27,0.13,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,8.5,0,0,0.89,0.24,0.12,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,8.5,0,5,0.9,0.26,0.13,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,8.5,0,10,0.91,0.28000000000000003,0.14000000000000001,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,8.5,0,15,0.91,0.3,0.15,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,9,0,0,0.87,0.27,0.13,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,9,0,5,0.88,0.28999999999999998,0.14000000000000001,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,9,0,10,0.88,0.31,0.15,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,9,0,15,0.89,0.32,0.15,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,9.5,0,0,0.84,0.3,0.14000000000000001,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,9.5,0,5,0.85,0.33,0.15,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,9.5,0,10,0.86,0.34,0.16,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,9.5,0,15,0.86,0.35,0.17,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,10,0,0,0.82,0.34,0.16,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,10,0,5,0.83,0.36,0.17,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,10,0,10,0.83,0.37,0.18,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",41,10,0,15,0.84,0.38,0.19,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,6,0,0,1.02,0.14000000000000001,0.05,5,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,6,0,5,1.03,0.15,0.05,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,6,0,10,1.03,0.16,0.06,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,6,0,15,1.04,0.17,0.06,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,6.5,0,0,0.99,0.17,7.0000000000000007E-2,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,6.5,0,5,0.99,0.18,7.0000000000000007E-2,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,6.5,0,10,1,0.19,0.08,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,6.5,0,15,1,0.2,0.08,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,7,0,0,0.95,0.19,0.08,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,7,0,5,0.96,0.19,0.08,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,7,0,10,0.97,0.21,0.09,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,7,0,15,0.97,0.22,0.09,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,7.5,0,0,0.93,0.2,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,7.5,0,5,0.94,0.21,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,7.5,0,10,0.94,0.23,0.1,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,7.5,0,15,0.95,0.24,0.1,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,8,0,0,0.9,0.21,0.1,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,8,0,5,0.91,0.23,0.11,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,8,0,10,0.91,0.25,0.11,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,8,0,15,0.92,0.26,0.12,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,8.5,0,0,0.87,0.23,0.12,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,8.5,0,5,0.88,0.25,0.12,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,8.5,0,10,0.88,0.27,0.13,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,8.5,0,15,0.89,0.28000000000000003,0.14000000000000001,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,9,0,0,0.85,0.26,0.13,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,9,0,5,0.86,0.28000000000000003,0.13,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,9,0,10,0.86,0.3,0.14000000000000001,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,9,0,15,0.86,0.31,0.15,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,9.5,0,0,0.82,0.28999999999999998,0.14000000000000001,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,9.5,0,5,0.83,0.31,0.15,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,9.5,0,10,0.84,0.32,0.15,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,9.5,0,15,0.84,0.33,0.16,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,10,0,0,0.8,0.32,0.15,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,10,0,5,0.81,0.34,0.17,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,10,0,10,0.81,0.36,0.17,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",42,10,0,15,0.82,0.36,0.18,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,6,0,0,1,0.13,0.05,5,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,6,0,5,1,0.14000000000000001,0.05,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,6,0,10,1.01,0.16,0.06,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,6,0,15,1.01,0.16,0.06,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,6.5,0,0,0.96,0.15,7.0000000000000007E-2,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,6.5,0,5,0.97,0.17,7.0000000000000007E-2,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,6.5,0,10,0.98,0.18,7.0000000000000007E-2,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,6.5,0,15,0.98,0.18,0.08,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,7,0,0,0.93,0.18,0.08,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,7,0,5,0.94,0.19,0.08,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,7,0,10,0.95,0.19,0.08,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,7,0,15,0.95,0.2,0.09,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,7.5,0,0,0.9,0.2,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,7.5,0,5,0.91,0.2,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,7.5,0,10,0.92,0.21,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,7.5,0,15,0.92,0.22,0.1,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,8,0,0,0.88,0.21,0.1,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,8,0,5,0.88,0.22,0.11,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,8,0,10,0.89,0.23,0.11,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,8,0,15,0.89,0.24,0.11,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,8.5,0,0,0.85,0.23,0.11,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,8.5,0,5,0.86,0.24,0.12,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,8.5,0,10,0.86,0.25,0.12,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,8.5,0,15,0.87,0.26,0.13,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,9,0,0,0.83,0.25,0.12,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,9,0,5,0.84,0.26,0.13,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,9,0,10,0.84,0.27,0.13,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,9,0,15,0.84,0.28999999999999998,0.14000000000000001,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,9.5,0,0,0.8,0.27,0.13,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,9.5,0,5,0.81,0.28999999999999998,0.14000000000000001,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,9.5,0,10,0.82,0.3,0.15,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,9.5,0,15,0.82,0.31,0.15,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,10,0,0,0.78,0.3,0.15,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,10,0,5,0.79,0.32,0.16,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,10,0,10,0.8,0.33,0.17,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",43,10,0,15,0.8,0.34,0.17,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,6,0,0,0.98,0.12,0.04,5,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,6,0,5,0.98,0.14000000000000001,0.05,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,6,0,10,0.99,0.15,0.06,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,6,0,15,0.99,0.15,0.06,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,6.5,0,0,0.94,0.14000000000000001,0.06,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,6.5,0,5,0.95,0.16,7.0000000000000007E-2,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,6.5,0,10,0.96,0.17,7.0000000000000007E-2,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,6.5,0,15,0.96,0.17,7.0000000000000007E-2,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,7,0,0,0.91,0.17,7.0000000000000007E-2,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,7,0,5,0.92,0.18,0.08,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,7,0,10,0.93,0.19,0.08,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,7,0,15,0.93,0.2,0.08,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,7.5,0,0,0.88,0.19,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,7.5,0,5,0.89,0.2,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,7.5,0,10,0.9,0.21,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,7.5,0,15,0.9,0.22,0.1,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,8,0,0,0.86,0.2,0.1,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,8,0,5,0.86,0.21,0.1,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,8,0,10,0.87,0.22,0.1,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,8,0,15,0.87,0.23,0.11,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,8.5,0,0,0.83,0.22,0.11,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,8.5,0,5,0.84,0.23,0.12,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,8.5,0,10,0.84,0.24,0.12,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,8.5,0,15,0.85,0.25,0.13,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,9,0,0,0.81,0.24,0.12,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,9,0,5,0.82,0.25,0.12,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,9,0,10,0.82,0.26,0.13,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,9,0,15,0.82,0.28000000000000003,0.13,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,9.5,0,0,0.79,0.26,0.13,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,9.5,0,5,0.79,0.28000000000000003,0.13,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,9.5,0,10,0.8,0.28999999999999998,0.14000000000000001,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,9.5,0,15,0.8,0.3,0.14000000000000001,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,10,0,0,0.77,0.28999999999999998,0.14000000000000001,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,10,0,5,0.77,0.31,0.15,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,10,0,10,0.78,0.32,0.16,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",44,10,0,15,0.78,0.32,0.16,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,6,0,0,0.95,0.12,0.04,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,6,0,5,0.96,0.13,0.04,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,6,0,10,0.97,0.15,0.05,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,6,0,15,0.97,0.15,0.06,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,6.5,0,0,0.92,0.14000000000000001,0.06,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,6.5,0,5,0.93,0.15,0.06,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,6.5,0,10,0.94,0.16,7.0000000000000007E-2,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,6.5,0,15,0.94,0.17,7.0000000000000007E-2,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,7,0,0,0.89,0.16,7.0000000000000007E-2,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,7,0,5,0.9,0.18,0.08,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,7,0,10,0.91,0.18,0.08,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,7,0,15,0.91,0.19,0.08,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,7.5,0,0,0.87,0.19,0.08,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,7.5,0,5,0.87,0.19,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,7.5,0,10,0.88,0.2,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,7.5,0,15,0.88,0.21,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,8,0,0,0.84,0.2,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,8,0,5,0.85,0.21,0.1,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,8,0,10,0.85,0.22,0.1,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,8,0,15,0.85,0.23,0.1,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,8.5,0,0,0.81,0.21,0.11,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,8.5,0,5,0.82,0.22,0.11,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,8.5,0,10,0.82,0.23,0.12,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,8.5,0,15,0.83,0.24,0.12,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,9,0,0,0.79,0.23,0.12,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,9,0,5,0.8,0.24,0.12,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,9,0,10,0.8,0.25,0.13,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,9,0,15,0.81,0.26,0.13,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,9.5,0,0,0.77,0.25,0.12,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,9.5,0,5,0.78,0.26,0.13,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,9.5,0,10,0.78,0.28000000000000003,0.13,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,9.5,0,15,0.78,0.28999999999999998,0.14000000000000001,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,10,0,0,0.75,0.27,0.13,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,10,0,5,0.76,0.28999999999999998,0.14000000000000001,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,10,0,10,0.76,0.3,0.15,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",45,10,0,15,0.76,0.31,0.15,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,6,0,0,0.93,0.11,0.04,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,6,0,5,0.94,0.12,0.04,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,6,0,10,0.94,0.13,0.05,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,6,0,15,0.95,0.14000000000000001,0.05,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,6.5,0,0,0.9,0.13,0.05,5,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,6.5,0,5,0.91,0.14000000000000001,0.06,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,6.5,0,10,0.91,0.16,0.06,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,6.5,0,15,0.92,0.17,0.06,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,7,0,0,0.87,0.15,7.0000000000000007E-2,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,7,0,5,0.88,0.16,7.0000000000000007E-2,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,7,0,10,0.89,0.18,0.08,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,7,0,15,0.89,0.19,0.08,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,7.5,0,0,0.85,0.17,0.08,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,7.5,0,5,0.85,0.19,0.08,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,7.5,0,10,0.86,0.2,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,7.5,0,15,0.86,0.2,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,8,0,0,0.82,0.19,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,8,0,5,0.83,0.21,0.1,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,8,0,10,0.83,0.21,0.1,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,8,0,15,0.84,0.22,0.1,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,8.5,0,0,0.8,0.22,0.11,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,8.5,0,5,0.8,0.22,0.11,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,8.5,0,10,0.81,0.23,0.11,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,8.5,0,15,0.81,0.24,0.11,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,9,0,0,0.77,0.23,0.11,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,9,0,5,0.78,0.24,0.11,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,9,0,10,0.79,0.25,0.12,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,9,0,15,0.79,0.26,0.12,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,9.5,0,0,0.75,0.25,0.12,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,9.5,0,5,0.76,0.26,0.12,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,9.5,0,10,0.76,0.27,0.13,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,9.5,0,15,0.77,0.28000000000000003,0.13,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,10,0,0,0.73,0.28000000000000003,0.13,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,10,0,5,0.74,0.28999999999999998,0.14000000000000001,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,10,0,10,0.74,0.3,0.14000000000000001,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",46,10,0,15,0.75,0.31,0.15,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,6,0,0,0.91,0.11,0.04,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,6,0,5,0.92,0.11,0.04,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,6,0,10,0.92,0.12,0.04,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,6,0,15,0.93,0.13,0.05,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,6.5,0,0,0.88,0.13,0.05,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,6.5,0,5,0.89,0.14000000000000001,0.05,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,6.5,0,10,0.89,0.15,0.06,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,6.5,0,15,0.9,0.16,0.06,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,7,0,0,0.85,0.15,0.06,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,7,0,5,0.86,0.16,7.0000000000000007E-2,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,7,0,10,0.87,0.18,7.0000000000000007E-2,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,7,0,15,0.87,0.19,0.08,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,7.5,0,0,0.83,0.17,7.0000000000000007E-2,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,7.5,0,5,0.84,0.18,0.08,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,7.5,0,10,0.84,0.19,0.08,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,7.5,0,15,0.85,0.2,0.08,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,8,0,0,0.8,0.19,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,8,0,5,0.81,0.2,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,8,0,10,0.81,0.21,0.1,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,8,0,15,0.82,0.21,0.1,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,8.5,0,0,0.78,0.21,0.1,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,8.5,0,5,0.79,0.22,0.11,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,8.5,0,10,0.79,0.22,0.11,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,8.5,0,15,0.79,0.23,0.11,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,9,0,0,0.76,0.23,0.11,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,9,0,5,0.76,0.23,0.11,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,9,0,10,0.77,0.24,0.12,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,9,0,15,0.77,0.25,0.12,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,9.5,0,0,0.74,0.24,0.12,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,9.5,0,5,0.74,0.25,0.12,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,9.5,0,10,0.75,0.26,0.12,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,9.5,0,15,0.75,0.27,0.13,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,10,0,0,0.72,0.26,0.13,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,10,0,5,0.72,0.28000000000000003,0.13,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,10,0,10,0.73,0.28999999999999998,0.14000000000000001,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",47,10,0,15,0.73,0.28999999999999998,0.14000000000000001,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,6,0,0,0.89,0.1,0.04,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,6,0,5,0.9,0.11,0.04,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,6,0,10,0.9,0.12,0.04,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,6,0,15,0.91,0.13,0.04,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,6.5,0,0,0.86,0.12,0.05,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,6.5,0,5,0.87,0.13,0.05,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,6.5,0,10,0.87,0.14000000000000001,0.05,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,6.5,0,15,0.88,0.15,0.06,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,7,0,0,0.84,0.14000000000000001,0.06,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,7,0,5,0.84,0.15,0.06,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,7,0,10,0.85,0.17,7.0000000000000007E-2,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,7,0,15,0.85,0.18,7.0000000000000007E-2,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,7.5,0,0,0.81,0.16,7.0000000000000007E-2,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,7.5,0,5,0.82,0.18,0.08,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,7.5,0,10,0.82,0.19,0.08,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,7.5,0,15,0.83,0.19,0.08,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,8,0,0,0.79,0.18,0.08,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,8,0,5,0.79,0.2,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,8,0,10,0.8,0.2,0.09,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,8,0,15,0.8,0.21,0.09,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,8.5,0,0,0.76,0.2,0.1,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,8.5,0,5,0.77,0.21,0.1,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,8.5,0,10,0.77,0.22,0.1,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,8.5,0,15,0.78,0.22,0.11,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,9,0,0,0.74,0.22,0.11,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,9,0,5,0.75,0.23,0.11,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,9,0,10,0.75,0.23,0.11,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,9,0,15,0.76,0.24,0.12,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,9.5,0,0,0.72,0.23,0.12,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,9.5,0,5,0.73,0.24,0.12,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,9.5,0,10,0.73,0.25,0.12,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,9.5,0,15,0.74,0.26,0.13,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,10,0,0,0.7,0.25,0.12,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,10,0,5,0.71,0.26,0.13,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,10,0,10,0.71,0.27,0.13,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",48,10,0,15,0.72,0.28000000000000003,0.14000000000000001,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,6,0,0,0.88,0.1,0.04,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,6,0,5,0.88,0.1,0.04,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,6,0,10,0.89,0.1,0.04,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,6,0,15,0.89,0.11,0.04,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,6.5,0,0,0.85,0.12,0.05,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,6.5,0,5,0.85,0.12,0.05,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,6.5,0,10,0.86,0.12,0.05,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,6.5,0,15,0.86,0.13,0.05,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,7,0,0,0.82,0.14000000000000001,0.06,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,7,0,5,0.83,0.14000000000000001,0.06,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,7,0,10,0.83,0.15,0.06,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,7,0,15,0.84,0.15,0.06,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,7.5,0,0,0.79,0.16,7.0000000000000007E-2,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,7.5,0,5,0.8,0.16,7.0000000000000007E-2,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,7.5,0,10,0.81,0.18,7.0000000000000007E-2,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,7.5,0,15,0.81,0.19,0.08,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,8,0,0,0.77,0.18,0.08,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,8,0,5,0.78,0.19,0.08,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,8,0,10,0.78,0.2,0.09,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,8,0,15,0.78,0.21,0.09,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,8.5,0,0,0.75,0.19,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,8.5,0,5,0.75,0.2,0.1,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,8.5,0,10,0.76,0.22,0.1,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,8.5,0,15,0.76,0.23,0.11,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,9,0,0,0.73,0.2,0.1,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,9,0,5,0.73,0.22,0.11,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,9,0,10,0.74,0.23,0.11,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,9,0,15,0.74,0.24,0.11,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,9.5,0,0,0.71,0.22,0.11,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,9.5,0,5,0.71,0.24,0.11,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,9.5,0,10,0.72,0.25,0.12,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,9.5,0,15,0.72,0.26,0.12,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,10,0,0,0.69,0.24,0.12,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,10,0,5,0.69,0.26,0.13,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,10,0,10,0.7,0.28000000000000003,0.13,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",49,10,0,15,0.7,0.28000000000000003,0.14000000000000001,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,6,0,0,0.86,0.09,0.03,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,6,0,5,0.86,0.1,0.04,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,6,0,10,0.87,0.1,0.04,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,6,0,15,0.87,0.1,0.04,6,0.87]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,6.5,0,0,0.83,0.11,0.05,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,6.5,0,5,0.84,0.12,0.05,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,6.5,0,10,0.84,0.12,0.05,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,6.5,0,15,0.85,0.12,0.05,6,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,7,0,0,0.8,0.13,0.05,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,7,0,5,0.81,0.13,0.06,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,7,0,10,0.82,0.14000000000000001,0.06,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,7,0,15,0.82,0.15,0.06,5,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,7.5,0,0,0.78,0.15,7.0000000000000007E-2,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,7.5,0,5,0.79,0.16,7.0000000000000007E-2,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,7.5,0,10,0.79,0.17,7.0000000000000007E-2,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,7.5,0,15,0.79,0.18,7.0000000000000007E-2,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,8,0,0,0.75,0.17,0.08,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,8,0,5,0.76,0.18,0.08,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,8,0,10,0.77,0.19,0.09,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,8,0,15,0.77,0.2,0.09,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,8.5,0,0,0.73,0.18,0.09,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,8.5,0,5,0.74,0.2,0.1,4,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,8.5,0,10,0.74,0.21,0.1,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,8.5,0,15,0.75,0.22,0.1,4,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,9,0,0,0.71,0.2,0.1,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,9,0,5,0.72,0.21,0.1,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,9,0,10,0.72,0.23,0.11,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,9,0,15,0.73,0.24,0.11,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,9.5,0,0,0.69,0.21,0.11,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,9.5,0,5,0.7,0.23,0.11,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,9.5,0,10,0.7,0.24,0.12,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,9.5,0,15,0.71,0.25,0.12,3,0.85]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,10,0,0,0.67,0.23,0.11,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,10,0,5,0.68,0.25,0.12,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,10,0,10,0.69,0.27,0.13,3,0.86]
[12,"BILATERAL DESPLAZADO","ME4b","A-LED NOVA-SL160 160W C/L SERIE PREMIUM","Definido por el usuario","Insuficiente",50,10,0,15,0.69,0.27,0.13,3,0.85]

{"sheet":"CALCULO","index":1,"n_rows":50,"n_cols":19,"rows_kept":50,"cut":false,"hidden":false,"merged":[[2,1,2,21],[32,6,32,10]]}
[]
[]
[null,"CALCULO DE ILUMINACION VIAL URBANA"]
[]
[null,"Distancia entre columnas\n\"D\"","Luminancia","Unif, gral","Unif. Long"]
[null,"Etiquetas de fila","Lm [cd/m²]-","U0."," Ul,"]
[null,"Adecuado/a"]
[null,10,2.16,0.44,0.94]
[null,11,1.97,0.45,0.93]
[null,12,1.8,0.44,0.92]
[null,13,1.66,0.44,0.91]
[null,14,1.55,0.44,0.9]
[null,15,1.44,0.43,0.89]
[null,16,1.35,0.43,0.87]
[null,17,1.27,0.43,0.87]
[null,18,1.2,0.43,0.85]
[null,19,1.1399999999999999,0.43,0.84]
[null,20,1.08,0.43,0.81]
[null,21,1.03,0.43,0.8]
[null,22,0.99,0.42,0.77]
[null,23,0.94,0.43,0.74,null,null,null,null,null,null,null,"VARIABLES DE CALCULO",null,null,null,null,"D: ","DISTANCIA ENTRE COLUMNAS"]
[null,24,0.9,0.43,0.72,null,null,null,null,null,null,null,"1.-","ALTURA DE MONTAJE"]
[null,25,0.87,0.43,0.69,null,null,null,null,null,null,null,"2.-","SALIENTE SOBRE LA CALZADA"]
[null,26,0.84,0.43,0.65,null,null,null,null,null,null,null,"3.-","INCLINACION DEL BRAZO (0-5-10-15º)"]
[null,27,0.8,0.42,0.61,null,null,null,null,null,null,null,"4.-","LONGITUD DEL BRAZO 2M"]
[null,28,0.78,0.41,0.57999999999999996,null,null,null,null,null,null,null,"5.-","ANCHO DE LA CALZADA"]
[null,29,0.75,0.4,0.54,null,null,null,null,null,null,null,"6.-","LUMINARIA"]
[]
[null,"Insuficiente",null,null,null,null,null,null,null,null,null,null,"PARAMETROS DE CALCULO"]
[null,30,0.72,0.39,0.51,null,null,null,null,null,null,null,"L (4.-): ","LONGITUD DEL PESCANTE FIJA 2m."]
[null,31,0.7,0.38,0.48,null,null,null,null,null,null,null,"B1:","SITUACION DE ILUMINACION Vm ENTRE 30 Y 60 km/h"]
[null,32,0.68,0.37,0.45,null,null,null,null,null,null,null,0.8,"FACTOR DE DEGRADACION"]
[null,33,0.66,0.36,0.42,null,"MANUAL DE USO Y APLICACIONES",null,null,null,null,null,"ME4b","CLASE DE ILUMINACION"]
[null,34,0.64,0.35,0.38]
[null,35,0.62,0.33,0.35,null,null,"ADECUADO:","Cumple con los requisitos minimos para una calzada urbana clase ME4b"]
[null,36,0.6,0.32,0.32,null,null,"INSUFICIENTE:","No cumple con los requisitos minimos para una calzada urbana clase ME4b"]
[null,37,0.59,0.31,0.3]
[null,38,0.56999999999999995,0.28999999999999998,0.28000000000000003]
[null,39,0.56000000000000005,0.28000000000000003,0.25]
[null,40,0.54,0.27,0.23]
[null,41,0.53,0.25,0.21]
[null,42,0.52,0.24,0.19]
[null,43,0.51,0.22,0.17]
[null,44,0.49,0.21,0.15]
[null,45,0.48,0.2,0.14000000000000001]
[null,46,0.47,0.18,0.12]
[null,47,0.46,0.16,0.11]
[null,48,0.45,0.15,0.09]
[null,49,0.44,0.14000000000000001,0.08]
[null,50,0.44,0.13,7.0000000000000007E-2]

{"sheet":"MANUAL DE USO","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"cut":false,"hidden":false,"merged":[[2,3,2,6],[2,1,2,2],[3,1,3,2],[12,1,12,2],[11,1,11,2],[4,1,4,2],[5,1,5,2]]}
[]
[]
[null,"INSTRUCTIVO DE USO",null,"VOLVER A LA HOJA DE CALCULO"]
[null,"El siguiente archivo es una guía rápida para verificar el montaje de luminarias en una calle tipo urbana, este archivo permite seleccionar una serie de parámetros variables, como el ancho de la calzada, la disposición de las columnas, la altura de montaje e inclinación.\nTrabajando con estas variables podemos verificar si, las disposiciones elegidas cumplen con las exigencias de iluminacion para una calle con clase de iluminacion ME4b, el resultado nos arroja la separación entre columnas que cumple con los requisitos de iluminacion.\nEsto es es util , tanto para el diseño de una nueva iluminación vial, y poder asi determinar la combinación óptima de distancias entre columnas, alturas de montaje, ángulo de inclinación y luminarias, como para la elección de luminarias para reemplazar las existentes con una disposición determinada.\n\nNOTA: Cabe aclarar que estos resultados son para los valores prefijados, tomando diferentes valores como longitud del pescante, Clase de iluminacion (superior o inferior exigencia a la ME4b), dichos valores pueden variar en mayor o menor distancia entre columnas, para todas las alternativas se tomaron fotometrías relevadas por el laboratorio de la UNT, aplicadas sobre el software de cálculo DIALUX\n"]
[null,"PARAMETROSD PREFIJADOS"]
[null,"Se toman, como parametros de calculo prefijados los siguientes valores"]
[null,"L: ","LONGITUD DEL PESCANTE FIJA 2m."]
[null,null,"SEPARACION DE LA COLUMNA A LA LINEA DE LA CALZADA 0,5m."]
[null,"B1:","SITUACION DE ILUMINACION Vel. Media. ENTRE 30 Y 60 km/h"]
[null,0.8,"FACTOR DE DEGRADACION"]
[null,"ME4b","CLASE DE ILUMINACION"]
[null,"PARAMETROS VARIABLES"]
[null,"Seleccionando los parámetros variables que queremos aplicar, el software nos indica las distancias de montaje entre columnas que cumplen con dichas exigencias, separándolo entre: \nADECUADO: Nos arroja como resultado las distancias entre columnas que cumple con las exigencias de iluminacion y uniformidades, \nINSUFICIENTE:  Nos brinda las distancias entre columnas que no cumplen con dichos requisitos.\n"]
[null,null,"ANCHO DE CALZADA: Podemos seleccionar entre dos anchos estándar típicos de calzadas ,7m y 12m."]
[null,"DISPOSICION: Nos brinda la posibilidad de elegir entre dos disposiciones diferentes, \nUNILATERAL: que ubica la línea de luminaria en un solo lado de la calzada, \nBILATERAL DESPLAZADA: o tres bolillos que ubica las luminarias a ambos lados de la calzada desplazadas."]
[null,null,"LUMINARIAS: Se puede seleccionar entre 2 tipos diferentes de luminarias y 5 potencias diferentes, cuyos catálogos se pueden bajar de nuestra WEB: http://www.hpelectricidad.com.ar/productos#productos esto nos permite ver entre la combinación de los parámetros que cumplen con las exigencias de calculo"]
[null,"ALTURA DE MONTAJE: esta es la altura de la columna, Nos permite seleccionar la altura de montaje deseada entre valores que oscilan entre 6 y 10m.\nPara ello debemos tener en cuenta que:\nA menor altura, mayor nivel de iluminacion y menor uniformidad\nA mayor altura, menor nivel de iluminacion, con mayor uniformidad (iluminacion con menos sombra, menos diferencia entre los niveles máximos y mínimos de iluminacion)\n"]
[null,null,"INCLINACION: Podemos seleccionar los valores de inclinación del pescante entre 0º a 15º, lo que nos permite ir llevando el centro de la directriz de iluminacion paso a paso hacia el centro de la calzada"]

{"sheet":"CONSULTA","index":3,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
[]
[null,"CODIGO","IMAGEN"]
[null,"A-LED NOVA-SL90 90W SERIE PREMIUM"]
[null,"A-LED NOVA-SL120 120W SERIE PREMIUM"]
[null,"A-LED NOVA-SL160 160W  SERIE PREMIUM"]
[null,"A-LED 105w"]
[null,"A-LED 140w"]
[null,"A-LED 200w"]